# Print output for @column tags ?>
Developers

- Design
- Develop
- Distribute

Developer Console

## Most visited

## Recently visited

## Results for

Summary: Nested Classes | Constants | Inherited Constants | Fields | Ctors | Methods | Inherited Methods

# ScanResult

`public final class ScanResult`
`extends Object` `implements Parcelable`

java.lang.Object
↳ | android.net.wifi.ScanResult

Describes information about a detected access point. In addition to the attributes described here, the supplicant keeps track of `quality`, `noise`, and `maxbitrate` attributes, but does not currently report them to external clients.

## Summary

### Nested classes
`class` | `ScanResult.InformationElement` information elements from beacon.

### Constants
`int` | `CHANNEL_WIDTH_160MHZ` AP Channel bandwidth is 160 MHZ
`int` | `CHANNEL_WIDTH_20MHZ` AP Channel bandwidth is 20 MHZ
`int` | `CHANNEL_WIDTH_40MHZ` AP Channel bandwidth is 40 MHZ
`int` | `CHANNEL_WIDTH_80MHZ` AP Channel bandwidth is 80 MHZ
`int` | `CHANNEL_WIDTH_80MHZ_PLUS_MHZ` AP Channel bandwidth is 160 MHZ, but 80MHZ + 80MHZ
`int` | `WIFI_STANDARD_11AC` Wi-Fi 802.11ac
`int` | `WIFI_STANDARD_11AX` Wi-Fi 802.11ax
`int` | `WIFI_STANDARD_11N` Wi-Fi 802.11n
`int` | `WIFI_STANDARD_LEGACY` Wi-Fi 802.11a/b/g
`int` | `WIFI_STANDARD_UNKNOWN` Wi-Fi unknown standard

### Inherited constants
From interface `android.os.Parcelable`
`int` | `CONTENTS_FILE_DESCRIPTOR` Descriptor bit used with `describeContents()`: indicates that the Parcelable object's flattened representation includes a file descriptor.
`int` | `PARCELABLE_WRITE_RETURN_VALUE` Flag for use with `writeToParcel(Parcel, int)`: the object being written is a return value, that is the result of a function such as "`Parcelable someFunction()`", "`void someFunction(out Parcelable)`", or "`void someFunction(inout Parcelable)`".

### Fields
`public String` | `BSSID` The address of the access point.
`public static final Creator<ScanResult>` | `CREATOR` Implement the Parcelable interface
`public String` | `SSID` The network name.
`public String` | `capabilities` Describes the authentication, key management, and encryption schemes supported by the access point.
`public int` | `centerFreq0` Not used if the AP bandwidth is 20 MHz If the AP use 40, 80 or 160 MHz, this is the center frequency (in MHz) if the AP use 80 + 80 MHz, this is the center frequency of the first segment (in MHz)
`public int` | `centerFreq1` Only used if the AP bandwidth is 80 + 80 MHz if the AP use 80 + 80 MHz, this is the center frequency of the second segment (in MHz)
`public int` | `channelWidth` AP Channel bandwidth; one of `CHANNEL_WIDTH_20MHZ`, `CHANNEL_WIDTH_40MHZ`, `CHANNEL_WIDTH_80MHZ`, `CHANNEL_WIDTH_160MHZ` or `CHANNEL_WIDTH_80MHZ_PLUS_MHZ`.
`public int` | `frequency` The primary 20 MHz frequency (in MHz) of the channel over which the client is communicating with the access point.
`public int` | `level` The detected signal level in dBm, also known as the RSSI.
`public CharSequence` | `operatorFriendlyName` Indicates Passpoint operator name published by access point.
`public long` | `timestamp` timestamp in microseconds (since boot) when this result was last seen.
`public CharSequence` | `venueName` Indicates venue name (such as 'San Francisco Airport') published by access point; only available on Passpoint network and if published by access point.

### Public constructors
`ScanResult(ScanResult source)` copy constructor
`ScanResult()` Construct an empty scan result.

### Public methods
`List<ScanResult.InformationElement>` | `getInformationElements()` Get all information elements found in the beacon.
`int` | `getWifiStandard()` return the AP wifi standard.
`boolean` | `is80211mcResponder()`
`boolean` | `isPasspointNetwork()`
`String` | `toString()` Returns a string representation of the object.

### Inherited methods
From class `java.lang.Object`
`Object` | `clone()` Creates and returns a copy of this object.
`boolean` | `equals(Object obj)` Indicates whether some other object is "equal to" this one.
`void` | `finalize()` Called by the garbage collector on an object when garbage collection determines that there are no more references to the object.
`final Class<?>` | `getClass()` Returns the runtime class of this `Object`.
`int` | `hashCode()` Returns a hash code value for the object.
`final void` | `notify()` Wakes up a single thread that is waiting on this object's monitor.
`final void` | `notifyAll()` Wakes up all threads that are waiting on this object's monitor.
`String` | `toString()` Returns a string representation of the object.
`final void` | `wait(long timeout, int nanos)` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object, or some other thread interrupts the current thread, or a certain amount of real time has elapsed.
`final void` | `wait(long timeout)` Causes the current thread to wait until either another thread invokes the `notify()` method or the `notifyAll()` method for this object, or a specified amount of time has elapsed.
`final void` | `wait()` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object.
From interface `android.os.Parcelable`
`abstract int` | `describeContents()` Describe the kinds of special objects contained in this Parcelable instance's marshaled representation.
`abstract void` | `writeToParcel(Parcel dest, int flags)` Flatten this object in to a Parcel.

## Constants

### CHANNEL_WIDTH_160MHZ

    public static final int CHANNEL_WIDTH_160MHZ

AP Channel bandwidth is 160 MHZ

Constant Value: 3 (0x00000003)

### CHANNEL_WIDTH_20MHZ

    public static final int CHANNEL_WIDTH_20MHZ

AP Channel bandwidth is 20 MHZ

Constant Value: 0 (0x00000000)

### CHANNEL_WIDTH_40MHZ

    public static final int CHANNEL_WIDTH_40MHZ

AP Channel bandwidth is 40 MHZ

Constant Value: 1 (0x00000001)

### CHANNEL_WIDTH_80MHZ

    public static final int CHANNEL_WIDTH_80MHZ

AP Channel bandwidth is 80 MHZ

Constant Value: 2 (0x00000002)

### CHANNEL_WIDTH_80MHZ_PLUS_MHZ

    public static final int CHANNEL_WIDTH_80MHZ_PLUS_MHZ

AP Channel bandwidth is 160 MHZ, but 80MHZ + 80MHZ

Constant Value: 4 (0x00000004)

### WIFI_STANDARD_11AC

    public static final int WIFI_STANDARD_11AC

Wi-Fi 802.11ac

Constant Value: 5 (0x00000005)

### WIFI_STANDARD_11AX

    public static final int WIFI_STANDARD_11AX

Wi-Fi 802.11ax

Constant Value: 6 (0x00000006)

### WIFI_STANDARD_11N

    public static final int WIFI_STANDARD_11N

Wi-Fi 802.11n

Constant Value: 4 (0x00000004)

### WIFI_STANDARD_LEGACY

    public static final int WIFI_STANDARD_LEGACY

Wi-Fi 802.11a/b/g

Constant Value: 1 (0x00000001)

### WIFI_STANDARD_UNKNOWN

    public static final int WIFI_STANDARD_UNKNOWN

Wi-Fi unknown standard

Constant Value: 0 (0x00000000)

## Fields

### BSSID

    public String BSSID

The address of the access point.

### CREATOR

    public static final Creator<ScanResult> CREATOR

Implement the Parcelable interface

### SSID

    public String SSID

The network name.

### capabilities

    public String capabilities

Describes the authentication, key management, and encryption schemes supported by the access point.

### centerFreq0

    public int centerFreq0

Not used if the AP bandwidth is 20 MHz If the AP use 40, 80 or 160 MHz, this is the center frequency (in MHz) if the AP use 80 + 80 MHz, this is the center frequency of the first segment (in MHz)

### centerFreq1

    public int centerFreq1

Only used if the AP bandwidth is 80 + 80 MHz if the AP use 80 + 80 MHz, this is the center frequency of the second segment (in MHz)

### channelWidth

    public int channelWidth

AP Channel bandwidth; one of `CHANNEL_WIDTH_20MHZ`, `CHANNEL_WIDTH_40MHZ`, `CHANNEL_WIDTH_80MHZ`, `CHANNEL_WIDTH_160MHZ` or `CHANNEL_WIDTH_80MHZ_PLUS_MHZ`.
Value is `CHANNEL_WIDTH_20MHZ`, `CHANNEL_WIDTH_40MHZ`, `CHANNEL_WIDTH_80MHZ`, `CHANNEL_WIDTH_160MHZ`, or `CHANNEL_WIDTH_80MHZ_PLUS_MHZ`

### frequency

    public int frequency

The primary 20 MHz frequency (in MHz) of the channel over which the client is communicating with the access point.

### level

    public int level

The detected signal level in dBm, also known as the RSSI.

Use `WifiManager.calculateSignalLevel(int)` to convert this number into an absolute signal level which can be displayed to a user.

### operatorFriendlyName

    public CharSequence operatorFriendlyName

Indicates Passpoint operator name published by access point.

### timestamp

    public long timestamp

timestamp in microseconds (since boot) when this result was last seen.

### venueName

    public CharSequence venueName

Indicates venue name (such as 'San Francisco Airport') published by access point; only available on Passpoint network and if published by access point.

## Public constructors

### ScanResult

    public ScanResult (ScanResult source)

copy constructor

Parameters
`source` | `ScanResult`: This value cannot be `null`.

### ScanResult

    public ScanResult ()

Construct an empty scan result.

## Public methods

### getInformationElements

    public List<ScanResult.InformationElement> getInformationElements ()

Get all information elements found in the beacon.

Returns
`List<ScanResult.InformationElement>` | This value cannot be `null`.

### getWifiStandard

    public int getWifiStandard ()

return the AP wifi standard.

Returns
`int` | Value is `WIFI_STANDARD_UNKNOWN`, `WIFI_STANDARD_LEGACY`, `WIFI_STANDARD_11N`, `WIFI_STANDARD_11AC`, or `WIFI_STANDARD_11AX`

### is80211mcResponder

    public boolean is80211mcResponder ()

Returns
`boolean` |

### isPasspointNetwork

    public boolean isPasspointNetwork ()

Returns
`boolean` |

### toString

    public String toString ()

Returns a string representation of the object. In general, the `toString` method returns a string that "textually represents" this object. The result should be a concise but informative representation that is easy for a person to read. It is recommended that all subclasses override this method.

The `toString` method for class `Object` returns a string consisting of the name of the class of which the object is an instance, the at-sign character ``@`', and the unsigned hexadecimal representation of the hash code of the object. In other words, this method returns a string equal to the value of:

>      getClass().getName() + '@' + Integer.toHexString(hashCode())

Returns
`String` | a string representation of the object.

Full name *
Email address *
Company / developer name
One of your Play Store app URLs *
Which best describes your business:*
Apps
Games
Apps & Games
*
*