# Print output for @column tags ?>
Developers

- Design
- Develop
- Distribute

Developer Console

## Most visited

## Recently visited

## Results for

Summary: Nested Classes | Constants | Ctors | Inherited Methods

# SecurityLog

`public class SecurityLog`
`extends Object` ``

java.lang.Object
↳ | android.app.admin.SecurityLog

Definitions for working with security logs.

Device owner apps can control the logging with `DevicePolicyManager#setSecurityLoggingEnabled`. When security logs are enabled, device owner apps receive periodic callbacks from `DeviceAdminReceiver#onSecurityLogsAvailable`, at which time new batch of logs can be collected via `DevicePolicyManager#retrieveSecurityLogs`. `SecurityEvent` describes the type and format of security logs being collected.

## Summary

### Nested classes
`class` | `SecurityLog.SecurityEvent` A class representing a security event log entry.

### Constants
`int` | `LEVEL_ERROR` Event severity level indicating that the event requires urgent admin action.
`int` | `LEVEL_INFO` Event severity level indicating that the event corresponds to normal workflow.
`int` | `LEVEL_WARNING` Event severity level indicating that the event may require admin attention.
`int` | `TAG_ADB_SHELL_CMD` Indicates that a shell command was issued over ADB via `adb shell <command>` The log entry contains a `String` payload containing the shell command, accessible via `SecurityEvent#getData()`.
`int` | `TAG_ADB_SHELL_INTERACTIVE` Indicates that an ADB interactive shell was opened via "adb shell".
`int` | `TAG_APP_PROCESS_START` Indicates that an app process was started.
`int` | `TAG_CAMERA_POLICY_SET` Indicates that the admin has set policy to disable camera.
`int` | `TAG_CERT_AUTHORITY_INSTALLED` Indicates that a new root certificate has been installed into system's trusted credential storage.
`int` | `TAG_CERT_AUTHORITY_REMOVED` Indicates that a new root certificate has been removed from system's trusted credential storage.
`int` | `TAG_CERT_VALIDATION_FAILURE` Indicates a failure to validate X.509v3 certificate.
`int` | `TAG_CRYPTO_SELF_TEST_COMPLETED` Indicates that cryptographic functionality self test has completed.
`int` | `TAG_KEYGUARD_DISABLED_FEATURES_SET` Indicates that an admin has set disabled keyguard features.
`int` | `TAG_KEYGUARD_DISMISSED` Indicates that keyguard has been dismissed.
`int` | `TAG_KEYGUARD_DISMISS_AUTH_ATTEMPT` Indicates that there has been an authentication attempt to dismiss the keyguard.
`int` | `TAG_KEYGUARD_SECURED` Indicates that the device has been locked, either by the user or by a timeout.
`int` | `TAG_KEY_DESTRUCTION` Indicates that a cryptographic key was destroyed.
`int` | `TAG_KEY_GENERATED` Indicates that a cryptographic key was generated.
`int` | `TAG_KEY_IMPORT` Indicates that a cryptographic key was imported.
`int` | `TAG_KEY_INTEGRITY_VIOLATION` Indicates a failed cryptographic key integrity check.
`int` | `TAG_LOGGING_STARTED` Indicates start-up of audit logging.
`int` | `TAG_LOGGING_STOPPED` Indicates shutdown of audit logging.
`int` | `TAG_LOG_BUFFER_SIZE_CRITICAL` Indicates that the audit log buffer has reached 90% of its capacity.
`int` | `TAG_MAX_PASSWORD_ATTEMPTS_SET` Indicates that an admin has set a maximum number of failed password attempts before wiping data.
`int` | `TAG_MAX_SCREEN_LOCK_TIMEOUT_SET` Indicates that an admin has set a maximum screen lock timeout.
`int` | `TAG_MEDIA_MOUNT` Indicates that removable media has been mounted on the device.
`int` | `TAG_MEDIA_UNMOUNT` Indicates that removable media was unmounted from the device.
`int` | `TAG_OS_SHUTDOWN` Indicates that the Android OS has shutdown.
`int` | `TAG_OS_STARTUP` Indicates that the Android OS has started.
`int` | `TAG_PASSWORD_COMPLEXITY_REQUIRED` Indicates that an admin has set a password complexity requirement, using the platform's pre-defined complexity levels.
`int` | `TAG_PASSWORD_COMPLEXITY_SET` Indicates that an admin has set a requirement for password complexity.
`int` | `TAG_PASSWORD_EXPIRATION_SET` Indicates that an admin has set a password expiration timeout.
`int` | `TAG_PASSWORD_HISTORY_LENGTH_SET` Indicates that an admin has set a password history length.
`int` | `TAG_REMOTE_LOCK` Indicates that an admin remotely locked the device or profile.
`int` | `TAG_SYNC_RECV_FILE` Indicates that a file was pulled from the device via the adb daemon, for example via `adb pull`.
`int` | `TAG_SYNC_SEND_FILE` Indicates that a file was pushed to the device via the adb daemon, for example via `adb push`.
`int` | `TAG_USER_RESTRICTION_ADDED` Indicates that an admin has set a user restriction.
`int` | `TAG_USER_RESTRICTION_REMOVED` Indicates that an admin has removed a user restriction.
`int` | `TAG_WIPE_FAILURE` Indicates a failure to wipe device or user data.

### Public constructors
`SecurityLog()`

### Inherited methods
From class `java.lang.Object`
`Object` | `clone()` Creates and returns a copy of this object.
`boolean` | `equals(Object obj)` Indicates whether some other object is "equal to" this one.
`void` | `finalize()` Called by the garbage collector on an object when garbage collection determines that there are no more references to the object.
`final Class<?>` | `getClass()` Returns the runtime class of this `Object`.
`int` | `hashCode()` Returns a hash code value for the object.
`final void` | `notify()` Wakes up a single thread that is waiting on this object's monitor.
`final void` | `notifyAll()` Wakes up all threads that are waiting on this object's monitor.
`String` | `toString()` Returns a string representation of the object.
`final void` | `wait(long timeout, int nanos)` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object, or some other thread interrupts the current thread, or a certain amount of real time has elapsed.
`final void` | `wait(long timeout)` Causes the current thread to wait until either another thread invokes the `notify()` method or the `notifyAll()` method for this object, or a specified amount of time has elapsed.
`final void` | `wait()` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object.

## Constants

### LEVEL_ERROR

    public static final int LEVEL_ERROR

Event severity level indicating that the event requires urgent admin action.

Constant Value: 3 (0x00000003)

### LEVEL_INFO

    public static final int LEVEL_INFO

Event severity level indicating that the event corresponds to normal workflow.

Constant Value: 1 (0x00000001)

### LEVEL_WARNING

    public static final int LEVEL_WARNING

Event severity level indicating that the event may require admin attention.

Constant Value: 2 (0x00000002)

### TAG_ADB_SHELL_CMD

    public static final int TAG_ADB_SHELL_CMD

Indicates that a shell command was issued over ADB via `adb shell <command>` The log entry contains a `String` payload containing the shell command, accessible via `SecurityEvent#getData()`. If security logging is enabled on organization-owned managed profile devices, the shell command will be redacted to an empty string.

Constant Value: 210002 (0x00033452)

### TAG_ADB_SHELL_INTERACTIVE

    public static final int TAG_ADB_SHELL_INTERACTIVE

Indicates that an ADB interactive shell was opened via "adb shell". There is no extra payload in the log event.

Constant Value: 210001 (0x00033451)

### TAG_APP_PROCESS_START

    public static final int TAG_APP_PROCESS_START

Indicates that an app process was started. The log entry contains the following information about the process encapsulated in an `Object` array, accessible via `SecurityEvent#getData()`:

- [0] process name (`String`)
- [1] exact start time in milliseconds according to `System.currentTimeMillis()` (`Long`)
- [2] app uid (`Integer`)
- [3] app pid (`Integer`)
- [4] seinfo tag (`String`)
- [5] SHA-256 hash of the base APK in hexadecimal (`String`) If security logging is enabled on organization-owned managed profile devices, only events happening inside the managed profile will be visible.

  Constant Value: 210005 (0x00033455)

### TAG_CAMERA_POLICY_SET

    public static final int TAG_CAMERA_POLICY_SET

Indicates that the admin has set policy to disable camera. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] admin package name (`String`)
- [1] admin user ID (`Integer`)
- [2] target user ID (`Integer`)
- [3] whether the camera is disabled or not (`Integer`, 1 if it's disabled, 0 if enabled)

  Constant Value: 210034 (0x00033472)

### TAG_CERT_AUTHORITY_INSTALLED

    public static final int TAG_CERT_AUTHORITY_INSTALLED

Indicates that a new root certificate has been installed into system's trusted credential storage. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] result (`Integer`, 0 if operation failed, 1 if succeeded)
- [1] subject of the certificate (`String`).
- [2] which user the certificate is installed for (`Integer`), only available from version `Build.VERSION_CODES.R`. If security logging is enabled on organization-owned managed profile devices, only events happening inside the managed profile will be visible.

  Constant Value: 210029 (0x0003346d)

### TAG_CERT_AUTHORITY_REMOVED

    public static final int TAG_CERT_AUTHORITY_REMOVED

Indicates that a new root certificate has been removed from system's trusted credential storage. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] result (`Integer`, 0 if operation failed, 1 if succeeded)
- [1] subject of the certificate (`String`).
- [2] which user the certificate is removed from (`Integer`), only available from version `Build.VERSION_CODES.R`. If security logging is enabled on organization-owned managed profile devices, only events happening inside the managed profile will be visible.

  Constant Value: 210030 (0x0003346e)

### TAG_CERT_VALIDATION_FAILURE

    public static final int TAG_CERT_VALIDATION_FAILURE

Indicates a failure to validate X.509v3 certificate. The log entry contains a `String` payload indicating the failure reason, accessible via `SecurityEvent#getData()`.

Constant Value: 210033 (0x00033471)

### TAG_CRYPTO_SELF_TEST_COMPLETED

    public static final int TAG_CRYPTO_SELF_TEST_COMPLETED

Indicates that cryptographic functionality self test has completed. The log entry contains an `Integer` payload, indicating the result of the test (0 if the test failed, 1 if succeeded) and accessible via `SecurityEvent#getData()`.

Constant Value: 210031 (0x0003346f)

### TAG_KEYGUARD_DISABLED_FEATURES_SET

    public static final int TAG_KEYGUARD_DISABLED_FEATURES_SET

Indicates that an admin has set disabled keyguard features. The log entry contains the following information about the event encapsulated in an `Object` array, accessible via `SecurityEvent#getData()`:

- [0] admin package name (`String`)
- [1] admin user ID (`Integer`)
- [2] target user ID (`Integer`)
- [3] disabled keyguard feature mask (`Integer`).

  See also:

  - `DevicePolicyManager.setKeyguardDisabledFeatures(ComponentName, int)`

  Constant Value: 210021 (0x00033465)

### TAG_KEYGUARD_DISMISSED

    public static final int TAG_KEYGUARD_DISMISSED

Indicates that keyguard has been dismissed. This event is only logged if the device has a secure keyguard. It is logged regardless of how keyguard is dismissed, including via PIN/pattern/password, biometrics or via a trust agent. There is no extra payload in the log event.

See also:

- `TAG_KEYGUARD_DISMISS_AUTH_ATTEMPT`

Constant Value: 210006 (0x00033456)

### TAG_KEYGUARD_DISMISS_AUTH_ATTEMPT

    public static final int TAG_KEYGUARD_DISMISS_AUTH_ATTEMPT

Indicates that there has been an authentication attempt to dismiss the keyguard. The log entry contains the following information about the attempt encapsulated in an `Object` array, accessible via `SecurityEvent#getData()`:

- [0] attempt result (`Integer`, 1 for successful, 0 for unsuccessful)
- [1] strength of authentication method (`Integer`, 1 if strong authentication method was used, 0 otherwise)

  Constant Value: 210007 (0x00033457)

### TAG_KEYGUARD_SECURED

    public static final int TAG_KEYGUARD_SECURED

Indicates that the device has been locked, either by the user or by a timeout. There is no extra payload in the log event.

Constant Value: 210008 (0x00033458)

### TAG_KEY_DESTRUCTION

    public static final int TAG_KEY_DESTRUCTION

Indicates that a cryptographic key was destroyed. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] result (`Integer`, 0 if operation failed, 1 if succeeded)
- [1] alias of the key (`String`)
- [2] requesting process uid (`Integer`). If security logging is enabled on organization-owned managed profile devices, only events happening inside the managed profile will be visible.

  Constant Value: 210026 (0x0003346a)

### TAG_KEY_GENERATED

    public static final int TAG_KEY_GENERATED

Indicates that a cryptographic key was generated. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] result (`Integer`, 0 if operation failed, 1 if succeeded)
- [1] alias of the key (`String`)
- [2] requesting process uid (`Integer`). If security logging is enabled on organization-owned managed profile devices, only events happening inside the managed profile will be visible.

  Constant Value: 210024 (0x00033468)

### TAG_KEY_IMPORT

    public static final int TAG_KEY_IMPORT

Indicates that a cryptographic key was imported. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] result (`Integer`, 0 if operation failed, 1 if succeeded)
- [1] alias of the key (`String`)
- [2] requesting process uid (`Integer`). If security logging is enabled on organization-owned managed profile devices, only events happening inside the managed profile will be visible.

  Constant Value: 210025 (0x00033469)

### TAG_KEY_INTEGRITY_VIOLATION

    public static final int TAG_KEY_INTEGRITY_VIOLATION

Indicates a failed cryptographic key integrity check. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] alias of the key (`String`)
- [1] owner application uid (`Integer`). If security logging is enabled on organization-owned managed profile devices, only events happening inside the managed profile will be visible.

  Constant Value: 210032 (0x00033470)

### TAG_LOGGING_STARTED

    public static final int TAG_LOGGING_STARTED

Indicates start-up of audit logging. There is no extra payload in the log event.

Constant Value: 210011 (0x0003345b)

### TAG_LOGGING_STOPPED

    public static final int TAG_LOGGING_STOPPED

Indicates shutdown of audit logging. There is no extra payload in the log event.

Constant Value: 210012 (0x0003345c)

### TAG_LOG_BUFFER_SIZE_CRITICAL

    public static final int TAG_LOG_BUFFER_SIZE_CRITICAL

Indicates that the audit log buffer has reached 90% of its capacity. There is no extra payload in the log event.

Constant Value: 210015 (0x0003345f)

### TAG_MAX_PASSWORD_ATTEMPTS_SET

    public static final int TAG_MAX_PASSWORD_ATTEMPTS_SET

Indicates that an admin has set a maximum number of failed password attempts before wiping data. The log entry contains the following information about the event encapsulated in an `Object` array, accessible via `SecurityEvent#getData()`:

- [0] admin package name (`String`)
- [1] admin user ID (`Integer`)
- [2] target user ID (`Integer`)
- [3] new maximum number of failed password attempts (`Integer`)

  See also:

  - `DevicePolicyManager.setMaximumFailedPasswordsForWipe(ComponentName, int)`

  Constant Value: 210020 (0x00033464)

### TAG_MAX_SCREEN_LOCK_TIMEOUT_SET

    public static final int TAG_MAX_SCREEN_LOCK_TIMEOUT_SET

Indicates that an admin has set a maximum screen lock timeout. The log entry contains the following information about the event encapsulated in an `Object` array, accessible via `SecurityEvent#getData()`:

- [0] admin package name (`String`)
- [1] admin user ID (`Integer`)
- [2] target user ID (`Integer`)
- [3] new screen lock timeout in milliseconds (`Long`)

  See also:

  - `DevicePolicyManager.setMaximumTimeToLock(ComponentName, long)`

  Constant Value: 210019 (0x00033463)

### TAG_MEDIA_MOUNT

    public static final int TAG_MEDIA_MOUNT

Indicates that removable media has been mounted on the device. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] mount point (`String`)
- [1] volume label (`String`). Redacted to empty string on organization-owned managed profile devices.

  Constant Value: 210013 (0x0003345d)

### TAG_MEDIA_UNMOUNT

    public static final int TAG_MEDIA_UNMOUNT

Indicates that removable media was unmounted from the device. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] mount point (`String`)
- [1] volume label (`String`). Redacted to empty string on organization-owned managed profile devices.

  Constant Value: 210014 (0x0003345e)

### TAG_OS_SHUTDOWN

    public static final int TAG_OS_SHUTDOWN

Indicates that the Android OS has shutdown. There is no extra payload in the log event.

Constant Value: 210010 (0x0003345a)

### TAG_OS_STARTUP

    public static final int TAG_OS_STARTUP

Indicates that the Android OS has started. The log entry contains the following information about the startup time software integrity check encapsulated in an `Object` array, accessible via `SecurityEvent#getData()`:

- [0] Verified Boot state (`String`)
- [1] dm-verity mode (`String`).

  Verified Boot state can be one of the following:

- `green` indicates that there is a full chain of trust extending from the bootloader to verified partitions including the bootloader, boot partition, and all verified partitions.
- `yellow` indicates that the boot partition has been verified using the embedded certificate and the signature is valid.
- `orange` indicates that the device may be freely modified. Device integrity is left to the user to verify out-of-band.

  dm-verity mode can be one of the following:

- `enforcing` indicates that the device will be restarted when corruption is detected.
- `eio` indicates that an I/O error will be returned for an attempt to read corrupted data blocks.
- `disabled` indicates that integrity check is disabled. For details see Verified Boot documentation.

  Constant Value: 210009 (0x00033459)

### TAG_PASSWORD_COMPLEXITY_REQUIRED

    public static final int TAG_PASSWORD_COMPLEXITY_REQUIRED

Indicates that an admin has set a password complexity requirement, using the platform's pre-defined complexity levels. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] admin package name (`String`)
- [1] admin user ID (`Integer`)
- [2] target user ID (`Integer`)
- [3] Password complexity (`Integer`)

  See also:

  - `DevicePolicyManager.setRequiredPasswordComplexity(int)`

  Constant Value: 210035 (0x00033473)

### TAG_PASSWORD_COMPLEXITY_SET

    public static final int TAG_PASSWORD_COMPLEXITY_SET

Indicates that an admin has set a requirement for password complexity. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] admin package name (`String`)
- [1] admin user ID (`Integer`)
- [2] target user ID (`Integer`)
- [3] minimum password length (`Integer`)
- [4] password quality constraint (`Integer`)
- [5] minimum number of letters (`Integer`)
- [6] minimum number of non-letters (`Integer`)
- [7] minimum number of digits (`Integer`)
- [8] minimum number of uppercase letters (`Integer`)
- [9] minimum number of lowercase letters (`Integer`)
- [10] minimum number of symbols (`Integer`)

  See also:

  - `DevicePolicyManager.setPasswordMinimumLength(ComponentName, int)`
  - `DevicePolicyManager.setPasswordQuality(ComponentName, int)`
  - `DevicePolicyManager.setPasswordMinimumLetters(ComponentName, int)`
  - `DevicePolicyManager.setPasswordMinimumNonLetter(ComponentName, int)`
  - `DevicePolicyManager.setPasswordMinimumLowerCase(ComponentName, int)`
  - `DevicePolicyManager.setPasswordMinimumUpperCase(ComponentName, int)`
  - `DevicePolicyManager.setPasswordMinimumNumeric(ComponentName, int)`
  - `DevicePolicyManager.setPasswordMinimumSymbols(ComponentName, int)`

  Constant Value: 210017 (0x00033461)

### TAG_PASSWORD_EXPIRATION_SET

    public static final int TAG_PASSWORD_EXPIRATION_SET

Indicates that an admin has set a password expiration timeout. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] admin package name (`String`)
- [1] admin user ID (`Integer`)
- [2] target user ID (`Integer`)
- [3] new password expiration timeout in milliseconds (`Long`).

  See also:

  - `DevicePolicyManager.setPasswordExpirationTimeout(ComponentName, long)`

  Constant Value: 210016 (0x00033460)

### TAG_PASSWORD_HISTORY_LENGTH_SET

    public static final int TAG_PASSWORD_HISTORY_LENGTH_SET

Indicates that an admin has set a password history length. The log entry contains the following information about the event encapsulated in an `Object` array, accessible via `SecurityEvent#getData()`:

- [0] admin package name (`String`)
- [1] admin user ID (`Integer`)
- [2] target user ID (`Integer`)
- [3] new password history length value (`Integer`)

  See also:

  - `DevicePolicyManager.setPasswordHistoryLength(ComponentName, int)`

  Constant Value: 210018 (0x00033462)

### TAG_REMOTE_LOCK

    public static final int TAG_REMOTE_LOCK

Indicates that an admin remotely locked the device or profile. The log entry contains the following information about the event encapsulated in an `Object` array, accessible via `SecurityEvent#getData()`:

- [0] admin package name (`String`),
- [1] admin user ID (`Integer`).
- [2] target user ID (`Integer`)

  Constant Value: 210022 (0x00033466)

### TAG_SYNC_RECV_FILE

    public static final int TAG_SYNC_RECV_FILE

Indicates that a file was pulled from the device via the adb daemon, for example via `adb pull`. The log entry contains a `String` payload containing the path of the pulled file on the device, accessible via `SecurityEvent#getData()`.

Constant Value: 210003 (0x00033453)

### TAG_SYNC_SEND_FILE

    public static final int TAG_SYNC_SEND_FILE

Indicates that a file was pushed to the device via the adb daemon, for example via `adb push`. The log entry contains a `String` payload containing the destination path of the pushed file, accessible via `SecurityEvent#getData()`.

Constant Value: 210004 (0x00033454)

### TAG_USER_RESTRICTION_ADDED

    public static final int TAG_USER_RESTRICTION_ADDED

Indicates that an admin has set a user restriction. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] admin package name (`String`)
- [1] admin user ID (`Integer`)
- [2] user restriction (`String`)

  See also:

  - `DevicePolicyManager.addUserRestriction(ComponentName, String)`

  Constant Value: 210027 (0x0003346b)

### TAG_USER_RESTRICTION_REMOVED

    public static final int TAG_USER_RESTRICTION_REMOVED

Indicates that an admin has removed a user restriction. The log entry contains the following information about the event, encapsulated in an `Object` array and accessible via `SecurityEvent#getData()`:

- [0] admin package name (`String`)
- [1] admin user ID (`Integer`)
- [2] user restriction (`String`)

  See also:

  - `DevicePolicyManager.clearUserRestriction(ComponentName, String)`

  Constant Value: 210028 (0x0003346c)

### TAG_WIPE_FAILURE

    public static final int TAG_WIPE_FAILURE

Indicates a failure to wipe device or user data. There is no extra payload in the log event.

Constant Value: 210023 (0x00033467)

## Public constructors

### SecurityLog

    public SecurityLog ()

Full name *
Email address *
Company / developer name
One of your Play Store app URLs *
Which best describes your business:*
Apps
Games
Apps & Games
*
*