# Print output for @column tags ?>
Developers

- Design
- Develop
- Distribute

Developer Console

## Most visited

## Recently visited

## Results for

Summary: Nested Classes | Constants | Fields | Methods | Inherited Methods

# TelephonyManager

`public class TelephonyManager`
`extends Object` ``

java.lang.Object
↳ | android.telephony.TelephonyManager

Provides access to information about the telephony services on the device. Applications can use the methods in this class to determine telephony services and states, as well as to access some types of subscriber information. Applications can also register a listener to receive notification of telephony state changes.

The returned TelephonyManager will use the default subscription for all calls. To call an API for a specific subscription, use `createForSubscriptionId(int)`. e.g. `telephonyManager = defaultSubTelephonyManager.createForSubscriptionId(subId);`

Note that access to some telephony information is permission-protected. Your application cannot access the protected information unless it has the appropriate permissions declared in its manifest file. Where permissions apply, they are noted in the the methods through which you access the protected information.

TelephonyManager is intended for use on devices that implement `FEATURE_TELEPHONY`. On devices that do not implement this feature, the behavior is not reliable.

## Summary

### Nested classes
`class` | `TelephonyManager.CallComposerException` Exception that may be supplied to the callback in `TelephonyManager.uploadCallComposerPicture(InputStream, String, Executor, OutcomeReceiver)` if something goes awry.
`class` | `TelephonyManager.CellInfoCallback` Callback for providing asynchronous `CellInfo` on request
`class` | `TelephonyManager.ModemErrorException` Exception that is supplied to the callback in `TelephonyManager.getNetworkSlicingConfiguration(Executor, OutcomeReceiver)` if the modem returned a failure.
`class` | `TelephonyManager.NetworkSlicingException` Exception that may be supplied to the callback in `TelephonyManager.getNetworkSlicingConfiguration(Executor, OutcomeReceiver)` if something goes awry.
`class` | `TelephonyManager.TimeoutException` Exception that is supplied to the callback in `TelephonyManager.getNetworkSlicingConfiguration(Executor, OutcomeReceiver)` if the system timed out waiting for a response from the Radio.
`class` | `TelephonyManager.UssdResponseCallback` Used to notify callers of `TelephonyManager#sendUssdRequest(String, UssdResponseCallback, Handler)` when the network either successfully executes a USSD request, or if there was a failure while executing the request.

### Constants
`String` | `ACTION_CARRIER_MESSAGING_CLIENT_SERVICE` A service action that identifies a `CarrierMessagingClientService` subclass in the AndroidManifest.xml.
`String` | `ACTION_CARRIER_SIGNAL_DEFAULT_NETWORK_AVAILABLE` Broadcast action sent when the availability of the system default network changes.
`String` | `ACTION_CARRIER_SIGNAL_PCO_VALUE` Broadcast action sent when a PCO value becomes available from the modem.
`String` | `ACTION_CARRIER_SIGNAL_REDIRECTED` Broadcast action sent when a data connection is redirected with validation failure.
`String` | `ACTION_CARRIER_SIGNAL_REQUEST_NETWORK_FAILED` Broadcast action sent when a data connection setup fails.
`String` | `ACTION_CARRIER_SIGNAL_RESET` Broadcast action sent when carrier apps should reset their internal state.
`String` | `ACTION_CONFIGURE_VOICEMAIL` Open the voicemail settings activity to make changes to voicemail configuration.
`String` | `ACTION_MULTI_SIM_CONFIG_CHANGED` Broadcast action to be received by Broadcast receivers.
`String` | `ACTION_NETWORK_COUNTRY_CHANGED` Broadcast intent action for network country code changes.
`String` | `ACTION_PHONE_STATE_CHANGED` Broadcast intent action indicating that the call state on the device has changed.
`String` | `ACTION_RESPOND_VIA_MESSAGE` The Phone app sends this intent when a user opts to respond-via-message during an incoming call.
`String` | `ACTION_SECRET_CODE` Broadcast Action: A debug code has been entered in the dialer.
`String` | `ACTION_SHOW_VOICEMAIL_NOTIFICATION` Broadcast intent action for letting the default dialer to know to show voicemail notification.
`String` | `ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED` Broadcast Action: The subscription carrier identity has changed.
`String` | `ACTION_SUBSCRIPTION_SPECIFIC_CARRIER_IDENTITY_CHANGED` Broadcast Action: The subscription specific carrier identity has changed.
`int` | `APPTYPE_CSIM` UICC application type is CSIM
`int` | `APPTYPE_ISIM` UICC application type is ISIM
`int` | `APPTYPE_RUIM` UICC application type is RUIM
`int` | `APPTYPE_SIM` UICC application type is SIM
`int` | `APPTYPE_UNKNOWN` UICC application type is unknown or not specified
`int` | `APPTYPE_USIM` UICC application type is USIM
`int` | `AUTHTYPE_EAP_AKA` Authentication type for UICC challenge is EAP AKA.
`int` | `AUTHTYPE_EAP_SIM` Authentication type for UICC challenge is EAP SIM.
`int` | `CALL_COMPOSER_STATUS_OFF` Call composer status OFF from user setting.
`int` | `CALL_COMPOSER_STATUS_ON` Call composer status ON from user setting.
`int` | `CALL_STATE_IDLE` Device call state: No activity.
`int` | `CALL_STATE_OFFHOOK` Device call state: Off-hook.
`int` | `CALL_STATE_RINGING` Device call state: Ringing.
`String` | `CAPABILITY_SLICING_CONFIG_SUPPORTED` Indicates whether `getNetworkSlicingConfiguration(Executor, OutcomeReceiver)` is supported.
`int` | `CDMA_ROAMING_MODE_AFFILIATED` Value for `CarrierConfigManager#KEY_CDMA_ROAMING_MODE_INT` which permits roaming on affiliated networks.
`int` | `CDMA_ROAMING_MODE_ANY` Value for `CarrierConfigManager#KEY_CDMA_ROAMING_MODE_INT` which permits roaming on any network.
`int` | `CDMA_ROAMING_MODE_HOME` Value for `CarrierConfigManager#KEY_CDMA_ROAMING_MODE_INT` which only permits connections on home networks.
`int` | `CDMA_ROAMING_MODE_RADIO_DEFAULT` Value for `CarrierConfigManager#KEY_CDMA_ROAMING_MODE_INT` which leaves the roaming mode set to the radio default or to the user's preference if they've indicated one.
`int` | `DATA_ACTIVITY_DORMANT` Data connection is active, but physical link is down
`int` | `DATA_ACTIVITY_IN` Data connection activity: Currently receiving IP PPP traffic.
`int` | `DATA_ACTIVITY_INOUT` Data connection activity: Currently both sending and receiving IP PPP traffic.
`int` | `DATA_ACTIVITY_NONE` Data connection activity: No traffic.
`int` | `DATA_ACTIVITY_OUT` Data connection activity: Currently sending IP PPP traffic.
`int` | `DATA_CONNECTED` Data connection state: Connected.
`int` | `DATA_CONNECTING` Data connection state: Currently setting up a data connection.
`int` | `DATA_DISCONNECTED` Data connection state: Disconnected.
`int` | `DATA_DISCONNECTING` Data connection state: Disconnecting.
`int` | `DATA_ENABLED_REASON_CARRIER` To indicate enable or disable carrier data by the system based on carrier signalling or carrier privileged apps.
`int` | `DATA_ENABLED_REASON_POLICY` To indicate that data control due to policy.
`int` | `DATA_ENABLED_REASON_THERMAL` To indicate enable or disable data by thermal service.
`int` | `DATA_ENABLED_REASON_USER` To indicate that user enabled or disabled data.
`int` | `DATA_SUSPENDED` Data connection state: Suspended.
`int` | `DATA_UNKNOWN` Data connection state: Unknown.
`int` | `ERI_FLASH` ERI (Enhanced Roaming Indicator) is FLASH i.e value 2 defined by 3GPP2 C.R1001-H v1.0 Table 8.1-1.
`int` | `ERI_OFF` ERI (Enhanced Roaming Indicator) is OFF i.e value 1 defined by 3GPP2 C.R1001-H v1.0 Table 8.1-1.
`int` | `ERI_ON` ERI (Enhanced Roaming Indicator) is ON i.e value 0 defined by 3GPP2 C.R1001-H v1.0 Table 8.1-1.
`String` | `EXTRA_ACTIVE_SIM_SUPPORTED_COUNT` The number of active SIM supported by current multi-SIM config.
`String` | `EXTRA_APN_PROTOCOL` An integer extra containing the protocol of the apn connection.
`String` | `EXTRA_APN_TYPE` An integer extra containing the APN type.
`String` | `EXTRA_CALL_VOICEMAIL_INTENT` The intent to call voicemail.
`String` | `EXTRA_CARRIER_ID` An int extra used with `ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED` which indicates the updated carrier id returned by `TelephonyManager#getSimCarrierId()`.
`String` | `EXTRA_CARRIER_NAME` An string extra used with `ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED` which indicates the updated carrier name of the current subscription.
`String` | `EXTRA_DATA_FAIL_CAUSE` An integer extra containing the data fail cause.
`String` | `EXTRA_DEFAULT_NETWORK_AVAILABLE` A boolean extra indicating the availability of the default network.
`String` | `EXTRA_HIDE_PUBLIC_SETTINGS` The boolean value indicating whether the voicemail settings activity launched by `ACTION_CONFIGURE_VOICEMAIL` should hide settings accessible through public API.
`String` | `EXTRA_INCOMING_NUMBER` This constant is deprecated. Companion apps for wearable devices should use the `InCallService` API to retrieve the phone number for calls instead. Apps performing call screening should use the `CallScreeningService` API instead.
`String` | `EXTRA_IS_REFRESH` Boolean value representing whether the `ACTION_SHOW_VOICEMAIL_NOTIFICATION` is new or a refresh of an existing notification.
`String` | `EXTRA_LAUNCH_VOICEMAIL_SETTINGS_INTENT` The intent to launch voicemail settings.
`String` | `EXTRA_NETWORK_COUNTRY` The extra used with an `ACTION_NETWORK_COUNTRY_CHANGED` to specify the the country code in ISO-3166-1 alpha-2 format.
`String` | `EXTRA_NOTIFICATION_COUNT` The number of voice messages associated with the notification.
`String` | `EXTRA_PCO_ID` An integer extra indicating the ID for the PCO data.
`String` | `EXTRA_PCO_VALUE` A byte array extra containing PCO data read from the modem.
`String` | `EXTRA_PHONE_ACCOUNT_HANDLE` The extra used with an `ACTION_CONFIGURE_VOICEMAIL` and `ACTION_SHOW_VOICEMAIL_NOTIFICATION` `Intent` to specify the `PhoneAccountHandle` the configuration or notification is for.
`String` | `EXTRA_REDIRECTION_URL` String extra containing the redirection URL sent with `ACTION_CARRIER_SIGNAL_REDIRECTED`.
`String` | `EXTRA_SPECIFIC_CARRIER_ID` An int extra used with `ACTION_SUBSCRIPTION_SPECIFIC_CARRIER_IDENTITY_CHANGED` which indicates the updated specific carrier id returned by `TelephonyManager#getSimSpecificCarrierId()`.
`String` | `EXTRA_SPECIFIC_CARRIER_NAME` An string extra used with `ACTION_SUBSCRIPTION_SPECIFIC_CARRIER_IDENTITY_CHANGED` which indicates the updated specific carrier name returned by `TelephonyManager#getSimSpecificCarrierIdName()`.
`String` | `EXTRA_STATE` The lookup key used with the `ACTION_PHONE_STATE_CHANGED` broadcast for a String containing the new call state.
`String` | `EXTRA_SUBSCRIPTION_ID` An int extra used with `ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED` to indicate the subscription which has changed; or in general whenever a subscription ID needs specified.
`String` | `EXTRA_VOICEMAIL_NUMBER` The voicemail number.
`String` | `METADATA_HIDE_VOICEMAIL_SETTINGS_MENU` A boolean meta-data value indicating whether the voicemail settings should be hidden in the call settings page launched by `TelecomManager.ACTION_SHOW_CALL_SETTINGS`.
`int` | `MULTISIM_ALLOWED` The usage of multiple SIM cards at the same time to register on the network (e.g. Dual Standby or Dual Active) is supported.
`int` | `MULTISIM_NOT_SUPPORTED_BY_CARRIER` The usage of multiple SIM cards at the same time to register on the network (e.g. Dual Standby or Dual Active) is supported by the hardware, but restricted by the carrier.
`int` | `MULTISIM_NOT_SUPPORTED_BY_HARDWARE` The usage of multiple SIM cards at the same time to register on the network (e.g. Dual Standby or Dual Active) is not supported by the hardware.
`int` | `NETWORK_SELECTION_MODE_AUTO`
`int` | `NETWORK_SELECTION_MODE_MANUAL`
`int` | `NETWORK_SELECTION_MODE_UNKNOWN`
`int` | `NETWORK_TYPE_1xRTT` Current network is 1xRTT
`int` | `NETWORK_TYPE_CDMA` Current network is CDMA: Either IS95A or IS95B
`int` | `NETWORK_TYPE_EDGE` Current network is EDGE
`int` | `NETWORK_TYPE_EHRPD` Current network is eHRPD
`int` | `NETWORK_TYPE_EVDO_0` Current network is EVDO revision 0
`int` | `NETWORK_TYPE_EVDO_A` Current network is EVDO revision A
`int` | `NETWORK_TYPE_EVDO_B` Current network is EVDO revision B
`int` | `NETWORK_TYPE_GPRS` Current network is GPRS
`int` | `NETWORK_TYPE_GSM` Current network is GSM
`int` | `NETWORK_TYPE_HSDPA` Current network is HSDPA
`int` | `NETWORK_TYPE_HSPA` Current network is HSPA
`int` | `NETWORK_TYPE_HSPAP` Current network is HSPA+
`int` | `NETWORK_TYPE_HSUPA` Current network is HSUPA
`int` | `NETWORK_TYPE_IDEN` Current network is iDen
`int` | `NETWORK_TYPE_IWLAN` Current network is IWLAN
`int` | `NETWORK_TYPE_LTE` Current network is LTE
`int` | `NETWORK_TYPE_NR` Current network is NR (New Radio) 5G.
`int` | `NETWORK_TYPE_TD_SCDMA` Current network is TD_SCDMA
`int` | `NETWORK_TYPE_UMTS` Current network is UMTS
`int` | `NETWORK_TYPE_UNKNOWN` Network type is unknown
`int` | `PHONE_TYPE_CDMA` Phone radio is CDMA.
`int` | `PHONE_TYPE_GSM` Phone radio is GSM.
`int` | `PHONE_TYPE_NONE` No phone radio.
`int` | `PHONE_TYPE_SIP` Phone is via SIP.
`int` | `SET_OPPORTUNISTIC_SUB_INACTIVE_SUBSCRIPTION` The subscription is not valid.
`int` | `SET_OPPORTUNISTIC_SUB_NO_OPPORTUNISTIC_SUB_AVAILABLE` The subscription is not valid.
`int` | `SET_OPPORTUNISTIC_SUB_REMOTE_SERVICE_EXCEPTION` Subscription service happened remote exception.
`int` | `SET_OPPORTUNISTIC_SUB_SUCCESS` No error.
`int` | `SET_OPPORTUNISTIC_SUB_VALIDATION_FAILED` Validation failed when trying to switch to preferred subscription.
`int` | `SIM_STATE_ABSENT` SIM card state: no SIM card is available in the device
`int` | `SIM_STATE_CARD_IO_ERROR` SIM card state: SIM Card Error, present but faulty
`int` | `SIM_STATE_CARD_RESTRICTED` SIM card state: SIM Card restricted, present but not usable due to carrier restrictions.
`int` | `SIM_STATE_NETWORK_LOCKED` SIM card state: Locked: requires a network PIN to unlock
`int` | `SIM_STATE_NOT_READY` SIM card state: SIM Card is NOT READY
`int` | `SIM_STATE_PERM_DISABLED` SIM card state: SIM Card Error, permanently disabled
`int` | `SIM_STATE_PIN_REQUIRED` SIM card state: Locked: requires the user's SIM PIN to unlock
`int` | `SIM_STATE_PUK_REQUIRED` SIM card state: Locked: requires the user's SIM PUK to unlock
`int` | `SIM_STATE_READY` SIM card state: Ready
`int` | `SIM_STATE_UNKNOWN` SIM card state: Unknown.
`int` | `UNINITIALIZED_CARD_ID` A UICC card identifier used before the UICC card is loaded.
`int` | `UNKNOWN_CARRIER_ID` An unknown carrier id.
`int` | `UNSUPPORTED_CARD_ID` A UICC card identifier used if the device does not support the operation.
`int` | `UPDATE_AVAILABLE_NETWORKS_ABORTED` The request is aborted.
`int` | `UPDATE_AVAILABLE_NETWORKS_DISABLE_MODEM_FAIL` Disable modem fail.
`int` | `UPDATE_AVAILABLE_NETWORKS_ENABLE_MODEM_FAIL` Enable modem fail.
`int` | `UPDATE_AVAILABLE_NETWORKS_INVALID_ARGUMENTS` The parameter passed in is invalid.
`int` | `UPDATE_AVAILABLE_NETWORKS_MULTIPLE_NETWORKS_NOT_SUPPORTED` Carrier app does not support multiple available networks.
`int` | `UPDATE_AVAILABLE_NETWORKS_NO_CARRIER_PRIVILEGE` No carrier privilege.
`int` | `UPDATE_AVAILABLE_NETWORKS_NO_OPPORTUNISTIC_SUB_AVAILABLE` The subscription is not valid.
`int` | `UPDATE_AVAILABLE_NETWORKS_REMOTE_SERVICE_EXCEPTION` There is no OpportunisticNetworkService.
`int` | `UPDATE_AVAILABLE_NETWORKS_SERVICE_IS_DISABLED` OpportunisticNetworkService is disabled.
`int` | `UPDATE_AVAILABLE_NETWORKS_SUCCESS` No error.
`int` | `UPDATE_AVAILABLE_NETWORKS_UNKNOWN_FAILURE` There is a unknown failure happened.
`int` | `USSD_ERROR_SERVICE_UNAVAIL` Failure code returned when a USSD request has failed to execute because the Telephony service is unavailable.
`int` | `USSD_RETURN_FAILURE` Failed code returned when the mobile network has failed to complete a USSD request.
`String` | `VVM_TYPE_CVVM` A flavor of OMTP protocol with a different mobile originated (MO) format
`String` | `VVM_TYPE_OMTP` The OMTP protocol.

### Fields
`public static final String` | `EXTRA_STATE_IDLE` Value used with `EXTRA_STATE` corresponding to `CALL_STATE_IDLE`.
`public static final String` | `EXTRA_STATE_OFFHOOK` Value used with `EXTRA_STATE` corresponding to `CALL_STATE_OFFHOOK`.
`public static final String` | `EXTRA_STATE_RINGING` Value used with `EXTRA_STATE` corresponding to `CALL_STATE_RINGING`.

### Public methods
`boolean` | `canChangeDtmfToneLength()` Whether the device supports configuring the DTMF tone length.
`void` | `clearSignalStrengthUpdateRequest(SignalStrengthUpdateRequest request)` Clear a `SignalStrengthUpdateRequest` from the system.
`TelephonyManager` | `createForPhoneAccountHandle(PhoneAccountHandle phoneAccountHandle)` Create a new TelephonyManager object pinned to the subscription ID associated with the given phone account.
`TelephonyManager` | `createForSubscriptionId(int subId)` Create a new TelephonyManager object pinned to the given subscription ID.
`boolean` | `doesSwitchMultiSimConfigTriggerReboot()` Get whether making changes to modem configurations by `switchMultiSimConfig(int)` will trigger device reboot.
`int` | `getActiveModemCount()` Returns the number of logical modems currently configured to be activated.
`List<CellInfo>` | `getAllCellInfo()` Requests all available cell information from all radios on the device including the camped/registered, serving, and neighboring cells.
`int` | `getCallComposerStatus()` Get the user-set status for enriched calling with call composer.
`int` | `getCallState()` This method is deprecated. Use `getCallStateForSubscription()` to retrieve the call state for a specific telephony subscription (which allows carrier privileged apps), `TelephonyCallback.CallStateListener` for real-time call state updates, or `TelecomManager#isInCall()`, which supplies an aggregate "in call" state for the entire device.
`int` | `getCallStateForSubscription()` Retrieve the call state for a specific subscription that was specified when this TelephonyManager instance was created.
`int` | `getCardIdForDefaultEuicc()` Get the card ID of the default eUICC card.
`PersistableBundle` | `getCarrierConfig()` Returns the carrier config of the subscription ID pinned to the TelephonyManager.
`int` | `getCarrierIdFromSimMccMnc()` Returns carrier id based on sim MCCMNC (returned by `getSimOperator()`) only.
`CellLocation` | `getCellLocation()` This method is deprecated. use `getAllCellInfo()` instead, which returns a superset of this API.
`int` | `getDataActivity()` Returns a constant indicating the type of activity on a data connection (cellular).
`int` | `getDataNetworkType()` Returns a constant indicating the radio technology (network type) currently in use on the device for data transmission.
`int` | `getDataState()` Returns a constant indicating the current data connection state (cellular).
`String` | `getDeviceId()` This method is deprecated. Use `getImei()` which returns IMEI for GSM or `getMeid()` which returns MEID for CDMA.
`String` | `getDeviceId(int slotIndex)` This method is deprecated. Use `getImei()` which returns IMEI for GSM or `getMeid()` which returns MEID for CDMA.
`String` | `getDeviceSoftwareVersion()` Returns the software version number for the device, for example, the IMEI/SV for GSM phones.
`Map<Integer, List<EmergencyNumber>>` | `getEmergencyNumberList()` Get the emergency number list based on current locale, sim, default, modem and network.
`Map<Integer, List<EmergencyNumber>>` | `getEmergencyNumberList(int categories)` Get the per-category emergency number list based on current locale, sim, default, modem and network.
`List<String>` | `getEquivalentHomePlmns()` Returns a list of the equivalent home PLMNs (EF_EHPLMN) from the USIM app.
`String[]` | `getForbiddenPlmns()` Returns an array of Forbidden PLMNs from the USIM App Returns null if the query fails.
`String` | `getGroupIdLevel1()` Returns the Group Identifier Level1 for a GSM phone.
`String` | `getIccAuthentication(int appType, int authType, String data)` Returns the response of authentication for the default subscription.
`String` | `getImei(int slotIndex)` Returns the IMEI (International Mobile Equipment Identity).
`String` | `getImei()` Returns the IMEI (International Mobile Equipment Identity).
`String` | `getLine1Number()` Returns the phone number string for line 1, for example, the MSISDN for a GSM phone for a particular subscription.
`String` | `getManualNetworkSelectionPlmn()` Get the PLMN chosen for Manual Network Selection if active.
`String` | `getManufacturerCode(int slotIndex)` Returns the Manufacturer Code from the MEID.
`String` | `getManufacturerCode()` Returns the Manufacturer Code from the MEID.
`static long` | `getMaximumCallComposerPictureSize()` Indicates the maximum size of the call composure picture.
`String` | `getMeid()` Returns the MEID (Mobile Equipment Identifier).
`String` | `getMeid(int slotIndex)` Returns the MEID (Mobile Equipment Identifier).
`String` | `getMmsUAProfUrl()` Returns the MMS user agent profile URL.
`String` | `getMmsUserAgent()` Returns the MMS user agent.
`String` | `getNai()` Returns the Network Access Identifier (NAI).
`String` | `getNetworkCountryIso()` Returns the ISO-3166-1 alpha-2 country code equivalent of the MCC (Mobile Country Code) of the current registered operator or the cell nearby, if available.
`String` | `getNetworkCountryIso(int slotIndex)` Returns the ISO-3166-1 alpha-2 country code equivalent of the MCC (Mobile Country Code) of the current registered operator or the cell nearby, if available.
`String` | `getNetworkOperator()` Returns the numeric name (MCC+MNC) of current registered operator.
`String` | `getNetworkOperatorName()` Returns the alphabetic name of current registered operator.
`int` | `getNetworkSelectionMode()` Get the network selection mode.
`void` | `getNetworkSlicingConfiguration(Executor executor, OutcomeReceiver<NetworkSlicingConfig, TelephonyManager.NetworkSlicingException> callback)` Request to get the current slicing configuration including URSP rules and NSSAIs (configured, allowed and rejected).
`String` | `getNetworkSpecifier()` Returns the network specifier of the subscription ID pinned to the TelephonyManager.
`int` | `getNetworkType()` This method is deprecated. use `getDataNetworkType()`
`PhoneAccountHandle` | `getPhoneAccountHandle()` Determines the `PhoneAccountHandle` associated with this TelephonyManager.
`int` | `getPhoneCount()` This method is deprecated. Use `getActiveModemCount()` instead.
`int` | `getPhoneType()` Returns a constant indicating the device phone type.
`int` | `getPreferredOpportunisticDataSubscription()` Get preferred opportunistic data subscription Id Requires that the calling app has carrier privileges (see `hasCarrierPrivileges()`), or has either READ_PRIVILEGED_PHONE_STATE or `READ_PHONE_STATE` permission.
`ServiceState` | `getServiceState()` Returns the current `ServiceState` information.
`SignalStrength` | `getSignalStrength()` Get the most recently available signal strength information.
`int` | `getSimCarrierId()` Returns carrier id of the current subscription.
`CharSequence` | `getSimCarrierIdName()` Returns carrier id name of the current subscription.
`String` | `getSimCountryIso()` Returns the ISO-3166-1 alpha-2 country code equivalent for the SIM provider's country code.
`String` | `getSimOperator()` Returns the MCC+MNC (mobile country code + mobile network code) of the provider of the SIM.
`String` | `getSimOperatorName()` Returns the Service Provider Name (SPN).
`String` | `getSimSerialNumber()` Returns the serial number of the SIM, if applicable.
`int` | `getSimSpecificCarrierId()` Returns fine-grained carrier ID of the current subscription.
`CharSequence` | `getSimSpecificCarrierIdName()` Similar like `getSimCarrierIdName()`, returns user-facing name of the specific carrier id returned by `getSimSpecificCarrierId()`.
`int` | `getSimState()` Returns a constant indicating the state of the default SIM card.
`int` | `getSimState(int slotIndex)` Returns a constant indicating the state of the device SIM card in a logical slot.
`String` | `getSubscriberId()` Returns the unique subscriber ID, for example, the IMSI for a GSM phone.
`int` | `getSubscriptionId(PhoneAccountHandle phoneAccountHandle)` Returns the subscription ID for the given phone account handle.
`int` | `getSubscriptionId()` Return an appropriate subscription ID for any situation.
`int` | `getSupportedModemCount()` Return how many logical modem can be potentially active simultaneously, in terms of hardware capability.
`String` | `getTypeAllocationCode()` Returns the Type Allocation Code from the IMEI.
`String` | `getTypeAllocationCode(int slotIndex)` Returns the Type Allocation Code from the IMEI.
`List<UiccCardInfo>` | `getUiccCardsInfo()` Gets information about currently inserted UICCs and eUICCs.
`String` | `getVisualVoicemailPackageName()` Returns the package responsible of processing visual voicemail for the subscription ID pinned to the TelephonyManager.
`String` | `getVoiceMailAlphaTag()` Retrieves the alphabetic identifier associated with the voice mail number.
`String` | `getVoiceMailNumber()` Returns the voice mail number.
`int` | `getVoiceNetworkType()` Returns the NETWORK_TYPE_xxxx for voice Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
`Uri` | `getVoicemailRingtoneUri(PhoneAccountHandle accountHandle)` Returns the URI for the per-account voicemail ringtone set in Phone settings.
`boolean` | `hasCarrierPrivileges()` Has the calling application been granted carrier privileges by the carrier.
`boolean` | `hasIccCard()`
`boolean` | `iccCloseLogicalChannel(int channel)` This method is deprecated. Use `SEService` APIs instead. See `Channel.close()`.
`byte[]` | `iccExchangeSimIO(int fileID, int command, int p1, int p2, int p3, String filePath)` This method is deprecated. Use `SEService` APIs instead. See `SEService.getUiccReader(int)`, `Reader.openSession()`, `Session.openBasicChannel(byte[], byte)`, `Channel.transmit(byte[])`.
`IccOpenLogicalChannelResponse` | `iccOpenLogicalChannel(String AID, int p2)` This method is deprecated. Use `SEService` APIs instead. See `SEService.getUiccReader(int)`, `Reader.openSession()`, `Session.openLogicalChannel(byte[], byte)`.
`IccOpenLogicalChannelResponse` | `iccOpenLogicalChannel(String AID)` This method is deprecated. Replaced by `iccOpenLogicalChannel(java.lang.String, int)`
`String` | `iccTransmitApduBasicChannel(int cla, int instruction, int p1, int p2, int p3, String data)` This method is deprecated. Use `SEService` APIs instead. See `SEService.getUiccReader(int)`, `Reader.openSession()`, `Session.openBasicChannel(byte[], byte)`, `Channel.transmit(byte[])`.
`String` | `iccTransmitApduLogicalChannel(int channel, int cla, int instruction, int p1, int p2, int p3, String data)` This method is deprecated. Use `SEService` APIs instead. See `Channel.transmit(byte[])`.
`boolean` | `isConcurrentVoiceAndDataSupported()` Whether the device is currently on a technology (e.g. UMTS or LTE) which can support voice and data simultaneously.
`boolean` | `isDataCapable()`
`boolean` | `isDataConnectionAllowed()` Checks whether cellular data connection is allowed in the device.
`boolean` | `isDataEnabled()` Returns whether mobile data is enabled or not per user setting.
`boolean` | `isDataEnabledForReason(int reason)` Return whether data is enabled for certain reason .
`boolean` | `isDataRoamingEnabled()` Returns whether mobile data roaming is enabled on the subscription.
`boolean` | `isEmergencyNumber(String number)` Identifies if the supplied phone number is an emergency number that matches a known emergency number based on current locale, SIM card(s), Android database, modem, network, or defaults.
`boolean` | `isHearingAidCompatibilitySupported()` Whether the phone supports hearing aid compatibility.
`boolean` | `isManualNetworkSelectionAllowed()` Checks if manual network selection is allowed.
`boolean` | `isModemEnabledForSlot(int slotIndex)` It indicates whether modem is enabled or not per slot.
`int` | `isMultiSimSupported()` Returns if the usage of multiple SIM cards at the same time to register on the network (e.g. Dual Standby or Dual Active) is supported by the device and by the carrier.
`boolean` | `isNetworkRoaming()` Returns true if the device is considered roaming on the current network, for GSM purposes.
`boolean` | `isRadioInterfaceCapabilitySupported(String capability)` Whether the device supports a given capability on the radio interface.
`boolean` | `isRttSupported()` Determines whether the device currently supports RTT (Real-time text).
`boolean` | `isSmsCapable()`
`boolean` | `isTtyModeSupported()` This method is deprecated. Use `TelecomManager#isTtySupported()` instead Whether the phone supports TTY mode.
`boolean` | `isVoiceCapable()`
`boolean` | `isVoicemailVibrationEnabled(PhoneAccountHandle accountHandle)` Returns whether vibration is set for voicemail notification in Phone settings.
`boolean` | `isWorldPhone()` Whether the device is a world phone.
`void` | `listen(PhoneStateListener listener, int events)` This method is deprecated. Use `registerTelephonyCallback(java.util.concurrent.Executor, android.telephony.TelephonyCallback)`.
`void` | `registerTelephonyCallback(Executor executor, TelephonyCallback callback)` Registers a callback object to receive notification of changes in specified telephony states.
`void` | `requestCellInfoUpdate(Executor executor, TelephonyManager.CellInfoCallback callback)` Requests all available cell information from the current subscription for observed camped/registered, serving, and neighboring cells.
`NetworkScan` | `requestNetworkScan(NetworkScanRequest request, Executor executor, TelephonyScanManager.NetworkScanCallback callback)` Request a network scan.
`void` | `sendDialerSpecialCode(String inputCode)` Send the special dialer code.
`String` | `sendEnvelopeWithStatus(String content)` This method is deprecated. Use `SEService` APIs instead. See `SEService.getUiccReader(int)`, `Reader.openSession()`, `Session.openBasicChannel(byte[], byte)`, `Channel.transmit(byte[])`.
`void` | `sendUssdRequest(String ussdRequest, TelephonyManager.UssdResponseCallback callback, Handler handler)` Sends an Unstructured Supplementary Service Data (USSD) request to the mobile network and informs the caller of the response via the supplied `callback`.
`void` | `sendVisualVoicemailSms(String number, int port, String text, PendingIntent sentIntent)` Send a visual voicemail SMS.
`void` | `setCallComposerStatus(int status)` Set the user-set status for enriched calling with call composer.
`void` | `setDataEnabled(boolean enable)` This method is deprecated. use setDataEnabledForReason with reason DATA_ENABLED_REASON_USER instead.
`void` | `setDataEnabledForReason(int reason, boolean enabled)` Control of data connection and provide the reason triggering the data connection control.
`int` | `setForbiddenPlmns(List<String> fplmns)` Replace the contents of the forbidden PLMN SIM file with the provided values.
`boolean` | `setLine1NumberForDisplay(String alphaTag, String number)` Set the line 1 phone number string and its alphatag for the current ICCID for display purpose only, for example, displayed in Phone Status.
`void` | `setNetworkSelectionModeAutomatic()` Sets the network selection mode to automatic.
`boolean` | `setNetworkSelectionModeManual(String operatorNumeric, boolean persistSelection, int ran)` Ask the radio to connect to the input network and change selection mode to manual.
`boolean` | `setNetworkSelectionModeManual(String operatorNumeric, boolean persistSelection)` Ask the radio to connect to the input network and change selection mode to manual.
`boolean` | `setOperatorBrandOverride(String brand)` Override the branding for the current ICCID.
`boolean` | `setPreferredNetworkTypeToGlobal()` Set the preferred network type to global mode which includes NR, LTE, CDMA, EvDo and GSM/WCDMA.
`void` | `setPreferredOpportunisticDataSubscription(int subId, boolean needValidation, Executor executor, Consumer<Integer> callback)` Set preferred opportunistic data subscription id.
`void` | `setSignalStrengthUpdateRequest(SignalStrengthUpdateRequest request)` Set a `SignalStrengthUpdateRequest` to receive notification when signal quality measurements breach the specified thresholds.
`void` | `setVisualVoicemailSmsFilterSettings(VisualVoicemailSmsFilterSettings settings)` Set the visual voicemail SMS filter settings for the subscription ID pinned to the TelephonyManager.
`boolean` | `setVoiceMailNumber(String alphaTag, String number)` Sets the voice mail number.
`void` | `setVoicemailRingtoneUri(PhoneAccountHandle phoneAccountHandle, Uri uri)` This method is deprecated. Use `Settings.ACTION_CHANNEL_NOTIFICATION_SETTINGS` instead.
`void` | `setVoicemailVibrationEnabled(PhoneAccountHandle phoneAccountHandle, boolean enabled)` This method is deprecated. Use `Settings.ACTION_CHANNEL_NOTIFICATION_SETTINGS` instead.
`void` | `switchMultiSimConfig(int numOfSims)` Switch configs to enable multi-sim or switch back to single-sim Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
`void` | `unregisterTelephonyCallback(TelephonyCallback callback)` Unregister an existing `TelephonyCallback`.
`void` | `updateAvailableNetworks(List<AvailableNetworkInfo> availableNetworks, Executor executor, Consumer<Integer> callback)` Update availability of a list of networks in the current location.
`void` | `uploadCallComposerPicture(InputStream pictureToUpload, String contentType, Executor executor, OutcomeReceiver<ParcelUuid, TelephonyManager.CallComposerException> callback)` Uploads a picture to the carrier network for use with call composer.
`void` | `uploadCallComposerPicture(Path pictureToUpload, String contentType, Executor executor, OutcomeReceiver<ParcelUuid, TelephonyManager.CallComposerException> callback)` Uploads a picture to the carrier network for use with call composer.

### Inherited methods
From class `java.lang.Object`
`Object` | `clone()` Creates and returns a copy of this object.
`boolean` | `equals(Object obj)` Indicates whether some other object is "equal to" this one.
`void` | `finalize()` Called by the garbage collector on an object when garbage collection determines that there are no more references to the object.
`final Class<?>` | `getClass()` Returns the runtime class of this `Object`.
`int` | `hashCode()` Returns a hash code value for the object.
`final void` | `notify()` Wakes up a single thread that is waiting on this object's monitor.
`final void` | `notifyAll()` Wakes up all threads that are waiting on this object's monitor.
`String` | `toString()` Returns a string representation of the object.
`final void` | `wait(long timeout, int nanos)` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object, or some other thread interrupts the current thread, or a certain amount of real time has elapsed.
`final void` | `wait(long timeout)` Causes the current thread to wait until either another thread invokes the `notify()` method or the `notifyAll()` method for this object, or a specified amount of time has elapsed.
`final void` | `wait()` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object.

## Constants

### ACTION_CARRIER_MESSAGING_CLIENT_SERVICE

    public static final String ACTION_CARRIER_MESSAGING_CLIENT_SERVICE

A service action that identifies a `CarrierMessagingClientService` subclass in the AndroidManifest.xml.

See `CarrierMessagingClientService` for the details.

Constant Value: "android.telephony.action.CARRIER_MESSAGING_CLIENT_SERVICE"

### ACTION_CARRIER_SIGNAL_DEFAULT_NETWORK_AVAILABLE

    public static final String ACTION_CARRIER_SIGNAL_DEFAULT_NETWORK_AVAILABLE

Broadcast action sent when the availability of the system default network changes.

See also:

- `This action is intended for carrier apps to set/reset carrier actions. It is only sent to the carrier apps specified in the carrier config for the subscription ID attached to this intent. The intent will have the following extra values:
  - {@link #EXTRA_DEFAULT_NETWORK_AVAILABLE}
    {@code true} if the default network is now available, {@code false} otherwise.
  - {@link android.telephony.SubscriptionManager#EXTRA_SUBSCRIPTION_INDEX SubscriptionManager#EXTRA_SUBSCRIPTION_INDEX}
    The subscription ID on which the default network availability changed.

  This is a protected intent that can only be sent by the system.

  `

Constant Value: "android.telephony.action.CARRIER_SIGNAL_DEFAULT_NETWORK_AVAILABLE"

### ACTION_CARRIER_SIGNAL_PCO_VALUE

    public static final String ACTION_CARRIER_SIGNAL_PCO_VALUE

Broadcast action sent when a PCO value becomes available from the modem. This action is intended for sim/account status checks and only sent to the carrier apps specified in the carrier config for the subscription ID that's attached to this intent. The intent will have the following extra values:

- `EXTRA_APN_TYPE`
  An integer indicating the apn type.
- `EXTRA_APN_PROTOCOL`
  An integer indicating the protocol of the apn connection
- `EXTRA_PCO_ID`
  An integer indicating the PCO id for the data.
- `EXTRA_PCO_VALUE`
  A byte array of PCO data read from modem.
- `SubscriptionManager#EXTRA_SUBSCRIPTION_INDEX`
  The subscription ID for which the PCO info was received.

This is a protected intent that can only be sent by the system.

Constant Value: "android.telephony.action.CARRIER_SIGNAL_PCO_VALUE"

### ACTION_CARRIER_SIGNAL_REDIRECTED

    public static final String ACTION_CARRIER_SIGNAL_REDIRECTED

Broadcast action sent when a data connection is redirected with validation failure. This action is intended for sim/account status checks and only sent to the carrier apps specified in the carrier config for the subscription ID that's attached to this intent. The intent will have the following extra values:

- `EXTRA_APN_TYPE`
  An integer indicating the apn type.
- `EXTRA_REDIRECTION_URL`
  A string indicating the redirection url
- `SubscriptionManager#EXTRA_SUBSCRIPTION_INDEX`
  The subscription ID on which the validation failure happened.

This is a protected intent that can only be sent by the system.

Constant Value: "android.telephony.action.CARRIER_SIGNAL_REDIRECTED"

### ACTION_CARRIER_SIGNAL_REQUEST_NETWORK_FAILED

    public static final String ACTION_CARRIER_SIGNAL_REQUEST_NETWORK_FAILED

Broadcast action sent when a data connection setup fails. This action is intended for sim/account status checks and only sent to the carrier apps specified in the carrier config for the subscription ID that's attached to this intent. The intent will have the following extra values:

- `EXTRA_APN_TYPE`
  An integer indicating the apn type.
- `EXTRA_DATA_FAIL_CAUSE`
  A integer indicating the data fail cause.
- `SubscriptionManager#EXTRA_SUBSCRIPTION_INDEX`
  The subscription ID on which the data setup failure happened.

This is a protected intent that can only be sent by the system.

Constant Value: "android.telephony.action.CARRIER_SIGNAL_REQUEST_NETWORK_FAILED"

### ACTION_CARRIER_SIGNAL_RESET

    public static final String ACTION_CARRIER_SIGNAL_RESET

Broadcast action sent when carrier apps should reset their internal state. Sent when certain events such as turning on/off mobile data, removing the SIM, etc. require carrier apps to reset their state. This action is intended to signal carrier apps to perform cleanup operations. It is only sent to the carrier apps specified in the carrier config for the subscription ID attached to this intent. The intent will have the following extra values:

- `SubscriptionManager#EXTRA_SUBSCRIPTION_INDEX`
  The subscription ID for which state should be reset.

This is a protected intent that can only be sent by the system.

Constant Value: "android.telephony.action.CARRIER_SIGNAL_RESET"

### ACTION_CONFIGURE_VOICEMAIL

    public static final String ACTION_CONFIGURE_VOICEMAIL

Open the voicemail settings activity to make changes to voicemail configuration.

The `EXTRA_PHONE_ACCOUNT_HANDLE` extra indicates which `PhoneAccountHandle` to configure voicemail. The `EXTRA_HIDE_PUBLIC_SETTINGS` hides settings the dialer will modify through public API if set.

See also:

- `EXTRA_PHONE_ACCOUNT_HANDLE`
- `EXTRA_HIDE_PUBLIC_SETTINGS`

Constant Value: "android.telephony.action.CONFIGURE_VOICEMAIL"

### ACTION_MULTI_SIM_CONFIG_CHANGED

    public static final String ACTION_MULTI_SIM_CONFIG_CHANGED

Broadcast action to be received by Broadcast receivers. Indicates multi-SIM configuration is changed. For example, it changed from single SIM capable to dual-SIM capable (DSDS or DSDA) or triple-SIM mode. It doesn't indicate how many subscriptions are actually active, or which states SIMs are, or that all steps during multi-SIM change are done. To know those information you still need to listen to SIM_STATE changes or active subscription changes. See extra of `EXTRA_ACTIVE_SIM_SUPPORTED_COUNT` for updated value.

Constant Value: "android.telephony.action.MULTI_SIM_CONFIG_CHANGED"

### ACTION_NETWORK_COUNTRY_CHANGED

    public static final String ACTION_NETWORK_COUNTRY_CHANGED

Broadcast intent action for network country code changes.

The `EXTRA_NETWORK_COUNTRY` extra indicates the country code of the current network returned by `getNetworkCountryIso()`.

There may be a delay of several minutes before reporting that no country is detected.

See also:

- `EXTRA_NETWORK_COUNTRY`
- `getNetworkCountryIso()`

Constant Value: "android.telephony.action.NETWORK_COUNTRY_CHANGED"

### ACTION_PHONE_STATE_CHANGED

    public static final String ACTION_PHONE_STATE_CHANGED

Broadcast intent action indicating that the call state on the device has changed.

The `EXTRA_STATE` extra indicates the new call state. If a receiving app has `Manifest.permission.READ_CALL_LOG` permission, a second extra `EXTRA_INCOMING_NUMBER` provides the phone number for incoming and outgoing calls as a String.

If the receiving app has `Manifest.permission.READ_CALL_LOG` and `Manifest.permission.READ_PHONE_STATE` permission, it will receive the broadcast twice; one with the `EXTRA_INCOMING_NUMBER` populated with the phone number, and another with it blank. Due to the nature of broadcasts, you cannot assume the order in which these broadcasts will arrive, however you are guaranteed to receive two in this case. Apps which are interested in the `EXTRA_INCOMING_NUMBER` can ignore the broadcasts where `EXTRA_INCOMING_NUMBER` is not present in the extras (e.g. where `Intent#hasExtra(String)` returns `false`).

This was a `sticky` broadcast in version 1.0, but it is no longer sticky. Instead, use `getCallState()` to synchronously query the current call state.
Requires `Manifest.permission.READ_PHONE_STATE`

See also:

- `EXTRA_STATE`
- `EXTRA_INCOMING_NUMBER`
- `getCallState()`

Constant Value: "android.intent.action.PHONE_STATE"

### ACTION_RESPOND_VIA_MESSAGE

    public static final String ACTION_RESPOND_VIA_MESSAGE

The Phone app sends this intent when a user opts to respond-via-message during an incoming call. By default, the device's default SMS app consumes this message and sends a text message to the caller. A third party app can also provide this functionality by consuming this Intent with a `Service` and sending the message using its own messaging system.

The intent contains a URI (available from `Intent.getData()`) describing the recipient, using either the `sms:`, `smsto:`, `mms:`, or `mmsto:` URI schema. Each of these URI schema carry the recipient information the same way: the path part of the URI contains the recipient's phone number or a comma-separated set of phone numbers if there are multiple recipients. For example, `smsto:2065551234`.

The intent may also contain extras for the message text (in `Intent.EXTRA_TEXT`) and a message subject (in `Intent.EXTRA_SUBJECT`).

Note: The intent-filter that consumes this Intent needs to be in a `Service` that requires the permission `Manifest.permission.SEND_RESPOND_VIA_MESSAGE`.

For example, the service that receives this intent can be declared in the manifest file with an intent filter like this:

     <!-- Service that delivers SMS messages received from the phone "quick response" -->
     <service android:name=".HeadlessSmsSendService"
              android:permission="android.permission.SEND_RESPOND_VIA_MESSAGE"
              android:exported="true" >
       <intent-filter>
         <action android:name="android.intent.action.RESPOND_VIA_MESSAGE" />
         <category android:name="android.intent.category.DEFAULT" />
         <data android:scheme="sms" />
         <data android:scheme="smsto" />
         <data android:scheme="mms" />
         <data android:scheme="mmsto" />
       </intent-filter>
     </service>

Output: nothing.

Constant Value: "android.intent.action.RESPOND_VIA_MESSAGE"

### ACTION_SECRET_CODE

    public static final String ACTION_SECRET_CODE

Broadcast Action: A debug code has been entered in the dialer.

This intent is broadcast by the system and OEM telephony apps may need to receive these broadcasts. And it requires the sender to be default dialer or has carrier privileges (see `hasCarrierPrivileges()`).

These "secret codes" are used to activate developer menus by dialing certain codes. And they are of the form `*#*#<code>#*#*`. The intent will have the data URI: `android_secret_code://<code>`. It is possible that a manifest receiver would be woken up even if it is not currently running.

It is supposed to replace `Telephony.Sms.Intents.SECRET_CODE_ACTION` in the next Android version. Before that both of these two actions will be broadcast.

Constant Value: "android.telephony.action.SECRET_CODE"

### ACTION_SHOW_VOICEMAIL_NOTIFICATION

    public static final String ACTION_SHOW_VOICEMAIL_NOTIFICATION

Broadcast intent action for letting the default dialer to know to show voicemail notification.

The `EXTRA_PHONE_ACCOUNT_HANDLE` extra indicates which `PhoneAccountHandle` the voicemail is received on. The `EXTRA_NOTIFICATION_COUNT` extra indicates the total numbers of unheard voicemails. The `EXTRA_VOICEMAIL_NUMBER` extra indicates the voicemail number if available. The `EXTRA_CALL_VOICEMAIL_INTENT` extra is a `PendingIntent` that will call the voicemail number when sent. This extra will be empty if the voicemail number is not set, and `EXTRA_LAUNCH_VOICEMAIL_SETTINGS_INTENT` will be set instead. The `EXTRA_LAUNCH_VOICEMAIL_SETTINGS_INTENT` extra is a `PendingIntent` that will launch the voicemail settings. This extra is only available when the voicemail number is not set. The `EXTRA_IS_REFRESH` extra indicates whether the notification is a refresh or a new notification.

See also:

- `EXTRA_PHONE_ACCOUNT_HANDLE`
- `EXTRA_NOTIFICATION_COUNT`
- `EXTRA_VOICEMAIL_NUMBER`
- `EXTRA_CALL_VOICEMAIL_INTENT`
- `EXTRA_LAUNCH_VOICEMAIL_SETTINGS_INTENT`
- `EXTRA_IS_REFRESH`

Constant Value: "android.telephony.action.SHOW_VOICEMAIL_NOTIFICATION"

### ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED

    public static final String ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED

Broadcast Action: The subscription carrier identity has changed. This intent could be sent on the following events:

- Subscription absent. Carrier identity could change from a valid id to `TelephonyManager#UNKNOWN_CARRIER_ID`.
- Subscription loaded. Carrier identity could change from `TelephonyManager#UNKNOWN_CARRIER_ID` to a valid id.
- The subscription carrier is recognized after a remote update.

The intent will have the following extra values:

- `EXTRA_CARRIER_ID` The up-to-date carrier id of the current subscription id.
- `EXTRA_CARRIER_NAME` The up-to-date carrier name of the current subscription.
- `EXTRA_SUBSCRIPTION_ID` The subscription id associated with the changed carrier identity.

This is a protected intent that can only be sent by the system.

Constant Value: "android.telephony.action.SUBSCRIPTION_CARRIER_IDENTITY_CHANGED"

### ACTION_SUBSCRIPTION_SPECIFIC_CARRIER_IDENTITY_CHANGED

    public static final String ACTION_SUBSCRIPTION_SPECIFIC_CARRIER_IDENTITY_CHANGED

Broadcast Action: The subscription specific carrier identity has changed. A specific carrier ID returns the fine-grained carrier ID of the current subscription. It can represent the fact that a carrier may be in effect an aggregation of other carriers (ie in an MVNO type scenario) where each of these specific carriers which are used to make up the actual carrier service may have different carrier configurations. A specific carrier ID could also be used, for example, in a scenario where a carrier requires different carrier configuration for different service offering such as a prepaid plan. the specific carrier ID would be used for configuration purposes, but apps wishing to know about the carrier itself should use the regular carrier ID returned by `getSimCarrierId()`.

Similar like `ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED`, this intent will be sent on the event of `ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED` while its also possible to be sent without `ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED` when specific carrier ID changes while carrier ID remains the same. e.g, the same subscription switches to different IMSI could potentially change its specific carrier ID while carrier id remains the same.

See also:

- `getSimSpecificCarrierId()`
- `The intent will have the following extra values:
  - {@link #EXTRA_SPECIFIC_CARRIER_ID} The up-to-date specific carrier id of the current subscription.
  - {@link #EXTRA_SPECIFIC_CARRIER_NAME} The up-to-date name of the specific carrier id.
  - {@link #EXTRA_SUBSCRIPTION_ID} The subscription id associated with the changed carrier identity.

  This is a protected intent that can only be sent by the system.

  `

Constant Value: "android.telephony.action.SUBSCRIPTION_SPECIFIC_CARRIER_IDENTITY_CHANGED"

### APPTYPE_CSIM

    public static final int APPTYPE_CSIM

UICC application type is CSIM

Constant Value: 4 (0x00000004)

### APPTYPE_ISIM

    public static final int APPTYPE_ISIM

UICC application type is ISIM

Constant Value: 5 (0x00000005)

### APPTYPE_RUIM

    public static final int APPTYPE_RUIM

UICC application type is RUIM

Constant Value: 3 (0x00000003)

### APPTYPE_SIM

    public static final int APPTYPE_SIM

UICC application type is SIM

Constant Value: 1 (0x00000001)

### APPTYPE_UNKNOWN

    public static final int APPTYPE_UNKNOWN

UICC application type is unknown or not specified

Constant Value: 0 (0x00000000)

### APPTYPE_USIM

    public static final int APPTYPE_USIM

UICC application type is USIM

Constant Value: 2 (0x00000002)

### AUTHTYPE_EAP_AKA

    public static final int AUTHTYPE_EAP_AKA

Authentication type for UICC challenge is EAP AKA. See RFC 4187 for details.

Constant Value: 129 (0x00000081)

### AUTHTYPE_EAP_SIM

    public static final int AUTHTYPE_EAP_SIM

Authentication type for UICC challenge is EAP SIM. See RFC 4186 for details.

Constant Value: 128 (0x00000080)

### CALL_COMPOSER_STATUS_OFF

    public static final int CALL_COMPOSER_STATUS_OFF

Call composer status OFF from user setting.

Constant Value: 0 (0x00000000)

### CALL_COMPOSER_STATUS_ON

    public static final int CALL_COMPOSER_STATUS_ON

Call composer status ON from user setting.

Constant Value: 1 (0x00000001)

### CALL_STATE_IDLE

    public static final int CALL_STATE_IDLE

Device call state: No activity.

Constant Value: 0 (0x00000000)

### CALL_STATE_OFFHOOK

    public static final int CALL_STATE_OFFHOOK

Device call state: Off-hook. At least one call exists that is dialing, active, or on hold, and no calls are ringing or waiting.

Constant Value: 2 (0x00000002)

### CALL_STATE_RINGING

    public static final int CALL_STATE_RINGING

Device call state: Ringing. A new call arrived and is ringing or waiting. In the latter case, another call is already active.

Constant Value: 1 (0x00000001)

### CAPABILITY_SLICING_CONFIG_SUPPORTED

    public static final String CAPABILITY_SLICING_CONFIG_SUPPORTED

Indicates whether `getNetworkSlicingConfiguration(Executor, OutcomeReceiver)` is supported. See comments on respective methods for more information.

Constant Value: "CAPABILITY_SLICING_CONFIG_SUPPORTED"

### CDMA_ROAMING_MODE_AFFILIATED

    public static final int CDMA_ROAMING_MODE_AFFILIATED

Value for `CarrierConfigManager#KEY_CDMA_ROAMING_MODE_INT` which permits roaming on affiliated networks.

Constant Value: 1 (0x00000001)

### CDMA_ROAMING_MODE_ANY

    public static final int CDMA_ROAMING_MODE_ANY

Value for `CarrierConfigManager#KEY_CDMA_ROAMING_MODE_INT` which permits roaming on any network.

Constant Value: 2 (0x00000002)

### CDMA_ROAMING_MODE_HOME

    public static final int CDMA_ROAMING_MODE_HOME

Value for `CarrierConfigManager#KEY_CDMA_ROAMING_MODE_INT` which only permits connections on home networks.

Constant Value: 0 (0x00000000)

### CDMA_ROAMING_MODE_RADIO_DEFAULT

    public static final int CDMA_ROAMING_MODE_RADIO_DEFAULT

Value for `CarrierConfigManager#KEY_CDMA_ROAMING_MODE_INT` which leaves the roaming mode set to the radio default or to the user's preference if they've indicated one.

Constant Value: -1 (0xffffffff)

### DATA_ACTIVITY_DORMANT

    public static final int DATA_ACTIVITY_DORMANT

Data connection is active, but physical link is down

Constant Value: 4 (0x00000004)

### DATA_ACTIVITY_IN

    public static final int DATA_ACTIVITY_IN

Data connection activity: Currently receiving IP PPP traffic.

Constant Value: 1 (0x00000001)

### DATA_ACTIVITY_INOUT

    public static final int DATA_ACTIVITY_INOUT

Data connection activity: Currently both sending and receiving IP PPP traffic.

Constant Value: 3 (0x00000003)

### DATA_ACTIVITY_NONE

    public static final int DATA_ACTIVITY_NONE

Data connection activity: No traffic.

Constant Value: 0 (0x00000000)

### DATA_ACTIVITY_OUT

    public static final int DATA_ACTIVITY_OUT

Data connection activity: Currently sending IP PPP traffic.

Constant Value: 2 (0x00000002)

### DATA_CONNECTED

    public static final int DATA_CONNECTED

Data connection state: Connected. IP traffic should be available.

Constant Value: 2 (0x00000002)

### DATA_CONNECTING

    public static final int DATA_CONNECTING

Data connection state: Currently setting up a data connection.

Constant Value: 1 (0x00000001)

### DATA_DISCONNECTED

    public static final int DATA_DISCONNECTED

Data connection state: Disconnected. IP traffic not available.

Constant Value: 0 (0x00000000)

### DATA_DISCONNECTING

    public static final int DATA_DISCONNECTING

Data connection state: Disconnecting. IP traffic may be available but will cease working imminently.

Constant Value: 4 (0x00000004)

### DATA_ENABLED_REASON_CARRIER

    public static final int DATA_ENABLED_REASON_CARRIER

To indicate enable or disable carrier data by the system based on carrier signalling or carrier privileged apps. Carrier data on/off won't affect user settings but will bypass the settings and turns off data internally if set to `false`.

Constant Value: 2 (0x00000002)

### DATA_ENABLED_REASON_POLICY

    public static final int DATA_ENABLED_REASON_POLICY

To indicate that data control due to policy. Usually used when data limit is passed. Policy data on/off won't affect user settings but will bypass the settings and turns off data internally if set to `false`.

Constant Value: 1 (0x00000001)

### DATA_ENABLED_REASON_THERMAL

    public static final int DATA_ENABLED_REASON_THERMAL

To indicate enable or disable data by thermal service. Thermal data on/off won't affect user settings but will bypass the settings and turns off data internally if set to `false`.

Constant Value: 3 (0x00000003)

### DATA_ENABLED_REASON_USER

    public static final int DATA_ENABLED_REASON_USER

To indicate that user enabled or disabled data.

Constant Value: 0 (0x00000000)

### DATA_SUSPENDED

    public static final int DATA_SUSPENDED

Data connection state: Suspended. The connection is up, but IP traffic is temporarily unavailable. For example, in a 2G network, data activity may be suspended when a voice call arrives.

Constant Value: 3 (0x00000003)

### DATA_UNKNOWN

    public static final int DATA_UNKNOWN

Data connection state: Unknown. Used before we know the state.

Constant Value: -1 (0xffffffff)

### ERI_FLASH

    public static final int ERI_FLASH

ERI (Enhanced Roaming Indicator) is FLASH i.e value 2 defined by 3GPP2 C.R1001-H v1.0 Table 8.1-1.

Constant Value: 2 (0x00000002)

### ERI_OFF

    public static final int ERI_OFF

ERI (Enhanced Roaming Indicator) is OFF i.e value 1 defined by 3GPP2 C.R1001-H v1.0 Table 8.1-1.

Constant Value: 1 (0x00000001)

### ERI_ON

    public static final int ERI_ON

ERI (Enhanced Roaming Indicator) is ON i.e value 0 defined by 3GPP2 C.R1001-H v1.0 Table 8.1-1.

Constant Value: 0 (0x00000000)

### EXTRA_ACTIVE_SIM_SUPPORTED_COUNT

    public static final String EXTRA_ACTIVE_SIM_SUPPORTED_COUNT

The number of active SIM supported by current multi-SIM config. It's not related to how many SIM/subscriptions are currently active. Same value will be returned by `getActiveModemCount()`. For single SIM mode, it's 1. For DSDS or DSDA mode, it's 2. For triple-SIM mode, it's 3. Extra of `ACTION_MULTI_SIM_CONFIG_CHANGED`. type: integer

Constant Value: "android.telephony.extra.ACTIVE_SIM_SUPPORTED_COUNT"

### EXTRA_APN_PROTOCOL

    public static final String EXTRA_APN_PROTOCOL

An integer extra containing the protocol of the apn connection. Sent with the `ACTION_CARRIER_SIGNAL_PCO_VALUE` broadcast. See the `PROTOCOL_*` constants in `ApnSetting` for a list of possible values.

Constant Value: "android.telephony.extra.APN_PROTOCOL"

### EXTRA_APN_TYPE

    public static final String EXTRA_APN_TYPE

An integer extra containing the APN type. Sent with the `ACTION_CARRIER_SIGNAL_REQUEST_NETWORK_FAILED`, `ACTION_CARRIER_SIGNAL_REDIRECTED`, and `ACTION_CARRIER_SIGNAL_PCO_VALUE` broadcasts. See the `TYPE_` constants in `ApnSetting` for a list of possible values.

Constant Value: "android.telephony.extra.APN_TYPE"

### EXTRA_CALL_VOICEMAIL_INTENT

    public static final String EXTRA_CALL_VOICEMAIL_INTENT

The intent to call voicemail.

Constant Value: "android.telephony.extra.CALL_VOICEMAIL_INTENT"

### EXTRA_CARRIER_ID

    public static final String EXTRA_CARRIER_ID

An int extra used with `ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED` which indicates the updated carrier id returned by `TelephonyManager#getSimCarrierId()`.

Will be `TelephonyManager#UNKNOWN_CARRIER_ID` if the subscription is unavailable or the carrier cannot be identified.

Constant Value: "android.telephony.extra.CARRIER_ID"

### EXTRA_CARRIER_NAME

    public static final String EXTRA_CARRIER_NAME

An string extra used with `ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED` which indicates the updated carrier name of the current subscription.

See also:

- `

  Carrier name is a user-facing name of the carrier id {@link #EXTRA_CARRIER_ID}, usually the brand name of the subsidiary (e.g. T-Mobile).

  `

Constant Value: "android.telephony.extra.CARRIER_NAME"

### EXTRA_DATA_FAIL_CAUSE

    public static final String EXTRA_DATA_FAIL_CAUSE

An integer extra containing the data fail cause. Sent with `ACTION_CARRIER_SIGNAL_REQUEST_NETWORK_FAILED`. See `DataFailCause` for a list of possible values.

Constant Value: "android.telephony.extra.DATA_FAIL_CAUSE"

### EXTRA_DEFAULT_NETWORK_AVAILABLE

    public static final String EXTRA_DEFAULT_NETWORK_AVAILABLE

A boolean extra indicating the availability of the default network. Sent with the `ACTION_CARRIER_SIGNAL_DEFAULT_NETWORK_AVAILABLE` broadcast.

Constant Value: "android.telephony.extra.DEFAULT_NETWORK_AVAILABLE"

### EXTRA_HIDE_PUBLIC_SETTINGS

    public static final String EXTRA_HIDE_PUBLIC_SETTINGS

The boolean value indicating whether the voicemail settings activity launched by `ACTION_CONFIGURE_VOICEMAIL` should hide settings accessible through public API. This is used by dialer implementations which provides their own voicemail settings UI, but still needs to expose device specific voicemail settings to the user.

See also:

- `ACTION_CONFIGURE_VOICEMAIL`
- `METADATA_HIDE_VOICEMAIL_SETTINGS_MENU`

Constant Value: "android.telephony.extra.HIDE_PUBLIC_SETTINGS"

### EXTRA_INCOMING_NUMBER

    public static final String EXTRA_INCOMING_NUMBER

This constant is deprecated.
Companion apps for wearable devices should use the `InCallService` API to retrieve the phone number for calls instead. Apps performing call screening should use the `CallScreeningService` API instead.

Extra key used with the `ACTION_PHONE_STATE_CHANGED` broadcast for a String containing the incoming or outgoing phone number.

This extra is only populated for receivers of the `ACTION_PHONE_STATE_CHANGED` broadcast which have been granted the `Manifest.permission.READ_CALL_LOG` and `Manifest.permission.READ_PHONE_STATE` permissions.

For incoming calls, the phone number is only guaranteed to be populated when the `EXTRA_STATE` changes from `EXTRA_STATE_IDLE` to `EXTRA_STATE_RINGING`. If the incoming caller is from an unknown number, the extra will be populated with an empty string. For outgoing calls, the phone number is only guaranteed to be populated when the `EXTRA_STATE` changes from `EXTRA_STATE_IDLE` to `EXTRA_STATE_OFFHOOK`.

Retrieve with `Intent.getStringExtra(String)`.

Constant Value: "incoming_number"

### EXTRA_IS_REFRESH

    public static final String EXTRA_IS_REFRESH

Boolean value representing whether the `ACTION_SHOW_VOICEMAIL_NOTIFICATION` is new or a refresh of an existing notification. Notification refresh happens after reboot or connectivity changes. The user has already been notified for the voicemail so it should not alert the user, and should not be shown again if the user has dismissed it.

Constant Value: "android.telephony.extra.IS_REFRESH"

### EXTRA_LAUNCH_VOICEMAIL_SETTINGS_INTENT

    public static final String EXTRA_LAUNCH_VOICEMAIL_SETTINGS_INTENT

The intent to launch voicemail settings.

Constant Value: "android.telephony.extra.LAUNCH_VOICEMAIL_SETTINGS_INTENT"

### EXTRA_NETWORK_COUNTRY

    public static final String EXTRA_NETWORK_COUNTRY

The extra used with an `ACTION_NETWORK_COUNTRY_CHANGED` to specify the the country code in ISO-3166-1 alpha-2 format.

Retrieve with `Intent.getStringExtra(String)`.

Constant Value: "android.telephony.extra.NETWORK_COUNTRY"

### EXTRA_NOTIFICATION_COUNT

    public static final String EXTRA_NOTIFICATION_COUNT

The number of voice messages associated with the notification.

Constant Value: "android.telephony.extra.NOTIFICATION_COUNT"

### EXTRA_PCO_ID

    public static final String EXTRA_PCO_ID

An integer extra indicating the ID for the PCO data. Sent with the `ACTION_CARRIER_SIGNAL_PCO_VALUE` broadcast.

Constant Value: "android.telephony.extra.PCO_ID"

### EXTRA_PCO_VALUE

    public static final String EXTRA_PCO_VALUE

A byte array extra containing PCO data read from the modem. Sent with the `ACTION_CARRIER_SIGNAL_PCO_VALUE` broadcast.

Constant Value: "android.telephony.extra.PCO_VALUE"

### EXTRA_PHONE_ACCOUNT_HANDLE

    public static final String EXTRA_PHONE_ACCOUNT_HANDLE

The extra used with an `ACTION_CONFIGURE_VOICEMAIL` and `ACTION_SHOW_VOICEMAIL_NOTIFICATION` `Intent` to specify the `PhoneAccountHandle` the configuration or notification is for.

Retrieve with `Intent.getParcelableExtra(String)`.

Constant Value: "android.telephony.extra.PHONE_ACCOUNT_HANDLE"

### EXTRA_REDIRECTION_URL

    public static final String EXTRA_REDIRECTION_URL

String extra containing the redirection URL sent with `ACTION_CARRIER_SIGNAL_REDIRECTED`.

Constant Value: "android.telephony.extra.REDIRECTION_URL"

### EXTRA_SPECIFIC_CARRIER_ID

    public static final String EXTRA_SPECIFIC_CARRIER_ID

An int extra used with `ACTION_SUBSCRIPTION_SPECIFIC_CARRIER_IDENTITY_CHANGED` which indicates the updated specific carrier id returned by `TelephonyManager#getSimSpecificCarrierId()`. Note, its possible specific carrier id changes while `ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED` remains the same e.g, when subscription switch to different IMSIs.

Will be `TelephonyManager#UNKNOWN_CARRIER_ID` if the subscription is unavailable or the carrier cannot be identified.

Constant Value: "android.telephony.extra.SPECIFIC_CARRIER_ID"

### EXTRA_SPECIFIC_CARRIER_NAME

    public static final String EXTRA_SPECIFIC_CARRIER_NAME

An string extra used with `ACTION_SUBSCRIPTION_SPECIFIC_CARRIER_IDENTITY_CHANGED` which indicates the updated specific carrier name returned by `TelephonyManager#getSimSpecificCarrierIdName()`.

it's a user-facing name of the specific carrier id `EXTRA_SPECIFIC_CARRIER_ID` e.g, Tracfone-AT&T

Constant Value: "android.telephony.extra.SPECIFIC_CARRIER_NAME"

### EXTRA_STATE

    public static final String EXTRA_STATE

The lookup key used with the `ACTION_PHONE_STATE_CHANGED` broadcast for a String containing the new call state.

Retrieve with `Intent.getStringExtra(String)`.

See also:

- `EXTRA_STATE_IDLE`
- `EXTRA_STATE_RINGING`
- `EXTRA_STATE_OFFHOOK`

Constant Value: "state"

### EXTRA_SUBSCRIPTION_ID

    public static final String EXTRA_SUBSCRIPTION_ID

An int extra used with `ACTION_SUBSCRIPTION_CARRIER_IDENTITY_CHANGED` to indicate the subscription which has changed; or in general whenever a subscription ID needs specified.

Constant Value: "android.telephony.extra.SUBSCRIPTION_ID"

### EXTRA_VOICEMAIL_NUMBER

    public static final String EXTRA_VOICEMAIL_NUMBER

The voicemail number.

Constant Value: "android.telephony.extra.VOICEMAIL_NUMBER"

### METADATA_HIDE_VOICEMAIL_SETTINGS_MENU

    public static final String METADATA_HIDE_VOICEMAIL_SETTINGS_MENU

A boolean meta-data value indicating whether the voicemail settings should be hidden in the call settings page launched by `TelecomManager.ACTION_SHOW_CALL_SETTINGS`. Dialer implementations (see `TelecomManager.getDefaultDialerPackage()`) which would also like to manage voicemail settings should set this meta-data to `true` in the manifest registration of their application.

See also:

- `TelecomManager.ACTION_SHOW_CALL_SETTINGS`
- `ACTION_CONFIGURE_VOICEMAIL`
- `EXTRA_HIDE_PUBLIC_SETTINGS`

Constant Value: "android.telephony.HIDE_VOICEMAIL_SETTINGS_MENU"

### MULTISIM_ALLOWED

    public static final int MULTISIM_ALLOWED

The usage of multiple SIM cards at the same time to register on the network (e.g. Dual Standby or Dual Active) is supported.

Constant Value: 0 (0x00000000)

### MULTISIM_NOT_SUPPORTED_BY_CARRIER

    public static final int MULTISIM_NOT_SUPPORTED_BY_CARRIER

The usage of multiple SIM cards at the same time to register on the network (e.g. Dual Standby or Dual Active) is supported by the hardware, but restricted by the carrier.

Constant Value: 2 (0x00000002)

### MULTISIM_NOT_SUPPORTED_BY_HARDWARE

    public static final int MULTISIM_NOT_SUPPORTED_BY_HARDWARE

The usage of multiple SIM cards at the same time to register on the network (e.g. Dual Standby or Dual Active) is not supported by the hardware.

Constant Value: 1 (0x00000001)

### NETWORK_SELECTION_MODE_AUTO

    public static final int NETWORK_SELECTION_MODE_AUTO

Constant Value: 1 (0x00000001)

### NETWORK_SELECTION_MODE_MANUAL

    public static final int NETWORK_SELECTION_MODE_MANUAL

Constant Value: 2 (0x00000002)

### NETWORK_SELECTION_MODE_UNKNOWN

    public static final int NETWORK_SELECTION_MODE_UNKNOWN

Constant Value: 0 (0x00000000)

### NETWORK_TYPE_1xRTT

    public static final int NETWORK_TYPE_1xRTT

Current network is 1xRTT

Constant Value: 7 (0x00000007)

### NETWORK_TYPE_CDMA

    public static final int NETWORK_TYPE_CDMA

Current network is CDMA: Either IS95A or IS95B

Constant Value: 4 (0x00000004)

### NETWORK_TYPE_EDGE

    public static final int NETWORK_TYPE_EDGE

Current network is EDGE

Constant Value: 2 (0x00000002)

### NETWORK_TYPE_EHRPD

    public static final int NETWORK_TYPE_EHRPD

Current network is eHRPD

Constant Value: 14 (0x0000000e)

### NETWORK_TYPE_EVDO_0

    public static final int NETWORK_TYPE_EVDO_0

Current network is EVDO revision 0

Constant Value: 5 (0x00000005)

### NETWORK_TYPE_EVDO_A

    public static final int NETWORK_TYPE_EVDO_A

Current network is EVDO revision A

Constant Value: 6 (0x00000006)

### NETWORK_TYPE_EVDO_B

    public static final int NETWORK_TYPE_EVDO_B

Current network is EVDO revision B

Constant Value: 12 (0x0000000c)

### NETWORK_TYPE_GPRS

    public static final int NETWORK_TYPE_GPRS

Current network is GPRS

Constant Value: 1 (0x00000001)

### NETWORK_TYPE_GSM

    public static final int NETWORK_TYPE_GSM

Current network is GSM

Constant Value: 16 (0x00000010)

### NETWORK_TYPE_HSDPA

    public static final int NETWORK_TYPE_HSDPA

Current network is HSDPA

Constant Value: 8 (0x00000008)

### NETWORK_TYPE_HSPA

    public static final int NETWORK_TYPE_HSPA

Current network is HSPA

Constant Value: 10 (0x0000000a)

### NETWORK_TYPE_HSPAP

    public static final int NETWORK_TYPE_HSPAP

Current network is HSPA+

Constant Value: 15 (0x0000000f)

### NETWORK_TYPE_HSUPA

    public static final int NETWORK_TYPE_HSUPA

Current network is HSUPA

Constant Value: 9 (0x00000009)

### NETWORK_TYPE_IDEN

    public static final int NETWORK_TYPE_IDEN

Current network is iDen

Constant Value: 11 (0x0000000b)

### NETWORK_TYPE_IWLAN

    public static final int NETWORK_TYPE_IWLAN

Current network is IWLAN

Constant Value: 18 (0x00000012)

### NETWORK_TYPE_LTE

    public static final int NETWORK_TYPE_LTE

Current network is LTE

Constant Value: 13 (0x0000000d)

### NETWORK_TYPE_NR

    public static final int NETWORK_TYPE_NR

Current network is NR (New Radio) 5G. This will only be returned for 5G SA. For 5G NSA, the network type will be `NETWORK_TYPE_LTE`.

Constant Value: 20 (0x00000014)

### NETWORK_TYPE_TD_SCDMA

    public static final int NETWORK_TYPE_TD_SCDMA

Current network is TD_SCDMA

Constant Value: 17 (0x00000011)

### NETWORK_TYPE_UMTS

    public static final int NETWORK_TYPE_UMTS

Current network is UMTS

Constant Value: 3 (0x00000003)

### NETWORK_TYPE_UNKNOWN

    public static final int NETWORK_TYPE_UNKNOWN

Network type is unknown

Constant Value: 0 (0x00000000)

### PHONE_TYPE_CDMA

    public static final int PHONE_TYPE_CDMA

Phone radio is CDMA.

Constant Value: 2 (0x00000002)

### PHONE_TYPE_GSM

    public static final int PHONE_TYPE_GSM

Phone radio is GSM.

Constant Value: 1 (0x00000001)

### PHONE_TYPE_NONE

    public static final int PHONE_TYPE_NONE

No phone radio.

Constant Value: 0 (0x00000000)

### PHONE_TYPE_SIP

    public static final int PHONE_TYPE_SIP

Phone is via SIP.

Constant Value: 3 (0x00000003)

### SET_OPPORTUNISTIC_SUB_INACTIVE_SUBSCRIPTION

    public static final int SET_OPPORTUNISTIC_SUB_INACTIVE_SUBSCRIPTION

The subscription is not valid. It must be an active opportunistic subscription.

Constant Value: 2 (0x00000002)

### SET_OPPORTUNISTIC_SUB_NO_OPPORTUNISTIC_SUB_AVAILABLE

    public static final int SET_OPPORTUNISTIC_SUB_NO_OPPORTUNISTIC_SUB_AVAILABLE

The subscription is not valid. It must be an opportunistic subscription.

Constant Value: 3 (0x00000003)

### SET_OPPORTUNISTIC_SUB_REMOTE_SERVICE_EXCEPTION

    public static final int SET_OPPORTUNISTIC_SUB_REMOTE_SERVICE_EXCEPTION

Subscription service happened remote exception.

Constant Value: 4 (0x00000004)

### SET_OPPORTUNISTIC_SUB_SUCCESS

    public static final int SET_OPPORTUNISTIC_SUB_SUCCESS

No error. Operation succeeded.

Constant Value: 0 (0x00000000)

### SET_OPPORTUNISTIC_SUB_VALIDATION_FAILED

    public static final int SET_OPPORTUNISTIC_SUB_VALIDATION_FAILED

Validation failed when trying to switch to preferred subscription.

Constant Value: 1 (0x00000001)

### SIM_STATE_ABSENT

    public static final int SIM_STATE_ABSENT

SIM card state: no SIM card is available in the device

Constant Value: 1 (0x00000001)

### SIM_STATE_CARD_IO_ERROR

    public static final int SIM_STATE_CARD_IO_ERROR

SIM card state: SIM Card Error, present but faulty

Constant Value: 8 (0x00000008)

### SIM_STATE_CARD_RESTRICTED

    public static final int SIM_STATE_CARD_RESTRICTED

SIM card state: SIM Card restricted, present but not usable due to carrier restrictions.

Constant Value: 9 (0x00000009)

### SIM_STATE_NETWORK_LOCKED

    public static final int SIM_STATE_NETWORK_LOCKED

SIM card state: Locked: requires a network PIN to unlock

Constant Value: 4 (0x00000004)

### SIM_STATE_NOT_READY

    public static final int SIM_STATE_NOT_READY

SIM card state: SIM Card is NOT READY

Constant Value: 6 (0x00000006)

### SIM_STATE_PERM_DISABLED

    public static final int SIM_STATE_PERM_DISABLED

SIM card state: SIM Card Error, permanently disabled

Constant Value: 7 (0x00000007)

### SIM_STATE_PIN_REQUIRED

    public static final int SIM_STATE_PIN_REQUIRED

SIM card state: Locked: requires the user's SIM PIN to unlock

Constant Value: 2 (0x00000002)

### SIM_STATE_PUK_REQUIRED

    public static final int SIM_STATE_PUK_REQUIRED

SIM card state: Locked: requires the user's SIM PUK to unlock

Constant Value: 3 (0x00000003)

### SIM_STATE_READY

    public static final int SIM_STATE_READY

SIM card state: Ready

Constant Value: 5 (0x00000005)

### SIM_STATE_UNKNOWN

    public static final int SIM_STATE_UNKNOWN

SIM card state: Unknown. Signifies that the SIM is in transition between states. For example, when the user inputs the SIM pin under PIN_REQUIRED state, a query for sim status returns this state before turning to SIM_STATE_READY. These are the ordinal value of IccCardConstants.State.

Constant Value: 0 (0x00000000)

### UNINITIALIZED_CARD_ID

    public static final int UNINITIALIZED_CARD_ID

A UICC card identifier used before the UICC card is loaded. See `getCardIdForDefaultEuicc()` and `UiccCardInfo#getCardId()`.

Note that once the UICC card is loaded, the card ID may become `UNSUPPORTED_CARD_ID`.

Constant Value: -2 (0xfffffffe)

### UNKNOWN_CARRIER_ID

    public static final int UNKNOWN_CARRIER_ID

An unknown carrier id. It could either be subscription unavailable or the subscription carrier cannot be recognized. Unrecognized carriers here means `MCC+MNC` cannot be identified.

Constant Value: -1 (0xffffffff)

### UNSUPPORTED_CARD_ID

    public static final int UNSUPPORTED_CARD_ID

A UICC card identifier used if the device does not support the operation. For example, `getCardIdForDefaultEuicc()` returns this value if the device has no eUICC, or the eUICC cannot be read.

Constant Value: -1 (0xffffffff)

### UPDATE_AVAILABLE_NETWORKS_ABORTED

    public static final int UPDATE_AVAILABLE_NETWORKS_ABORTED

The request is aborted.

Constant Value: 2 (0x00000002)

### UPDATE_AVAILABLE_NETWORKS_DISABLE_MODEM_FAIL

    public static final int UPDATE_AVAILABLE_NETWORKS_DISABLE_MODEM_FAIL

Disable modem fail.

Constant Value: 5 (0x00000005)

### UPDATE_AVAILABLE_NETWORKS_ENABLE_MODEM_FAIL

    public static final int UPDATE_AVAILABLE_NETWORKS_ENABLE_MODEM_FAIL

Enable modem fail.

Constant Value: 6 (0x00000006)

### UPDATE_AVAILABLE_NETWORKS_INVALID_ARGUMENTS

    public static final int UPDATE_AVAILABLE_NETWORKS_INVALID_ARGUMENTS

The parameter passed in is invalid.

Constant Value: 3 (0x00000003)

### UPDATE_AVAILABLE_NETWORKS_MULTIPLE_NETWORKS_NOT_SUPPORTED

    public static final int UPDATE_AVAILABLE_NETWORKS_MULTIPLE_NETWORKS_NOT_SUPPORTED

Carrier app does not support multiple available networks.

Constant Value: 7 (0x00000007)

### UPDATE_AVAILABLE_NETWORKS_NO_CARRIER_PRIVILEGE

    public static final int UPDATE_AVAILABLE_NETWORKS_NO_CARRIER_PRIVILEGE

No carrier privilege.

Constant Value: 4 (0x00000004)

### UPDATE_AVAILABLE_NETWORKS_NO_OPPORTUNISTIC_SUB_AVAILABLE

    public static final int UPDATE_AVAILABLE_NETWORKS_NO_OPPORTUNISTIC_SUB_AVAILABLE

The subscription is not valid. It must be an opportunistic subscription.

Constant Value: 8 (0x00000008)

### UPDATE_AVAILABLE_NETWORKS_REMOTE_SERVICE_EXCEPTION

    public static final int UPDATE_AVAILABLE_NETWORKS_REMOTE_SERVICE_EXCEPTION

There is no OpportunisticNetworkService.

Constant Value: 9 (0x00000009)

### UPDATE_AVAILABLE_NETWORKS_SERVICE_IS_DISABLED

    public static final int UPDATE_AVAILABLE_NETWORKS_SERVICE_IS_DISABLED

OpportunisticNetworkService is disabled.

Constant Value: 10 (0x0000000a)

### UPDATE_AVAILABLE_NETWORKS_SUCCESS

    public static final int UPDATE_AVAILABLE_NETWORKS_SUCCESS

No error. Operation succeeded.

Constant Value: 0 (0x00000000)

### UPDATE_AVAILABLE_NETWORKS_UNKNOWN_FAILURE

    public static final int UPDATE_AVAILABLE_NETWORKS_UNKNOWN_FAILURE

There is a unknown failure happened.

Constant Value: 1 (0x00000001)

### USSD_ERROR_SERVICE_UNAVAIL

    public static final int USSD_ERROR_SERVICE_UNAVAIL

Failure code returned when a USSD request has failed to execute because the Telephony service is unavailable.

Returned via `TelephonyManager.UssdResponseCallback#onReceiveUssdResponseFailed( TelephonyManager, String, int)`.

Constant Value: -2 (0xfffffffe)

### USSD_RETURN_FAILURE

    public static final int USSD_RETURN_FAILURE

Failed code returned when the mobile network has failed to complete a USSD request.

Returned via `TelephonyManager.UssdResponseCallback#onReceiveUssdResponseFailed( TelephonyManager, String, int)`.

Constant Value: -1 (0xffffffff)

### VVM_TYPE_CVVM

    public static final String VVM_TYPE_CVVM

A flavor of OMTP protocol with a different mobile originated (MO) format

Constant Value: "vvm_type_cvvm"

### VVM_TYPE_OMTP

    public static final String VVM_TYPE_OMTP

The OMTP protocol.

Constant Value: "vvm_type_omtp"

## Fields

### EXTRA_STATE_IDLE

    public static final String EXTRA_STATE_IDLE

Value used with `EXTRA_STATE` corresponding to `CALL_STATE_IDLE`.

### EXTRA_STATE_OFFHOOK

    public static final String EXTRA_STATE_OFFHOOK

Value used with `EXTRA_STATE` corresponding to `CALL_STATE_OFFHOOK`.

### EXTRA_STATE_RINGING

    public static final String EXTRA_STATE_RINGING

Value used with `EXTRA_STATE` corresponding to `CALL_STATE_RINGING`.

## Public methods

### canChangeDtmfToneLength

    public boolean canChangeDtmfToneLength ()

Whether the device supports configuring the DTMF tone length.

Returns
`boolean` | `true` if the DTMF tone length can be changed, and `false` otherwise.

### clearSignalStrengthUpdateRequest

    public void clearSignalStrengthUpdateRequest (SignalStrengthUpdateRequest request)

Clear a `SignalStrengthUpdateRequest` from the system.

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `TelephonyManager#hasCarrierPrivileges`).

If the given request was not set before, this operation is a no-op.
Requires `Manifest.permission.MODIFY_PHONE_STATE`

Parameters
`request` | `SignalStrengthUpdateRequest`: the SignalStrengthUpdateRequest to be cleared from the System This value cannot be `null`.

See also:

- `setSignalStrengthUpdateRequest(SignalStrengthUpdateRequest)`

### createForPhoneAccountHandle

    public TelephonyManager createForPhoneAccountHandle (PhoneAccountHandle phoneAccountHandle)

Create a new TelephonyManager object pinned to the subscription ID associated with the given phone account.

Parameters
`phoneAccountHandle` | `PhoneAccountHandle`

Returns
`TelephonyManager` | a TelephonyManager that uses the given phone account for all calls, or `null` if the phone account does not correspond to a valid subscription ID.

### createForSubscriptionId

    public TelephonyManager createForSubscriptionId (int subId)

Create a new TelephonyManager object pinned to the given subscription ID.

Parameters
`subId` | `int`

Returns
`TelephonyManager` | a TelephonyManager that uses the given subId for all calls.

### doesSwitchMultiSimConfigTriggerReboot

    public boolean doesSwitchMultiSimConfigTriggerReboot ()

Get whether making changes to modem configurations by `switchMultiSimConfig(int)` will trigger device reboot. The modem configuration change refers to switching from single SIM configuration to DSDS or the other way around.

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`boolean` | `true` if reboot will be triggered after making changes to modem configurations, otherwise return `false`.

### getActiveModemCount

    public int getActiveModemCount ()

Returns the number of logical modems currently configured to be activated. Returns 0 if none of voice, sms, data is not supported Returns 1 for Single standby mode (Single SIM functionality). Returns 2 for Dual standby mode (Dual SIM functionality). Returns 3 for Tri standby mode (Tri SIM functionality).

Returns
`int` |

### getAllCellInfo

    public List<CellInfo> getAllCellInfo ()

Requests all available cell information from all radios on the device including the camped/registered, serving, and neighboring cells.

The response can include one or more `CellInfoGsm`, `CellInfoCdma`, `CellInfoTdscdma`, `CellInfoLte`, and `CellInfoWcdma` objects, in any combination. It is typical to see instances of one or more of any these in the list. In addition, zero or more of the returned objects may be considered registered; that is, their `CellInfo.isRegistered()` methods may return true, indicating that the cell is being used or would be used for signaling communication if necessary.

Beginning with `Android Q`, if this API results in a change of the cached CellInfo, that change will be reported via `onCellInfoChanged()`.

Apps targeting `Android Q` or higher will no longer trigger a refresh of the cached CellInfo by invoking this API. Instead, those apps will receive the latest cached results, which may not be current. Apps targeting `Android Q` or higher that wish to request updated CellInfo should call `requestCellInfoUpdate()`; however, in all cases, updates will be rate-limited and are not guaranteed. To determine the recency of CellInfo data, callers should check `CellInfo#getTimeStamp()`.

This method returns valid data for devices with `FEATURE_TELEPHONY`. In cases where only partial information is available for a particular CellInfo entry, unavailable fields will be reported as `CellInfo.UNAVAILABLE`. All reported cells will include at least a valid set of technology-specific identification info and a power level measurement.

This method is preferred over using `getCellLocation()`.
Requires `Manifest.permission.ACCESS_FINE_LOCATION`

Returns
`List<CellInfo>` | List of `CellInfo`; null if cell information is unavailable.

### getCallComposerStatus

    public int getCallComposerStatus ()

Get the user-set status for enriched calling with call composer.

If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()`
Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Returns
`int` | the user-set status for enriched calling with call composer, either of `CALL_COMPOSER_STATUS_ON` or `CALL_COMPOSER_STATUS_OFF`. Value is `CALL_COMPOSER_STATUS_ON`, or `CALL_COMPOSER_STATUS_OFF`

Throws
`SecurityException` | if the caller does not have the permission.

### getCallState

    public int getCallState ()

This method is deprecated.
Use `getCallStateForSubscription()` to retrieve the call state for a specific telephony subscription (which allows carrier privileged apps), `TelephonyCallback.CallStateListener` for real-time call state updates, or `TelecomManager#isInCall()`, which supplies an aggregate "in call" state for the entire device.

Returns the state of all calls on the device.

This method considers not only calls in the Telephony stack, but also calls via other `ConnectionService` implementations.

Note: The call state returned via this method may differ from what is reported by `PhoneStateListener#onCallStateChanged(int, String)`, as that callback only considers Telephony (mobile) calls.

Requires Permission: `READ_PHONE_STATE` for applications targeting API level 31+.

Returns
`int` | the current call state. Value is `CALL_STATE_IDLE`, `CALL_STATE_RINGING`, or `CALL_STATE_OFFHOOK`

### getCallStateForSubscription

    public int getCallStateForSubscription ()

Retrieve the call state for a specific subscription that was specified when this TelephonyManager instance was created.

Requires Permission: `READ_PHONE_STATE` or that the calling application has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`int` | The call state of the subscription associated with this TelephonyManager instance. Value is `CALL_STATE_IDLE`, `CALL_STATE_RINGING`, or `CALL_STATE_OFFHOOK`

See also:

- `createForSubscriptionId(int)`
- `createForPhoneAccountHandle(PhoneAccountHandle)`

### getCardIdForDefaultEuicc

    public int getCardIdForDefaultEuicc ()

Get the card ID of the default eUICC card. If the eUICCs have not yet been loaded, returns `UNINITIALIZED_CARD_ID`. If there is no eUICC or the device does not support card IDs for eUICCs, returns `UNSUPPORTED_CARD_ID`.

The card ID is a unique identifier associated with a UICC or eUICC card. Card IDs are unique to a device, and always refer to the same UICC or eUICC card unless the device goes through a factory reset.

Returns
`int` | card ID of the default eUICC card, if loaded.

### getCarrierConfig

    public PersistableBundle getCarrierConfig ()

Returns the carrier config of the subscription ID pinned to the TelephonyManager. If an invalid subscription ID is pinned to the TelephonyManager, the returned config will contain default values.

This method may take several seconds to complete, so it should only be called from a worker thread.

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
This method may take several seconds to complete, so it should only be called from a worker thread.
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`PersistableBundle` |

See also:

- `CarrierConfigManager.getConfigForSubId(int)`
- `createForSubscriptionId(int)`
- `createForPhoneAccountHandle(PhoneAccountHandle)`

### getCarrierIdFromSimMccMnc

    public int getCarrierIdFromSimMccMnc ()

Returns carrier id based on sim MCCMNC (returned by `getSimOperator()`) only. This is used for fallback when configurations/logic for exact carrier id `getSimCarrierId()` are not found. Android carrier id table here can be updated out-of-band, its possible a MVNO (Mobile Virtual Network Operator) carrier was not fully recognized and assigned to its MNO (Mobile Network Operator) carrier id by default. After carrier id table update, a new carrier id was assigned. If apps don't take the update with the new id, it might be helpful to always fallback by using carrier id based on MCCMNC if there is no match.

Returns
`int` | matching carrier id from sim MCCMNC. Return `UNKNOWN_CARRIER_ID` if the subscription is unavailable or the carrier cannot be identified.

### getCellLocation

    public CellLocation getCellLocation ()

This method is deprecated.
use `getAllCellInfo()` instead, which returns a superset of this API.

Returns the current location of the device.

If there is only one radio in the device and that radio has an LTE connection, this method will return null. The implementation must not to try add LTE identifiers into the existing cdma/gsm classes.

Requires `Manifest.permission.ACCESS_FINE_LOCATION`

Returns
`CellLocation` | Current location of the device or null if not available.

### getDataActivity

    public int getDataActivity ()

Returns a constant indicating the type of activity on a data connection (cellular).

Returns
`int` |

See also:

- `DATA_ACTIVITY_NONE`
- `DATA_ACTIVITY_IN`
- `DATA_ACTIVITY_OUT`
- `DATA_ACTIVITY_INOUT`
- `DATA_ACTIVITY_DORMANT`

### getDataNetworkType

    public int getDataNetworkType ()

Returns a constant indicating the radio technology (network type) currently in use on the device for data transmission. If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultDataSubscriptionId()`

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`int` | the network type Value is `NETWORK_TYPE_UNKNOWN`, `NETWORK_TYPE_GPRS`, `NETWORK_TYPE_EDGE`, `NETWORK_TYPE_UMTS`, `NETWORK_TYPE_CDMA`, `NETWORK_TYPE_EVDO_0`, `NETWORK_TYPE_EVDO_A`, `NETWORK_TYPE_1xRTT`, `NETWORK_TYPE_HSDPA`, `NETWORK_TYPE_HSUPA`, `NETWORK_TYPE_HSPA`, `NETWORK_TYPE_IDEN`, `NETWORK_TYPE_EVDO_B`, `NETWORK_TYPE_LTE`, `NETWORK_TYPE_EHRPD`, `NETWORK_TYPE_HSPAP`, `NETWORK_TYPE_GSM`, `NETWORK_TYPE_TD_SCDMA`, `NETWORK_TYPE_IWLAN`, or `NETWORK_TYPE_NR`

See also:

- `NETWORK_TYPE_UNKNOWN`
- `NETWORK_TYPE_GPRS`
- `NETWORK_TYPE_EDGE`
- `NETWORK_TYPE_UMTS`
- `NETWORK_TYPE_HSDPA`
- `NETWORK_TYPE_HSUPA`
- `NETWORK_TYPE_HSPA`
- `NETWORK_TYPE_CDMA`
- `NETWORK_TYPE_EVDO_0`
- `NETWORK_TYPE_EVDO_A`
- `NETWORK_TYPE_EVDO_B`
- `NETWORK_TYPE_1xRTT`
- `NETWORK_TYPE_IDEN`
- `NETWORK_TYPE_LTE`
- `NETWORK_TYPE_EHRPD`
- `NETWORK_TYPE_HSPAP`
- `NETWORK_TYPE_NR`

### getDataState

    public int getDataState ()

Returns a constant indicating the current data connection state (cellular).

Returns
`int` |

See also:

- `DATA_DISCONNECTED`
- `DATA_CONNECTING`
- `DATA_CONNECTED`
- `DATA_SUSPENDED`
- `DATA_DISCONNECTING`

### getDeviceId

    public String getDeviceId ()

This method is deprecated.
Use `getImei()` which returns IMEI for GSM or `getMeid()` which returns MEID for CDMA.

Returns the unique device ID, for example, the IMEI for GSM and the MEID or ESN for CDMA phones. Return null if device ID is not available.

Starting with API level 29, persistent device identifiers are guarded behind additional restrictions, and apps are recommended to use resettable identifiers (see Best practices for unique identifiers). This method can be invoked if one of the following requirements is met:

- If the calling app has been granted the READ_PRIVILEGED_PHONE_STATE permission; this is a privileged permission that can only be granted to apps preloaded on the device.
- If the calling app is the device owner of a fully-managed device, a profile owner of an organization-owned device, or their delegates (see `DevicePolicyManager.getEnrollmentSpecificId()`).
- If the calling app has carrier privileges (see `hasCarrierPrivileges()`) on any active subscription.
- If the calling app is the default SMS role holder (see `RoleManager.isRoleHeld(java.lang.String)`).

If the calling app does not meet one of these requirements then this method will behave as follows:

- If the calling app's target SDK is API level 28 or lower and the app has the READ_PHONE_STATE permission then null is returned.
- If the calling app's target SDK is API level 28 or lower and the app does not have the READ_PHONE_STATE permission, or if the calling app is targeting API level 29 or higher, then a SecurityException is thrown.

Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Returns
`String` |

### getDeviceId

    public String getDeviceId (int slotIndex)

This method is deprecated.
Use `getImei()` which returns IMEI for GSM or `getMeid()` which returns MEID for CDMA.

Returns the unique device ID of a subscription, for example, the IMEI for GSM and the MEID for CDMA phones. Return null if device ID is not available.

Starting with API level 29, persistent device identifiers are guarded behind additional restrictions, and apps are recommended to use resettable identifiers (see Best practices for unique identifiers). This method can be invoked if one of the following requirements is met:

- If the calling app has been granted the READ_PRIVILEGED_PHONE_STATE permission; this is a privileged permission that can only be granted to apps preloaded on the device.
- If the calling app is the device owner of a fully-managed device, a profile owner of an organization-owned device, or their delegates (see `DevicePolicyManager.getEnrollmentSpecificId()`).
- If the calling app has carrier privileges (see `hasCarrierPrivileges()`) on any active subscription.
- If the calling app is the default SMS role holder (see `RoleManager.isRoleHeld(java.lang.String)`).

If the calling app does not meet one of these requirements then this method will behave as follows:

- If the calling app's target SDK is API level 28 or lower and the app has the READ_PHONE_STATE permission then null is returned.
- If the calling app's target SDK is API level 28 or lower and the app does not have the READ_PHONE_STATE permission, or if the calling app is targeting API level 29 or higher, then a SecurityException is thrown.

Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Parameters
`slotIndex` | `int`: of which deviceID is returned

Returns
`String` |

### getDeviceSoftwareVersion

    public String getDeviceSoftwareVersion ()

Returns the software version number for the device, for example, the IMEI/SV for GSM phones. Return null if the software version is not available.

Requires Permission: `READ_PHONE_STATE`.
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`String` |

### getEmergencyNumberList

    public Map<Integer, List<EmergencyNumber>> getEmergencyNumberList ()

Get the emergency number list based on current locale, sim, default, modem and network.

In each returned list, the emergency number `EmergencyNumber` coming from higher priority sources will be located at the smaller index; the priority order of sources are: `EmergencyNumber#EMERGENCY_NUMBER_SOURCE_NETWORK_SIGNALING` > `EmergencyNumber#EMERGENCY_NUMBER_SOURCE_SIM` > `EmergencyNumber#EMERGENCY_NUMBER_SOURCE_DATABASE` > `EmergencyNumber#EMERGENCY_NUMBER_SOURCE_DEFAULT` > `EmergencyNumber#EMERGENCY_NUMBER_SOURCE_MODEM_CONFIG`

The subscriptions which the returned list would be based on, are all the active subscriptions, no matter which subscription could be used to create TelephonyManager.

Requires permission `Manifest.permission.READ_PHONE_STATE` or the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`Map<Integer, List<EmergencyNumber>>` | Map including the keys as the active subscription IDs (Note: if there is no active subscription, the key is `SubscriptionManager#getDefaultSubscriptionId`) and the value as the list of `EmergencyNumber`; empty Map if this information is not available; or throw a SecurityException if the caller does not have the permission. This value cannot be `null`.

### getEmergencyNumberList

    public Map<Integer, List<EmergencyNumber>> getEmergencyNumberList (int categories)

Get the per-category emergency number list based on current locale, sim, default, modem and network.

In each returned list, the emergency number `EmergencyNumber` coming from higher priority sources will be located at the smaller index; the priority order of sources are: `EmergencyNumber#EMERGENCY_NUMBER_SOURCE_NETWORK_SIGNALING` > `EmergencyNumber#EMERGENCY_NUMBER_SOURCE_SIM` > `EmergencyNumber#EMERGENCY_NUMBER_SOURCE_DATABASE` > `EmergencyNumber#EMERGENCY_NUMBER_SOURCE_DEFAULT` > `EmergencyNumber#EMERGENCY_NUMBER_SOURCE_MODEM_CONFIG`

The subscriptions which the returned list would be based on, are all the active subscriptions, no matter which subscription could be used to create TelephonyManager.

Requires permission `Manifest.permission.READ_PHONE_STATE` or the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Parameters
`categories` | `int`: the emergency service categories which are the bitwise-OR combination of the following constants: `EmergencyNumber#EMERGENCY_SERVICE_CATEGORY_UNSPECIFIED` `EmergencyNumber#EMERGENCY_SERVICE_CATEGORY_POLICE` `EmergencyNumber#EMERGENCY_SERVICE_CATEGORY_AMBULANCE` `EmergencyNumber#EMERGENCY_SERVICE_CATEGORY_FIRE_BRIGADE` `EmergencyNumber#EMERGENCY_SERVICE_CATEGORY_MARINE_GUARD` `EmergencyNumber#EMERGENCY_SERVICE_CATEGORY_MOUNTAIN_RESCUE` `EmergencyNumber#EMERGENCY_SERVICE_CATEGORY_MIEC` `EmergencyNumber#EMERGENCY_SERVICE_CATEGORY_AIEC` Value is either `0` or a combination of `EmergencyNumber.EMERGENCY_SERVICE_CATEGORY_UNSPECIFIED`, `EmergencyNumber.EMERGENCY_SERVICE_CATEGORY_POLICE`, `EmergencyNumber.EMERGENCY_SERVICE_CATEGORY_AMBULANCE`, `EmergencyNumber.EMERGENCY_SERVICE_CATEGORY_FIRE_BRIGADE`, `EmergencyNumber.EMERGENCY_SERVICE_CATEGORY_MARINE_GUARD`, `EmergencyNumber.EMERGENCY_SERVICE_CATEGORY_MOUNTAIN_RESCUE`, `EmergencyNumber.EMERGENCY_SERVICE_CATEGORY_MIEC`, and `EmergencyNumber.EMERGENCY_SERVICE_CATEGORY_AIEC`

Returns
`Map<Integer, List<EmergencyNumber>>` | Map including the keys as the active subscription IDs (Note: if there is no active subscription, the key is `SubscriptionManager#getDefaultSubscriptionId`) and the value as the list of `EmergencyNumber`; empty Map if this information is not available; or throw a SecurityException if the caller does not have the permission. This value cannot be `null`.

Throws
`IllegalStateException` | if the Telephony process is not currently available.

### getEquivalentHomePlmns

    public List<String> getEquivalentHomePlmns ()

Returns a list of the equivalent home PLMNs (EF_EHPLMN) from the USIM app.

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`List<String>` | A list of equivalent home PLMNs. Returns an empty list if EF_EHPLMN is empty or does not exist on the SIM card. This value cannot be `null`.

Throws
`IllegalStateException` | if the Telephony process is not currently available.
`SecurityException` | if the caller doesn't have the permission.

### getForbiddenPlmns

    public String[] getForbiddenPlmns ()

Returns an array of Forbidden PLMNs from the USIM App Returns null if the query fails.

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`String[]` | an array of forbidden PLMNs or null if not available

### getGroupIdLevel1

    public String getGroupIdLevel1 ()

Returns the Group Identifier Level1 for a GSM phone. Return null if it is unavailable.

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`String` |

### getIccAuthentication

    public String getIccAuthentication (int appType,
                    int authType,
                    String data)

Returns the response of authentication for the default subscription. Returns null if the authentication hasn't been successful

Requires one of the following permissions:

- READ_PRIVILEGED_PHONE_STATE
- the calling app has carrier privileges (see `hasCarrierPrivileges()`).
- the calling app has been granted the `Manifest.permission#USE_ICC_AUTH_WITH_DEVICE_IDENTIFIER` permission.

Parameters
`appType` | `int`: the icc application type, like `APPTYPE_USIM`
`authType` | `int`: the authentication type, `AUTHTYPE_EAP_AKA` or `AUTHTYPE_EAP_SIM`
`data` | `String`: authentication challenge data, base64 encoded. See 3GPP TS 31.102 7.1.2 for more details.

Returns
`String` | the response of authentication. This value will be null in the following cases: Authentication error, incorrect MAC Authentication error, security context not supported Key freshness failure Authentication error, no memory space available Authentication error, no memory space available in EFMUK

### getImei

    public String getImei (int slotIndex)

Returns the IMEI (International Mobile Equipment Identity). Return null if IMEI is not available.

Starting with API level 29, persistent device identifiers are guarded behind additional restrictions, and apps are recommended to use resettable identifiers (see Best practices for unique identifiers). This method can be invoked if one of the following requirements is met:

- If the calling app has been granted the READ_PRIVILEGED_PHONE_STATE permission; this is a privileged permission that can only be granted to apps preloaded on the device.
- If the calling app is the device owner of a fully-managed device, a profile owner of an organization-owned device, or their delegates (see `DevicePolicyManager.getEnrollmentSpecificId()`).
- If the calling app has carrier privileges (see `hasCarrierPrivileges()`) on any active subscription.
- If the calling app is the default SMS role holder (see `RoleManager.isRoleHeld(java.lang.String)`).
- If the calling app has been granted the `Manifest.permission#USE_ICC_AUTH_WITH_DEVICE_IDENTIFIER` permission.

If the calling app does not meet one of these requirements then this method will behave as follows:

- If the calling app's target SDK is API level 28 or lower and the app has the READ_PHONE_STATE permission then null is returned.
- If the calling app's target SDK is API level 28 or lower and the app does not have the READ_PHONE_STATE permission, or if the calling app is targeting API level 29 or higher, then a SecurityException is thrown.

Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Parameters
`slotIndex` | `int`: of which IMEI is returned

Returns
`String` |

### getImei

    public String getImei ()

Returns the IMEI (International Mobile Equipment Identity). Return null if IMEI is not available. See `getImei(int)` for details on the required permissions and behavior when the caller does not hold sufficient permissions.
Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Returns
`String` |

### getLine1Number

    public String getLine1Number ()

Returns the phone number string for line 1, for example, the MSISDN for a GSM phone for a particular subscription. Return null if it is unavailable.

The default SMS app can also use this.

Requires Permission: `READ_SMS`, `READ_PHONE_NUMBERS`, that the caller is the default SMS app, or that the caller has carrier privileges (see `hasCarrierPrivileges()`) for any API level. `READ_PHONE_STATE` for apps targeting SDK API level 29 and below.
Requires `Manifest.permission.READ_PHONE_STATE` or `Manifest.permission.READ_SMS` or `Manifest.permission.READ_PHONE_NUMBERS`

Returns
`String` |

### getManualNetworkSelectionPlmn

    public String getManualNetworkSelectionPlmn ()

Get the PLMN chosen for Manual Network Selection if active. Return null string if in automatic selection.

Requires Permission: `READ_PRECISE_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`)
Requires `Manifest.permission.READ_PRECISE_PHONE_STATE`

Returns
`String` | manually selected network info on success or null string on failure

### getManufacturerCode

    public String getManufacturerCode (int slotIndex)

Returns the Manufacturer Code from the MEID. Return null if Manufacturer Code is not available.

Parameters
`slotIndex` | `int`: of which Type Allocation Code is returned

Returns
`String` |

### getManufacturerCode

    public String getManufacturerCode ()

Returns the Manufacturer Code from the MEID. Return null if Manufacturer Code is not available.

Returns
`String` |

### getMaximumCallComposerPictureSize

    public static long getMaximumCallComposerPictureSize ()

Indicates the maximum size of the call composure picture. Pictures sent via `uploadCallComposerPicture(java.io.InputStream, java.lang.String, java.util.concurrent.Executor, android.os.OutcomeReceiver)` or `uploadCallComposerPicture(java.nio.file.Path, java.lang.String, java.util.concurrent.Executor, android.os.OutcomeReceiver)` must not exceed this size, or an error will be returned via the callback in those methods.
Value is a non-negative number of bytes.

Returns
`long` | Maximum file size in bytes. Value is a non-negative number of bytes.

### getMeid

    public String getMeid ()

Returns the MEID (Mobile Equipment Identifier). Return null if MEID is not available.

Starting with API level 29, persistent device identifiers are guarded behind additional restrictions, and apps are recommended to use resettable identifiers (see Best practices for unique identifiers). This method can be invoked if one of the following requirements is met:

- If the calling app has been granted the READ_PRIVILEGED_PHONE_STATE permission; this is a privileged permission that can only be granted to apps preloaded on the device.
- If the calling app is the device owner of a fully-managed device, a profile owner of an organization-owned device, or their delegates (see `DevicePolicyManager.getEnrollmentSpecificId()`).
- If the calling app has carrier privileges (see `hasCarrierPrivileges()`) on any active subscription.
- If the calling app is the default SMS role holder (see `RoleManager.isRoleHeld(java.lang.String)`).

If the calling app does not meet one of these requirements then this method will behave as follows:

- If the calling app's target SDK is API level 28 or lower and the app has the READ_PHONE_STATE permission then null is returned.
- If the calling app's target SDK is API level 28 or lower and the app does not have the READ_PHONE_STATE permission, or if the calling app is targeting API level 29 or higher, then a SecurityException is thrown.

Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Returns
`String` |

### getMeid

    public String getMeid (int slotIndex)

Returns the MEID (Mobile Equipment Identifier). Return null if MEID is not available.

Starting with API level 29, persistent device identifiers are guarded behind additional restrictions, and apps are recommended to use resettable identifiers (see Best practices for unique identifiers). This method can be invoked if one of the following requirements is met:

- If the calling app has been granted the READ_PRIVILEGED_PHONE_STATE permission; this is a privileged permission that can only be granted to apps preloaded on the device.
- If the calling app is the device owner of a fully-managed device, a profile owner of an organization-owned device, or their delegates (see `DevicePolicyManager.getEnrollmentSpecificId()`).
- If the calling app has carrier privileges (see `hasCarrierPrivileges()`) on any active subscription.
- If the calling app is the default SMS role holder (see `RoleManager.isRoleHeld(java.lang.String)`).

If the calling app does not meet one of these requirements then this method will behave as follows:

- If the calling app's target SDK is API level 28 or lower and the app has the READ_PHONE_STATE permission then null is returned.
- If the calling app's target SDK is API level 28 or lower and the app does not have the READ_PHONE_STATE permission, or if the calling app is targeting API level 29 or higher, then a SecurityException is thrown.

Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Parameters
`slotIndex` | `int`: of which MEID is returned

Returns
`String` |

### getMmsUAProfUrl

    public String getMmsUAProfUrl ()

Returns the MMS user agent profile URL.

Returns
`String` |

### getMmsUserAgent

    public String getMmsUserAgent ()

Returns the MMS user agent.

Returns
`String` |

### getNai

    public String getNai ()

Returns the Network Access Identifier (NAI). Return null if NAI is not available.

Starting with API level 29, persistent device identifiers are guarded behind additional restrictions, and apps are recommended to use resettable identifiers (see Best practices for unique identifiers). This method can be invoked if one of the following requirements is met:

- If the calling app has been granted the READ_PRIVILEGED_PHONE_STATE permission; this is a privileged permission that can only be granted to apps preloaded on the device.
- If the calling app is the device owner of a fully-managed device, a profile owner of an organization-owned device, or their delegates (see `DevicePolicyManager.getEnrollmentSpecificId()`).
- If the calling app has carrier privileges (see `hasCarrierPrivileges()`).
- If the calling app is the default SMS role holder (see `RoleManager.isRoleHeld(java.lang.String)`).

If the calling app does not meet one of these requirements then this method will behave as follows:

- If the calling app's target SDK is API level 28 or lower and the app has the READ_PHONE_STATE permission then null is returned.
- If the calling app's target SDK is API level 28 or lower and the app does not have the READ_PHONE_STATE permission, or if the calling app is targeting API level 29 or higher, then a SecurityException is thrown.

Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Returns
`String` |

### getNetworkCountryIso

    public String getNetworkCountryIso ()

Returns the ISO-3166-1 alpha-2 country code equivalent of the MCC (Mobile Country Code) of the current registered operator or the cell nearby, if available. Note: Result may be unreliable on CDMA networks (use `getPhoneType()` to determine if on a CDMA network).

Returns
`String` | the lowercase 2 character ISO-3166-1 alpha-2 country code, or empty string if not available.

### getNetworkCountryIso

    public String getNetworkCountryIso (int slotIndex)

Returns the ISO-3166-1 alpha-2 country code equivalent of the MCC (Mobile Country Code) of the current registered operator or the cell nearby, if available. This is same as `getNetworkCountryIso()` but allowing specifying the SIM slot index. This is used for accessing network country info from the SIM slot that does not have SIM inserted. Note: Result may be unreliable on CDMA networks (use `getPhoneType()` to determine if on a CDMA network).

Parameters
`slotIndex` | `int`: the SIM slot index to get network country ISO.

Returns
`String` | the lowercase 2 character ISO-3166-1 alpha-2 country code, or empty string if not available. This value cannot be `null`.

Throws
`IllegalArgumentException` | when the slotIndex is invalid.

### getNetworkOperator

    public String getNetworkOperator ()

Returns the numeric name (MCC+MNC) of current registered operator.

Availability: Only when user is registered to a network. Result may be unreliable on CDMA networks (use `getPhoneType()` to determine if on a CDMA network).

Returns
`String` |

### getNetworkOperatorName

    public String getNetworkOperatorName ()

Returns the alphabetic name of current registered operator.

Availability: Only when user is registered to a network. Result may be unreliable on CDMA networks (use `getPhoneType()` to determine if on a CDMA network).

Returns
`String` |

### getNetworkSelectionMode

    public int getNetworkSelectionMode ()

Get the network selection mode.

If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()`

Requires Permission: `READ_PRECISE_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE or `Manifest.permission.READ_PRECISE_PHONE_STATE`

Returns
`int` | the network selection mode. Value is `NETWORK_SELECTION_MODE_UNKNOWN`, `NETWORK_SELECTION_MODE_AUTO`, or `NETWORK_SELECTION_MODE_MANUAL`

### getNetworkSlicingConfiguration

    public void getNetworkSlicingConfiguration (Executor executor,
                    OutcomeReceiver<NetworkSlicingConfig, TelephonyManager.NetworkSlicingException> callback)

Request to get the current slicing configuration including URSP rules and NSSAIs (configured, allowed and rejected). This method can be invoked if one of the following requirements is met:

- If the calling app has been granted the READ_PRIVILEGED_PHONE_STATE permission; this is a privileged permission that can only be granted to apps preloaded on the device.
- If the calling app has carrier privileges (see `hasCarrierPrivileges()`).

This will be invalid if the device does not support android.telephony.TelephonyManager#CAPABILITY_SLICING_CONFIG_SUPPORTED.
Requires the `TelephonyManager#CAPABILITY_SLICING_CONFIG_SUPPORTED` feature which can be detected using `PackageManager.hasSystemFeature(String)`.
Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Parameters
`executor` | `Executor`: the executor on which callback will be invoked. This value cannot be `null`. Callback and listener events are dispatched through this `Executor`, providing an easy way to control which thread is used. To dispatch events through the main thread of your application, you can use `Context.getMainExecutor()`. To dispatch events through a shared thread pool, you can use `AsyncTask#THREAD_POOL_EXECUTOR`.
`callback` | `OutcomeReceiver`: a callback to receive the current slicing configuration. This value cannot be `null`.

### getNetworkSpecifier

    public String getNetworkSpecifier ()

Returns the network specifier of the subscription ID pinned to the TelephonyManager. The network specifier is used by `NetworkRequest.Builder.setNetworkSpecifier(String)` to create a `NetworkRequest` that connects through the subscription.

Returns
`String` |

See also:

- `NetworkRequest.Builder.setNetworkSpecifier(String)`
- `createForSubscriptionId(int)`
- `createForPhoneAccountHandle(PhoneAccountHandle)`

### getNetworkType

    public int getNetworkType ()

This method is deprecated.
use `getDataNetworkType()`

Return the current data network type.
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`int` | the NETWORK_TYPE_xxxx for current data connection. Value is `NETWORK_TYPE_UNKNOWN`, `NETWORK_TYPE_GPRS`, `NETWORK_TYPE_EDGE`, `NETWORK_TYPE_UMTS`, `NETWORK_TYPE_CDMA`, `NETWORK_TYPE_EVDO_0`, `NETWORK_TYPE_EVDO_A`, `NETWORK_TYPE_1xRTT`, `NETWORK_TYPE_HSDPA`, `NETWORK_TYPE_HSUPA`, `NETWORK_TYPE_HSPA`, `NETWORK_TYPE_IDEN`, `NETWORK_TYPE_EVDO_B`, `NETWORK_TYPE_LTE`, `NETWORK_TYPE_EHRPD`, `NETWORK_TYPE_HSPAP`, `NETWORK_TYPE_GSM`, `NETWORK_TYPE_TD_SCDMA`, `NETWORK_TYPE_IWLAN`, or `NETWORK_TYPE_NR`

### getPhoneAccountHandle

    public PhoneAccountHandle getPhoneAccountHandle ()

Determines the `PhoneAccountHandle` associated with this TelephonyManager.

If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()`

Requires Permission android.Manifest.permission#READ_PRIVILEGED_PHONE_STATE or that the calling app has carrier privileges (see `hasCarrierPrivileges()`)
Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Returns
`PhoneAccountHandle` | The `PhoneAccountHandle` associated with the TelphonyManager, or `null` if there is no associated `PhoneAccountHandle`; this can happen if the subscription is data-only or an opportunistic subscription.

### getPhoneCount

    public int getPhoneCount ()

This method is deprecated.
Use `getActiveModemCount()` instead.

Returns the number of phones available. Returns 0 if none of voice, sms, data is not supported Returns 1 for Single standby mode (Single SIM functionality). Returns 2 for Dual standby mode (Dual SIM functionality). Returns 3 for Tri standby mode (Tri SIM functionality).

Returns
`int` |

### getPhoneType

    public int getPhoneType ()

Returns a constant indicating the device phone type. This indicates the type of radio used to transmit voice calls.

Returns
`int` |

See also:

- `PHONE_TYPE_NONE`
- `PHONE_TYPE_GSM`
- `PHONE_TYPE_CDMA`
- `PHONE_TYPE_SIP`

### getPreferredOpportunisticDataSubscription

    public int getPreferredOpportunisticDataSubscription ()

Get preferred opportunistic data subscription Id

Requires that the calling app has carrier privileges (see `hasCarrierPrivileges()`), or has either READ_PRIVILEGED_PHONE_STATE or `READ_PHONE_STATE` permission.
Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE or `Manifest.permission.READ_PHONE_STATE`

Returns
`int` | subId preferred opportunistic subscription id or `SubscriptionManager#DEFAULT_SUBSCRIPTION_ID` if there are no preferred subscription id

### getServiceState

    public ServiceState getServiceState ()

Returns the current `ServiceState` information.

If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()` If you want continuous updates of service state info, register a `PhoneStateListener` via `listen(PhoneStateListener, int)` with the `PhoneStateListener#LISTEN_SERVICE_STATE` event.

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`) and `Manifest.permission.ACCESS_COARSE_LOCATION`. May return `null` when the subscription is inactive or when there was an error communicating with the phone process.
Requires `Manifest.permission.READ_PHONE_STATE` and `Manifest.permission.ACCESS_COARSE_LOCATION`

Returns
`ServiceState` |

### getSignalStrength

    public SignalStrength getSignalStrength ()

Get the most recently available signal strength information. Get the most recent SignalStrength information reported by the modem. Due to power saving this information may not always be current.

Returns
`SignalStrength` | the most recent cached signal strength info from the modem This value may be `null`.

### getSimCarrierId

    public int getSimCarrierId ()

Returns carrier id of the current subscription.

To recognize a carrier (including MVNO) as a first-class identity, Android assigns each carrier with a canonical integer a.k.a. carrier id. The carrier ID is an Android platform-wide identifier for a carrier. AOSP maintains carrier ID assignments in here

Apps which have carrier-specific configurations or business logic can use the carrier id as an Android platform-wide identifier for carriers.

Returns
`int` | Carrier id of the current subscription. Return `UNKNOWN_CARRIER_ID` if the subscription is unavailable or the carrier cannot be identified.

### getSimCarrierIdName

    public CharSequence getSimCarrierIdName ()

Returns carrier id name of the current subscription.

Carrier id name is a user-facing name of carrier id returned by `getSimCarrierId()`, usually the brand name of the subsidiary (e.g. T-Mobile). Each carrier could configure multiple `SPN` but should have a single carrier name. Carrier name is not a canonical identity, use `getSimCarrierId()` instead.

The returned carrier name is unlocalized.

Returns
`CharSequence` | Carrier name of the current subscription. Return `null` if the subscription is unavailable or the carrier cannot be identified.

### getSimCountryIso

    public String getSimCountryIso ()

Returns the ISO-3166-1 alpha-2 country code equivalent for the SIM provider's country code.

The ISO-3166-1 alpha-2 country code is provided in lowercase 2 character format.

Returns
`String` | the lowercase 2 character ISO-3166-1 alpha-2 country code, or empty string is not available.

### getSimOperator

    public String getSimOperator ()

Returns the MCC+MNC (mobile country code + mobile network code) of the provider of the SIM. 5 or 6 decimal digits.

Availability: SIM state must be `SIM_STATE_READY`

Returns
`String` |

See also:

- `getSimState()`

### getSimOperatorName

    public String getSimOperatorName ()

Returns the Service Provider Name (SPN).

Availability: SIM state must be `SIM_STATE_READY`

Returns
`String` |

See also:

- `getSimState()`

### getSimSerialNumber

    public String getSimSerialNumber ()

Returns the serial number of the SIM, if applicable. Return null if it is unavailable.

Starting with API level 29, persistent device identifiers are guarded behind additional restrictions, and apps are recommended to use resettable identifiers (see Best practices for unique identifiers). This method can be invoked if one of the following requirements is met:

- If the calling app has been granted the READ_PRIVILEGED_PHONE_STATE permission; this is a privileged permission that can only be granted to apps preloaded on the device.
- If the calling app is the device owner of a fully-managed device, a profile owner of an organization-owned device, or their delegates (see `DevicePolicyManager.getEnrollmentSpecificId()`).
- If the calling app has carrier privileges (see `hasCarrierPrivileges()`).
- If the calling app is the default SMS role holder (see `RoleManager.isRoleHeld(java.lang.String)`).

If the calling app does not meet one of these requirements then this method will behave as follows:

- If the calling app's target SDK is API level 28 or lower and the app has the READ_PHONE_STATE permission then null is returned.
- If the calling app's target SDK is API level 28 or lower and the app does not have the READ_PHONE_STATE permission, or if the calling app is targeting API level 29 or higher, then a SecurityException is thrown.

Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Returns
`String` |

### getSimSpecificCarrierId

    public int getSimSpecificCarrierId ()

Returns fine-grained carrier ID of the current subscription. A specific carrier ID can represent the fact that a carrier may be in effect an aggregation of other carriers (ie in an MVNO type scenario) where each of these specific carriers which are used to make up the actual carrier service may have different carrier configurations. A specific carrier ID could also be used, for example, in a scenario where a carrier requires different carrier configuration for different service offering such as a prepaid plan. the specific carrier ID would be used for configuration purposes, but apps wishing to know about the carrier itself should use the regular carrier ID returned by `getSimCarrierId()`. e.g, Tracfone SIMs could return different specific carrier ID based on IMSI from current subscription while carrier ID remains the same.

For carriers without fine-grained specific carrier ids, return `getSimCarrierId()`

Specific carrier ids are defined in the same way as carrier id here except each with a "parent" id linking to its top-level carrier id.

Returns
`int` | Returns fine-grained carrier id of the current subscription. Return `UNKNOWN_CARRIER_ID` if the subscription is unavailable or the carrier cannot be identified.

### getSimSpecificCarrierIdName

    public CharSequence getSimSpecificCarrierIdName ()

Similar like `getSimCarrierIdName()`, returns user-facing name of the specific carrier id returned by `getSimSpecificCarrierId()`. The specific carrier ID would be used for configuration purposes, but apps wishing to know about the carrier itself should use the regular carrier ID returned by `getSimCarrierIdName()`.

The returned name is unlocalized.

Returns
`CharSequence` | user-facing name of the subscription specific carrier id. Return `null` if the subscription is unavailable or the carrier cannot be identified.

### getSimState

    public int getSimState ()

Returns a constant indicating the state of the default SIM card.

Returns
`int` | Value is `SIM_STATE_UNKNOWN`, `SIM_STATE_ABSENT`, `SIM_STATE_PIN_REQUIRED`, `SIM_STATE_PUK_REQUIRED`, `SIM_STATE_NETWORK_LOCKED`, `SIM_STATE_READY`, `SIM_STATE_NOT_READY`, `SIM_STATE_PERM_DISABLED`, `SIM_STATE_CARD_IO_ERROR`, `SIM_STATE_CARD_RESTRICTED`, android.telephony.TelephonyManager.SIM_STATE_LOADED, or android.telephony.TelephonyManager.SIM_STATE_PRESENT

See also:

- `SIM_STATE_UNKNOWN`
- `SIM_STATE_ABSENT`
- `SIM_STATE_PIN_REQUIRED`
- `SIM_STATE_PUK_REQUIRED`
- `SIM_STATE_NETWORK_LOCKED`
- `SIM_STATE_READY`
- `SIM_STATE_NOT_READY`
- `SIM_STATE_PERM_DISABLED`
- `SIM_STATE_CARD_IO_ERROR`
- `SIM_STATE_CARD_RESTRICTED`

### getSimState

    public int getSimState (int slotIndex)

Returns a constant indicating the state of the device SIM card in a logical slot.

Parameters
`slotIndex` | `int`: logical slot index

Returns
`int` | Value is `SIM_STATE_UNKNOWN`, `SIM_STATE_ABSENT`, `SIM_STATE_PIN_REQUIRED`, `SIM_STATE_PUK_REQUIRED`, `SIM_STATE_NETWORK_LOCKED`, `SIM_STATE_READY`, `SIM_STATE_NOT_READY`, `SIM_STATE_PERM_DISABLED`, `SIM_STATE_CARD_IO_ERROR`, `SIM_STATE_CARD_RESTRICTED`, android.telephony.TelephonyManager.SIM_STATE_LOADED, or android.telephony.TelephonyManager.SIM_STATE_PRESENT

See also:

- `SIM_STATE_UNKNOWN`
- `SIM_STATE_ABSENT`
- `SIM_STATE_PIN_REQUIRED`
- `SIM_STATE_PUK_REQUIRED`
- `SIM_STATE_NETWORK_LOCKED`
- `SIM_STATE_READY`
- `SIM_STATE_NOT_READY`
- `SIM_STATE_PERM_DISABLED`
- `SIM_STATE_CARD_IO_ERROR`
- `SIM_STATE_CARD_RESTRICTED`

### getSubscriberId

    public String getSubscriberId ()

Returns the unique subscriber ID, for example, the IMSI for a GSM phone. Return null if it is unavailable.

Starting with API level 29, persistent device identifiers are guarded behind additional restrictions, and apps are recommended to use resettable identifiers (see Best practices for unique identifiers). This method can be invoked if one of the following requirements is met:

- If the calling app has been granted the READ_PRIVILEGED_PHONE_STATE permission; this is a privileged permission that can only be granted to apps preloaded on the device.
- If the calling app is the device owner of a fully-managed device, a profile owner of an organization-owned device, or their delegates (see `DevicePolicyManager.getEnrollmentSpecificId()`).
- If the calling app has carrier privileges (see `hasCarrierPrivileges()`).
- If the calling app is the default SMS role holder (see `RoleManager.isRoleHeld(java.lang.String)`).
- If the calling app has been granted the `Manifest.permission#USE_ICC_AUTH_WITH_DEVICE_IDENTIFIER` permission.

If the calling app does not meet one of these requirements then this method will behave as follows:

- If the calling app's target SDK is API level 28 or lower and the app has the READ_PHONE_STATE permission then null is returned.
- If the calling app's target SDK is API level 28 or lower and the app does not have the READ_PHONE_STATE permission, or if the calling app is targeting API level 29 or higher, then a SecurityException is thrown.

Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Returns
`String` |

### getSubscriptionId

    public int getSubscriptionId (PhoneAccountHandle phoneAccountHandle)

Returns the subscription ID for the given phone account handle.
Requires `Manifest.permission.READ_PHONE_STATE`

Parameters
`phoneAccountHandle` | `PhoneAccountHandle`: the phone account handle for outgoing calls This value cannot be `null`.

Returns
`int` | subscription ID for the given phone account handle; or `SubscriptionManager#INVALID_SUBSCRIPTION_ID` if not available; or throw a SecurityException if the caller doesn't have the permission.

### getSubscriptionId

    public int getSubscriptionId ()

Return an appropriate subscription ID for any situation. If this object has been created with `createForSubscriptionId(int)`, then the provided subscription ID is returned. Otherwise, the default subscription ID will be returned.

Returns
`int` |

### getSupportedModemCount

    public int getSupportedModemCount ()

Return how many logical modem can be potentially active simultaneously, in terms of hardware capability. It might return different value from `getActiveModemCount()`. For example, for a dual-SIM capable device operating in single SIM mode (only one logical modem is turned on), `getActiveModemCount()` returns 1 while this API returns 2.

Returns
`int` |

### getTypeAllocationCode

    public String getTypeAllocationCode ()

Returns the Type Allocation Code from the IMEI. Return null if Type Allocation Code is not available.

Returns
`String` |

### getTypeAllocationCode

    public String getTypeAllocationCode (int slotIndex)

Returns the Type Allocation Code from the IMEI. Return null if Type Allocation Code is not available.

Parameters
`slotIndex` | `int`: of which Type Allocation Code is returned

Returns
`String` |

### getUiccCardsInfo

    public List<UiccCardInfo> getUiccCardsInfo ()

Gets information about currently inserted UICCs and eUICCs.

Requires that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

If the caller has carrier priviliges on any active subscription, then they have permission to get simple information like the card ID (`UiccCardInfo#getCardId()`), whether the card is an eUICC (`UiccCardInfo#isEuicc()`), and the slot index where the card is inserted (`UiccCardInfo#getSlotIndex()`).

To get private information such as the EID (`UiccCardInfo#getEid()`) or ICCID (`UiccCardInfo#getIccId()`), the caller must have carrier priviliges on that specific UICC or eUICC card.

See `UiccCardInfo` for more details on the kind of information available.
Requires android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Returns
`List<UiccCardInfo>` | a list of UiccCardInfo objects, representing information on the currently inserted UICCs and eUICCs. Each UiccCardInfo in the list will have private information filtered out if the caller does not have adequate permissions for that card. This value cannot be `null`.

### getVisualVoicemailPackageName

    public String getVisualVoicemailPackageName ()

Returns the package responsible of processing visual voicemail for the subscription ID pinned to the TelephonyManager. Returns `null` when there is no package responsible for processing visual voicemail for the subscription.

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`String` |

See also:

- `createForSubscriptionId(int)`
- `createForPhoneAccountHandle(PhoneAccountHandle)`
- `VisualVoicemailService`

### getVoiceMailAlphaTag

    public String getVoiceMailAlphaTag ()

Retrieves the alphabetic identifier associated with the voice mail number.

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`String` |

### getVoiceMailNumber

    public String getVoiceMailNumber ()

Returns the voice mail number. Return null if it is unavailable.

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`String` |

### getVoiceNetworkType

    public int getVoiceNetworkType ()

Returns the NETWORK_TYPE_xxxx for voice

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`int` | Value is `NETWORK_TYPE_UNKNOWN`, `NETWORK_TYPE_GPRS`, `NETWORK_TYPE_EDGE`, `NETWORK_TYPE_UMTS`, `NETWORK_TYPE_CDMA`, `NETWORK_TYPE_EVDO_0`, `NETWORK_TYPE_EVDO_A`, `NETWORK_TYPE_1xRTT`, `NETWORK_TYPE_HSDPA`, `NETWORK_TYPE_HSUPA`, `NETWORK_TYPE_HSPA`, `NETWORK_TYPE_IDEN`, `NETWORK_TYPE_EVDO_B`, `NETWORK_TYPE_LTE`, `NETWORK_TYPE_EHRPD`, `NETWORK_TYPE_HSPAP`, `NETWORK_TYPE_GSM`, `NETWORK_TYPE_TD_SCDMA`, `NETWORK_TYPE_IWLAN`, or `NETWORK_TYPE_NR`

### getVoicemailRingtoneUri

    public Uri getVoicemailRingtoneUri (PhoneAccountHandle accountHandle)

Returns the URI for the per-account voicemail ringtone set in Phone settings.

Parameters
`accountHandle` | `PhoneAccountHandle`: The handle for the `PhoneAccount` for which to retrieve the voicemail ringtone.

Returns
`Uri` | The URI for the ringtone to play when receiving a voicemail from a specific PhoneAccount. May be `null` if no ringtone is set.

### hasCarrierPrivileges

    public boolean hasCarrierPrivileges ()

Has the calling application been granted carrier privileges by the carrier. If any of the packages in the calling UID has carrier privileges, the call will return true. This access is granted by the owner of the UICC card and does not depend on the registered carrier. Note that this API applies to both physical and embedded subscriptions and is a superset of the checks done in SubscriptionManager#canManageSubscription.

Returns
`boolean` | true if the app has carrier privileges.

### hasIccCard

    public boolean hasIccCard ()

Returns
`boolean` | true if a ICC card is present

### iccCloseLogicalChannel

    public boolean iccCloseLogicalChannel (int channel)

This method is deprecated.
Use `SEService` APIs instead. See `Channel.close()`.

Closes a previously opened logical channel to the ICC card. Input parameters equivalent to TS 27.007 AT+CCHC command.

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Parameters
`channel` | `int`: is the channel id to be closed as returned by a successful iccOpenLogicalChannel.

Returns
`boolean` | true if the channel was closed successfully.

### iccExchangeSimIO

    public byte[] iccExchangeSimIO (int fileID,
                    int command,
                    int p1,
                    int p2,
                    int p3,
                    String filePath)

This method is deprecated.
Use `SEService` APIs instead. See `SEService.getUiccReader(int)`, `Reader.openSession()`, `Session.openBasicChannel(byte[], byte)`, `Channel.transmit(byte[])`.

Returns the response APDU for a command APDU sent through SIM_IO.

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Parameters
`p1` | `int`: P1 value of the APDU command.
`p2` | `int`: P2 value of the APDU command.
`p3` | `int`: P3 value of the APDU command.

Returns
`byte[]` | The APDU response.

### iccOpenLogicalChannel

    public IccOpenLogicalChannelResponse iccOpenLogicalChannel (String AID,
                    int p2)

This method is deprecated.
Use `SEService` APIs instead. See `SEService.getUiccReader(int)`, `Reader.openSession()`, `Session.openLogicalChannel(byte[], byte)`.

Opens a logical channel to the ICC card. This operation wraps two APDU instructions:

- MANAGE CHANNEL to open a logical channel
- SELECT the given `AID` using the given `p2`

Per Open Mobile API Specification v3.2 section 6.2.7.h, only p2 values of 0x00, 0x04, 0x08, and 0x0C are guaranteed to be supported. If the SELECT command's status word is not '9000', '62xx', or '63xx', the status word will be considered an error and the channel shall not be opened. Input parameters equivalent to TS 27.007 AT+CCHO command.

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Parameters
`AID` | `String`: Application id. See ETSI 102.221 and 101.220.
`p2` | `int`: P2 parameter (described in ISO 7816-4).

Returns
`IccOpenLogicalChannelResponse` | an IccOpenLogicalChannelResponse object.

### iccOpenLogicalChannel

    public IccOpenLogicalChannelResponse iccOpenLogicalChannel (String AID)

This method is deprecated.
Replaced by `iccOpenLogicalChannel(java.lang.String, int)`

Opens a logical channel to the ICC card. Input parameters equivalent to TS 27.007 AT+CCHO command.

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Parameters
`AID` | `String`: Application id. See ETSI 102.221 and 101.220.

Returns
`IccOpenLogicalChannelResponse` | an IccOpenLogicalChannelResponse object.

### iccTransmitApduBasicChannel

    public String iccTransmitApduBasicChannel (int cla,
                    int instruction,
                    int p1,
                    int p2,
                    int p3,
                    String data)

This method is deprecated.
Use `SEService` APIs instead. See `SEService.getUiccReader(int)`, `Reader.openSession()`, `Session.openBasicChannel(byte[], byte)`, `Channel.transmit(byte[])`.

Transmit an APDU to the ICC card over the basic channel. Input parameters equivalent to TS 27.007 AT+CSIM command.

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Parameters
`cla` | `int`: Class of the APDU command.
`instruction` | `int`: Instruction of the APDU command.
`p1` | `int`: P1 value of the APDU command.
`p2` | `int`: P2 value of the APDU command.
`p3` | `int`: P3 value of the APDU command. If p3 is negative a 4 byte APDU is sent to the SIM.
`data` | `String`: Data to be sent with the APDU.

Returns
`String` | The APDU response from the ICC card with the status appended at the end.

### iccTransmitApduLogicalChannel

    public String iccTransmitApduLogicalChannel (int channel,
                    int cla,
                    int instruction,
                    int p1,
                    int p2,
                    int p3,
                    String data)

This method is deprecated.
Use `SEService` APIs instead. See `Channel.transmit(byte[])`.

Transmit an APDU to the ICC card over a logical channel. Input parameters equivalent to TS 27.007 AT+CGLA command.

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Parameters
`channel` | `int`: is the channel id to be closed as returned by a successful iccOpenLogicalChannel.
`cla` | `int`: Class of the APDU command.
`instruction` | `int`: Instruction of the APDU command.
`p1` | `int`: P1 value of the APDU command.
`p2` | `int`: P2 value of the APDU command.
`p3` | `int`: P3 value of the APDU command. If p3 is negative a 4 byte APDU is sent to the SIM.
`data` | `String`: Data to be sent with the APDU.

Returns
`String` | The APDU response from the ICC card with the status appended at the end.

### isConcurrentVoiceAndDataSupported

    public boolean isConcurrentVoiceAndDataSupported ()

Whether the device is currently on a technology (e.g. UMTS or LTE) which can support voice and data simultaneously. This can change based on location or network condition.

Returns
`boolean` | `true` if simultaneous voice and data supported, and `false` otherwise.

### isDataCapable

    public boolean isDataCapable ()

Returns
`boolean` | true if the current device is "data capable" over a radio on the device. "Data capable" means that this device supports packet-switched data connections over the telephony network.

### isDataConnectionAllowed

    public boolean isDataConnectionAllowed ()

Checks whether cellular data connection is allowed in the device.

Whether cellular data connection is allowed considers all factors below:

- User turned on data setting `isDataEnabled()`.
- Carrier allows data to be on.
- Network policy.
- And possibly others.

Requires `Manifest.permission.ACCESS_NETWORK_STATE` or `Manifest.permission.READ_PHONE_STATE` or android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Returns
`boolean` | `true` if the overall data connection is allowed; `false` if not. Requires Permission: `READ_PHONE_STATE` or `Manifest.permission.ACCESS_NETWORK_STATE` or android.Manifest.permission#READ_PRIVILEGED_PHONE_STATE

### isDataEnabled

    public boolean isDataEnabled ()

Returns whether mobile data is enabled or not per user setting. There are other factors that could disable mobile data, but they are not considered here. If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultDataSubscriptionId()`

Requires one of the following permissions: `Manifest.permission.ACCESS_NETWORK_STATE`, `Manifest.permission.MODIFY_PHONE_STATE`, or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Note that this does not take into account any data restrictions that may be present on the calling app. Such restrictions may be inspected with `ConnectivityManager#getRestrictBackgroundStatus`.
Requires `Manifest.permission.ACCESS_NETWORK_STATE` or `Manifest.permission.MODIFY_PHONE_STATE` or `Manifest.permission.READ_PHONE_STATE`

Returns
`boolean` | true if mobile data is enabled.

### isDataEnabledForReason

    public boolean isDataEnabledForReason (int reason)

Return whether data is enabled for certain reason . If `isDataEnabledForReason(int)` returns false, it means in data enablement for a specific reason is turned off. If any of the reason is off, then it will result in bypassing user preference and result in data to be turned off. Call `isDataConnectionAllowed()` in order to know whether data connection is allowed on the device.

If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultDataSubscriptionId()`
Requires `Manifest.permission.ACCESS_NETWORK_STATE` or `Manifest.permission.READ_PHONE_STATE`

Parameters
`reason` | `int`: the reason the data enable change is taking place Value is `DATA_ENABLED_REASON_USER`, `DATA_ENABLED_REASON_POLICY`, `DATA_ENABLED_REASON_CARRIER`, or `DATA_ENABLED_REASON_THERMAL`

Returns
`boolean` | whether data is enabled for a reason. Requires Permission: `READ_PHONE_STATE` or `Manifest.permission.ACCESS_NETWORK_STATE`

Throws
`IllegalStateException` | if the Telephony process is not currently available.

### isDataRoamingEnabled

    public boolean isDataRoamingEnabled ()

Returns whether mobile data roaming is enabled on the subscription.

If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultDataSubscriptionId()`

Requires one of the following permissions: `Manifest.permission.ACCESS_NETWORK_STATE`, `Manifest.permission.READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.ACCESS_NETWORK_STATE` or `Manifest.permission.READ_PHONE_STATE`

Returns
`boolean` | `true` if the data roaming is enabled on the subscription, otherwise return `false`.

### isEmergencyNumber

    public boolean isEmergencyNumber (String number)

Identifies if the supplied phone number is an emergency number that matches a known emergency number based on current locale, SIM card(s), Android database, modem, network, or defaults.

This method assumes that only dialable phone numbers are passed in; non-dialable numbers are not considered emergency numbers. A dialable phone number consists only of characters/digits identified by `PhoneNumberUtils#isDialable(char)`.

The subscriptions which the identification would be based on, are all the active subscriptions, no matter which subscription could be used to create TelephonyManager.

Parameters
`number` | `String`: - the number to look up This value cannot be `null`.

Returns
`boolean` | `true` if the given number is an emergency number based on current locale, SIM card(s), Android database, modem, network or defaults; `false` otherwise.

Throws
`IllegalStateException` | if the Telephony process is not currently available.

### isHearingAidCompatibilitySupported

    public boolean isHearingAidCompatibilitySupported ()

Whether the phone supports hearing aid compatibility.

Returns
`boolean` | `true` if the device supports hearing aid compatibility, and `false` otherwise.

### isManualNetworkSelectionAllowed

    public boolean isManualNetworkSelectionAllowed ()

Checks if manual network selection is allowed.

Requires Permission: `READ_PRECISE_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`)

If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()`.
Requires `Manifest.permission.READ_PRECISE_PHONE_STATE` or android.Manifest.permission.READ_PRIVILEGED_PHONE_STATE

Returns
`boolean` | `true` if manual network selection is allowed, otherwise return `false`.

### isModemEnabledForSlot

    public boolean isModemEnabledForSlot (int slotIndex)

It indicates whether modem is enabled or not per slot. It's the corresponding status of TelephonyManager.enableModemForSlot.

Requires Permission: READ_PRIVILEGED_PHONE_STATE or `READ_PHONE_STATE`
Requires `Manifest.permission.READ_PHONE_STATE`

Parameters
`slotIndex` | `int`: which slot it's checking.

Returns
`boolean` |

### isMultiSimSupported

    public int isMultiSimSupported ()

Returns if the usage of multiple SIM cards at the same time to register on the network (e.g. Dual Standby or Dual Active) is supported by the device and by the carrier.

Requires Permission: `READ_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.READ_PHONE_STATE`

Returns
`int` | `MULTISIM_ALLOWED` if the device supports multiple SIMs. `MULTISIM_NOT_SUPPORTED_BY_HARDWARE` if the device does not support multiple SIMs. `MULTISIM_NOT_SUPPORTED_BY_CARRIER` in the device supports multiple SIMs, but the functionality is restricted by the carrier. Value is `MULTISIM_ALLOWED`, `MULTISIM_NOT_SUPPORTED_BY_HARDWARE`, or `MULTISIM_NOT_SUPPORTED_BY_CARRIER`

### isNetworkRoaming

    public boolean isNetworkRoaming ()

Returns true if the device is considered roaming on the current network, for GSM purposes.

Availability: Only when user registered to a network.

Returns
`boolean` |

### isRadioInterfaceCapabilitySupported

    public boolean isRadioInterfaceCapabilitySupported (String capability)

Whether the device supports a given capability on the radio interface. If the capability is not in the set of radio interface capabilities, false is returned.

Parameters
`capability` | `String`: the name of the capability to check for This value cannot be `null`. Value is `CAPABILITY_SLICING_CONFIG_SUPPORTED`, or android.telephony.TelephonyManager.CAPABILITY_SIM_PHONEBOOK_IN_MODEM

Returns
`boolean` | the availability of the capability

### isRttSupported

    public boolean isRttSupported ()

Determines whether the device currently supports RTT (Real-time text). Based both on carrier support for the feature and device firmware support.

Returns
`boolean` | `true` if the device and carrier both support RTT, `false` otherwise.

### isSmsCapable

    public boolean isSmsCapable ()

Returns
`boolean` | true if the current device supports sms service. If true, this means that the device supports both sending and receiving sms via the telephony network. Note: Voicemail waiting sms, cell broadcasting sms, and MMS are disabled when device doesn't support sms.

### isTtyModeSupported

    public boolean isTtyModeSupported ()

This method is deprecated.
Use `TelecomManager#isTtySupported()` instead Whether the phone supports TTY mode.

Returns
`boolean` | `true` if the device supports TTY mode, and `false` otherwise.

### isVoiceCapable

    public boolean isVoiceCapable ()

Returns
`boolean` | true if the current device is "voice capable". "Voice capable" means that this device supports circuit-switched (i.e. voice) phone calls over the telephony network, and is allowed to display the in-call UI while a cellular voice call is active. This will be false on "data only" devices which can't make voice calls and don't support any in-call UI. Note: the meaning of this flag is subtly different from the PackageManager.FEATURE_TELEPHONY system feature, which is available on any device with a telephony radio, even if the device is data-only.

### isVoicemailVibrationEnabled

    public boolean isVoicemailVibrationEnabled (PhoneAccountHandle accountHandle)

Returns whether vibration is set for voicemail notification in Phone settings.

Parameters
`accountHandle` | `PhoneAccountHandle`: The handle for the `PhoneAccount` for which to retrieve the voicemail vibration setting.

Returns
`boolean` | `true` if the vibration is set for this PhoneAccount, `false` otherwise.

### isWorldPhone

    public boolean isWorldPhone ()

Whether the device is a world phone.

Returns
`boolean` | `true` if the device is a world phone, and `false` otherwise.

### listen

    public void listen (PhoneStateListener listener,
                    int events)

This method is deprecated.
Use `registerTelephonyCallback(java.util.concurrent.Executor, android.telephony.TelephonyCallback)`.

Registers a listener object to receive notification of changes in specified telephony states.

To register a listener, pass a `PhoneStateListener` and specify at least one telephony state of interest in the events argument. At registration, and when a specified telephony state changes, the telephony manager invokes the appropriate callback method on the listener object and passes the current (updated) values.

To un-register a listener, pass the listener object and set the events argument to `LISTEN_NONE` (0). If this TelephonyManager object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()`. To listen events for multiple subIds, pass a separate listener object to each TelephonyManager object created with `createForSubscriptionId(int)`. Note: if you call this method while in the middle of a binder transaction, you must call `Binder.clearCallingIdentity()` before calling this method. A `SecurityException` will be thrown otherwise. This API should be used sparingly -- large numbers of listeners will cause system instability. If a process has registered too many listeners without unregistering them, it may encounter an `IllegalStateException` when trying to register more listeners.

Parameters
`listener` | `PhoneStateListener`: The `PhoneStateListener` object to register (or unregister)
`events` | `int`: The telephony state(s) of interest to the listener, as a bitwise-OR combination of `PhoneStateListener` LISTEN_ flags.

### registerTelephonyCallback

    public void registerTelephonyCallback (Executor executor,
                    TelephonyCallback callback)

Registers a callback object to receive notification of changes in specified telephony states.

To register a callback, pass a `TelephonyCallback` which implements interfaces of events. For example, FakeServiceStateCallback extends `TelephonyCallback` implements `TelephonyCallback.ServiceStateListener`. At registration, and when a specified telephony state changes, the telephony manager invokes the appropriate callback method on the callback object and passes the current (updated) values.

If this TelephonyManager object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()`. To register events for multiple subIds, pass a separate callback object to each TelephonyManager object created with `createForSubscriptionId(int)`. Note: if you call this method while in the middle of a binder transaction, you must call `Binder.clearCallingIdentity()` before calling this method. A `SecurityException` will be thrown otherwise. This API should be used sparingly -- large numbers of callbacks will cause system instability. If a process has registered too many callbacks without unregistering them, it may encounter an `IllegalStateException` when trying to register more callbacks.

Parameters
`executor` | `Executor`: The executor of where the callback will execute. This value cannot be `null`. Callback and listener events are dispatched through this `Executor`, providing an easy way to control which thread is used. To dispatch events through the main thread of your application, you can use `Context.getMainExecutor()`. To dispatch events through a shared thread pool, you can use `AsyncTask#THREAD_POOL_EXECUTOR`.
`callback` | `TelephonyCallback`: The `TelephonyCallback` object to register. This value cannot be `null`.

### requestCellInfoUpdate

    public void requestCellInfoUpdate (Executor executor,
                    TelephonyManager.CellInfoCallback callback)

Requests all available cell information from the current subscription for observed camped/registered, serving, and neighboring cells.

Any available results from this request will be provided by calls to `onCellInfoChanged()` for each active subscription.

This method returns valid data for devices with `FEATURE_TELEPHONY`. On devices that do not implement this feature, the behavior is not reliable.
Requires `Manifest.permission.ACCESS_FINE_LOCATION`

Parameters
`executor` | `Executor`: the executor on which callback will be invoked. This value cannot be `null`. Callback and listener events are dispatched through this `Executor`, providing an easy way to control which thread is used. To dispatch events through the main thread of your application, you can use `Context.getMainExecutor()`. To dispatch events through a shared thread pool, you can use `AsyncTask#THREAD_POOL_EXECUTOR`.
`callback` | `TelephonyManager.CellInfoCallback`: a callback to receive CellInfo. This value cannot be `null`.

### requestNetworkScan

    public NetworkScan requestNetworkScan (NetworkScanRequest request,
                    Executor executor,
                    TelephonyScanManager.NetworkScanCallback callback)

Request a network scan. This method is asynchronous, so the network scan results will be returned by callback. The returned NetworkScan will contain a callback method which can be used to stop the scan.

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`) and `Manifest.permission.ACCESS_FINE_LOCATION`. If the system-wide location switch is off, apps may still call this API, with the following constraints:

1. The app must hold the `android.permission.NETWORK_SCAN` permission.
2. The app must not supply any specific bands or channels to scan.
3. The app must only specify MCC/MNC pairs that are associated to a SIM in the device.
4. Returned results will have no meaningful info other than signal strength and MCC/MNC info.

Requires `Manifest.permission.MODIFY_PHONE_STATE` and `Manifest.permission.ACCESS_FINE_LOCATION`

Parameters
`request` | `NetworkScanRequest`: Contains all the RAT with bands/channels that need to be scanned.
`executor` | `Executor`: The executor through which the callback should be invoked. Since the scan request may trigger multiple callbacks and they must be invoked in the same order as they are received by the platform, the user should provide an executor which executes tasks one at a time in serial order. For example AsyncTask.SERIAL_EXECUTOR.
`callback` | `TelephonyScanManager.NetworkScanCallback`: Returns network scan results or errors.

Returns
`NetworkScan` | A NetworkScan obj which contains a callback which can be used to stop the scan.

### sendDialerSpecialCode

    public void sendDialerSpecialCode (String inputCode)

Send the special dialer code. The IPC caller must be the current default dialer or have carrier privileges (see `hasCarrierPrivileges()`).

Parameters
`inputCode` | `String`: The special dialer code to send

Throws
`SecurityException` | if the caller does not have carrier privileges or is not the current default dialer

### sendEnvelopeWithStatus

    public String sendEnvelopeWithStatus (String content)

This method is deprecated.
Use `SEService` APIs instead. See `SEService.getUiccReader(int)`, `Reader.openSession()`, `Session.openBasicChannel(byte[], byte)`, `Channel.transmit(byte[])`.

Send ENVELOPE to the SIM and return the response.

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Parameters
`content` | `String`: String containing SAT/USAT response in hexadecimal format starting with command tag. See TS 102 223 for details.

Returns
`String` | The APDU response from the ICC card in hexadecimal format with the last 4 bytes being the status word. If the command fails, returns an empty string.

### sendUssdRequest

    public void sendUssdRequest (String ussdRequest,
                    TelephonyManager.UssdResponseCallback callback,
                    Handler handler)

Sends an Unstructured Supplementary Service Data (USSD) request to the mobile network and informs the caller of the response via the supplied `callback`.

Carriers define USSD codes which can be sent by the user to request information such as the user's current data balance or minutes balance.

Requires permission: `Manifest.permission.CALL_PHONE`
Requires `Manifest.permission.CALL_PHONE`

Parameters
`ussdRequest` | `String`: the USSD command to be executed.
`callback` | `TelephonyManager.UssdResponseCallback`: called by the framework to inform the caller of the result of executing the USSD request (see `UssdResponseCallback`).
`handler` | `Handler`: the `Handler` to run the request on.

### sendVisualVoicemailSms

    public void sendVisualVoicemailSms (String number,
                    int port,
                    String text,
                    PendingIntent sentIntent)

Send a visual voicemail SMS. The caller must be the current default dialer. A `VisualVoicemailService` uses this method to send a command via SMS to the carrier's visual voicemail server. Some examples for carriers using the OMTP standard include activating and deactivating visual voicemail, or requesting the current visual voicemail provisioning status. See the OMTP Visual Voicemail specification for more information on the format of these SMS messages.

Requires Permission: `SEND_SMS`

Parameters
`number` | `String`: The destination number.
`port` | `int`: The destination port for data SMS, or 0 for text SMS.
`text` | `String`: The message content. For data sms, it will be encoded as a UTF-8 byte stream.
`sentIntent` | `PendingIntent`: The sent intent passed to the `SmsManager`

Throws
`SecurityException` | if the caller is not the current default dialer

See also:

- `SmsManager.sendDataMessage(String, String, short, byte[], PendingIntent, PendingIntent)`
- `SmsManager.sendTextMessage(String, String, String, PendingIntent, PendingIntent)`

### setCallComposerStatus

    public void setCallComposerStatus (int status)

Set the user-set status for enriched calling with call composer.
Requires `Manifest.permission.MODIFY_PHONE_STATE`

Parameters
`status` | `int`: user-set status for enriched calling with call composer. If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()` Value is `CALL_COMPOSER_STATUS_ON`, or `CALL_COMPOSER_STATUS_OFF`

Throws
`IllegalArgumentException` | if requested state is invalid.
`SecurityException` | if the caller does not have the permission.

### setDataEnabled

    public void setDataEnabled (boolean enable)

This method is deprecated.
use setDataEnabledForReason with reason DATA_ENABLED_REASON_USER instead.

Turns mobile data on or off. If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultDataSubscriptionId()`

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.MODIFY_PHONE_STATE`

Parameters
`enable` | `boolean`: Whether to enable mobile data.

### setDataEnabledForReason

    public void setDataEnabledForReason (int reason,
                    boolean enabled)

Control of data connection and provide the reason triggering the data connection control. This can be called for following reasons

1. data limit is passed `DATA_ENABLED_REASON_POLICY`
2. data disabled by carrier `DATA_ENABLED_REASON_CARRIER`
3. data disabled by user `DATA_ENABLED_REASON_USER`
4. data disabled due to thermal `DATA_ENABLED_REASON_THERMAL`

If any of the reason is off, then it will result in bypassing user preference and result in data to be turned off.

If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultDataSubscriptionId()`
Requires `Manifest.permission.MODIFY_PHONE_STATE`

Parameters
`reason` | `int`: the reason the data enable change is taking place Value is `DATA_ENABLED_REASON_USER`, `DATA_ENABLED_REASON_POLICY`, `DATA_ENABLED_REASON_CARRIER`, or `DATA_ENABLED_REASON_THERMAL`
`enabled` | `boolean`: True if enabling the data, otherwise disabling. Requires Permission: The calling app has carrier privileges (see `hasCarrierPrivileges()`) if the reason is `DATA_ENABLED_REASON_USER` or `DATA_ENABLED_REASON_CARRIER` or the call app has `MODIFY_PHONE_STATE` irrespective of the reason.

Throws
`IllegalStateException` | if the Telephony process is not currently available.

### setForbiddenPlmns

    public int setForbiddenPlmns (List<String> fplmns)

Replace the contents of the forbidden PLMN SIM file with the provided values. Passing an empty list will clear the contents of the EFfplmn file. If the provided list is shorter than the size of EFfplmn, then the list will be padded up to the file size with 'FFFFFF'. (required by 3GPP TS 31.102 spec 4.2.16) If the list is longer than the size of EFfplmn, then the file will be written from the beginning of the list up to the file size.

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.MODIFY_PHONE_STATE`

Parameters
`fplmns` | `List`: a list of PLMNs to be forbidden. This value cannot be `null`.

Returns
`int` | number of PLMNs that were successfully written to the SIM FPLMN list. This may be less than the number of PLMNs passed in where the SIM file does not have enough room for all of the values passed in. Return -1 in the event of an unexpected failure

### setLine1NumberForDisplay

    public boolean setLine1NumberForDisplay (String alphaTag,
                    String number)

Set the line 1 phone number string and its alphatag for the current ICCID for display purpose only, for example, displayed in Phone Status. It won't change the actual MSISDN/MDN. To unset alphatag or number, pass in a null value.

Requires that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Parameters
`alphaTag` | `String`: alpha-tagging of the dailing nubmer
`number` | `String`: The dialing number

Returns
`boolean` | true if the operation was executed correctly.

### setNetworkSelectionModeAutomatic

    public void setNetworkSelectionModeAutomatic ()

Sets the network selection mode to automatic.

If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()`

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.MODIFY_PHONE_STATE`

### setNetworkSelectionModeManual

    public boolean setNetworkSelectionModeManual (String operatorNumeric,
                    boolean persistSelection,
                    int ran)

Ask the radio to connect to the input network and change selection mode to manual.

If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()`

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.MODIFY_PHONE_STATE`

Parameters
`operatorNumeric` | `String`: the PLMN ID of the network to select. This value cannot be `null`.
`persistSelection` | `boolean`: whether the selection will persist until reboot. If true, only allows attaching to the selected PLMN until reboot; otherwise, attach to the chosen PLMN and resume normal network selection next time.
`ran` | `int`: the initial suggested radio access network type. If registration fails, the RAN is not available after, the RAN is not within the network types specified by the preferred network types, or the value is `AccessNetworkConstants.AccessNetworkType#UNKNOWN`, modem will select the next best RAN for network registration. Value is `AccessNetworkConstants.AccessNetworkType.UNKNOWN`, `AccessNetworkConstants.AccessNetworkType.GERAN`, `AccessNetworkConstants.AccessNetworkType.UTRAN`, `AccessNetworkConstants.AccessNetworkType.EUTRAN`, `AccessNetworkConstants.AccessNetworkType.CDMA2000`, `AccessNetworkConstants.AccessNetworkType.IWLAN`, or `AccessNetworkConstants.AccessNetworkType.NGRAN`

Returns
`boolean` | `true` on success; `false` on any failure.

### setNetworkSelectionModeManual

    public boolean setNetworkSelectionModeManual (String operatorNumeric,
                    boolean persistSelection)

Ask the radio to connect to the input network and change selection mode to manual.

If this object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()`

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`).
Requires `Manifest.permission.MODIFY_PHONE_STATE`

Parameters
`operatorNumeric` | `String`: the PLMN ID of the network to select.
`persistSelection` | `boolean`: whether the selection will persist until reboot. If true, only allows attaching to the selected PLMN until reboot; otherwise, attach to the chosen PLMN and resume normal network selection next time.

Returns
`boolean` | `true` on success; `false` on any failure.

### setOperatorBrandOverride

    public boolean setOperatorBrandOverride (String brand)

Override the branding for the current ICCID. Once set, whenever the SIM is present in the device, the service provider name (SPN) and the operator name will both be replaced by the brand value input. To unset the value, the same function should be called with a null brand value.

Requires that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Parameters
`brand` | `String`: The brand name to display/set.

Returns
`boolean` | true if the operation was executed correctly.

### setPreferredNetworkTypeToGlobal

    public boolean setPreferredNetworkTypeToGlobal ()

Set the preferred network type to global mode which includes NR, LTE, CDMA, EvDo and GSM/WCDMA.

Requires that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Returns
`boolean` | true on success; false on any failure.

### setPreferredOpportunisticDataSubscription

    public void setPreferredOpportunisticDataSubscription (int subId,
                    boolean needValidation,
                    Executor executor,
                    Consumer<Integer> callback)

Set preferred opportunistic data subscription id. Switch internet data to preferred opportunistic data subscription id. This api can result in lose of internet connectivity for short period of time while internet data is handed over.

Requires that the calling app has carrier privileges on both primary and secondary subscriptions (see `hasCarrierPrivileges()`), or has permission `MODIFY_PHONE_STATE`.

Parameters
`subId` | `int`: which opportunistic subscription `SubscriptionManager#getOpportunisticSubscriptions` is preferred for cellular data. Pass `SubscriptionManager#DEFAULT_SUBSCRIPTION_ID` to unset the preference
`needValidation` | `boolean`: whether validation is needed before switch happens.
`executor` | `Executor`: The executor of where the callback will execute. This value may be `null`. Callback and listener events are dispatched through this `Executor`, providing an easy way to control which thread is used. To dispatch events through the main thread of your application, you can use `Context.getMainExecutor()`. To dispatch events through a shared thread pool, you can use `AsyncTask#THREAD_POOL_EXECUTOR`.
`callback` | `Consumer`: Callback will be triggered once it succeeds or failed. See `TelephonyManager.SetOpportunisticSubscriptionResult` for more details. Pass null if don't care about the result. This value may be `null`.

### setSignalStrengthUpdateRequest

    public void setSignalStrengthUpdateRequest (SignalStrengthUpdateRequest request)

Set a `SignalStrengthUpdateRequest` to receive notification when signal quality measurements breach the specified thresholds. To be notified, set the signal strength update request and then register `TelephonyManager#listen(PhoneStateListener, int)` with `PhoneStateListener#LISTEN_SIGNAL_STRENGTHS`. The notification will arrive through `PhoneStateListener#onSignalStrengthsChanged(SignalStrength)`. To stop receiving the notification over the specified thresholds, pass the same `SignalStrengthUpdateRequest` object to `clearSignalStrengthUpdateRequest(android.telephony.SignalStrengthUpdateRequest)`. System will clean up the `SignalStrengthUpdateRequest` if the caller process died without calling `clearSignalStrengthUpdateRequest(android.telephony.SignalStrengthUpdateRequest)`. If this TelephonyManager object has been created with `createForSubscriptionId(int)`, applies to the given subId. Otherwise, applies to `SubscriptionManager#getDefaultSubscriptionId()`. To request for multiple subIds, pass a request object to each TelephonyManager object created with `createForSubscriptionId(int)`.

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `TelephonyManager#hasCarrierPrivileges`). Note that the thresholds in the request will be used on a best-effort basis; the system may modify requests to multiplex various request sources or to optimize power consumption. The caller should not expect to be notified with the exactly the same thresholds.
Requires `Manifest.permission.MODIFY_PHONE_STATE`

Parameters
`request` | `SignalStrengthUpdateRequest`: the SignalStrengthUpdateRequest to be set into the System This value cannot be `null`.

Throws
`IllegalStateException` | if a new request is set with same subId from the same caller

See also:

- `clearSignalStrengthUpdateRequest(SignalStrengthUpdateRequest)`

### setVisualVoicemailSmsFilterSettings

    public void setVisualVoicemailSmsFilterSettings (VisualVoicemailSmsFilterSettings settings)

Set the visual voicemail SMS filter settings for the subscription ID pinned to the TelephonyManager. When the filter is enabled, `VisualVoicemailService.onSmsReceived(android.telephony.VisualVoicemailService.VisualVoicemailTask, android.telephony.VisualVoicemailSms)` will be called when a SMS matching the settings is received. Caller must be the default dialer, system dialer, or carrier visual voicemail app.

Parameters
`settings` | `VisualVoicemailSmsFilterSettings`: The settings for the filter, or `null` to disable the filter.

See also:

- `TelecomManager.getDefaultDialerPackage()`
- `CarrierConfigManager.KEY_CARRIER_VVM_PACKAGE_NAME_STRING_ARRAY`

### setVoiceMailNumber

    public boolean setVoiceMailNumber (String alphaTag,
                    String number)

Sets the voice mail number.

Requires that the calling app has carrier privileges (see `hasCarrierPrivileges()`).

Parameters
`alphaTag` | `String`: The alpha tag to display.
`number` | `String`: The voicemail number.

Returns
`boolean` |

### setVoicemailRingtoneUri

    public void setVoicemailRingtoneUri (PhoneAccountHandle phoneAccountHandle,
                    Uri uri)

This method is deprecated.
Use `Settings.ACTION_CHANNEL_NOTIFICATION_SETTINGS` instead.

Sets the per-account voicemail ringtone.

Requires that the calling app is the default dialer, or has carrier privileges (see `hasCarrierPrivileges()`, or has permission `MODIFY_PHONE_STATE`.

Parameters
`phoneAccountHandle` | `PhoneAccountHandle`: The handle for the `PhoneAccount` for which to set the voicemail ringtone.
`uri` | `Uri`: The URI for the ringtone to play when receiving a voicemail from a specific PhoneAccount.

### setVoicemailVibrationEnabled

    public void setVoicemailVibrationEnabled (PhoneAccountHandle phoneAccountHandle,
                    boolean enabled)

This method is deprecated.
Use `Settings.ACTION_CHANNEL_NOTIFICATION_SETTINGS` instead.

Sets the per-account preference whether vibration is enabled for voicemail notifications.

Requires that the calling app is the default dialer, or has carrier privileges (see `hasCarrierPrivileges()`, or has permission `MODIFY_PHONE_STATE`.

Parameters
`phoneAccountHandle` | `PhoneAccountHandle`: The handle for the `PhoneAccount` for which to set the voicemail vibration setting.
`enabled` | `boolean`: Whether to enable or disable vibration for voicemail notifications from a specific PhoneAccount.

### switchMultiSimConfig

    public void switchMultiSimConfig (int numOfSims)

Switch configs to enable multi-sim or switch back to single-sim

Requires Permission: `MODIFY_PHONE_STATE` or that the calling app has carrier privileges (see `hasCarrierPrivileges()`). Note: with only carrier privileges, it is not allowed to switch from multi-sim to single-sim
Requires `Manifest.permission.MODIFY_PHONE_STATE`

Parameters
`numOfSims` | `int`: number of live SIMs we want to switch to

Throws
`` | android.os.RemoteException

### unregisterTelephonyCallback

    public void unregisterTelephonyCallback (TelephonyCallback callback)

Unregister an existing `TelephonyCallback`.

Parameters
`callback` | `TelephonyCallback`: The `TelephonyCallback` object to unregister. This value cannot be `null`.

### updateAvailableNetworks

    public void updateAvailableNetworks (List<AvailableNetworkInfo> availableNetworks,
                    Executor executor,
                    Consumer<Integer> callback)

Update availability of a list of networks in the current location. This api should be called to inform OpportunisticNetwork Service about the availability of a network at the current location. This information will be used by OpportunisticNetwork service to enable modem stack and to attach to the network. If an empty list is passed, it is assumed that no network is available and will result in disabling the modem stack to save power. This api do not switch internet data once network attach is completed. Use `TelephonyManager#setPreferredOpportunisticDataSubscription` to switch internet data after network attach is complete. Requires that the calling app has carrier privileges on both primary and secondary subscriptions (see `hasCarrierPrivileges()`), or has permission `MODIFY_PHONE_STATE`.

Parameters
`availableNetworks` | `List`: is a list of available network information. This value cannot be `null`.
`executor` | `Executor`: The executor of where the callback will execute. This value may be `null`. Callback and listener events are dispatched through this `Executor`, providing an easy way to control which thread is used. To dispatch events through the main thread of your application, you can use `Context.getMainExecutor()`. To dispatch events through a shared thread pool, you can use `AsyncTask#THREAD_POOL_EXECUTOR`.
`callback` | `Consumer`: Callback will be triggered once it succeeds or failed. Value is `UPDATE_AVAILABLE_NETWORKS_SUCCESS`, `UPDATE_AVAILABLE_NETWORKS_UNKNOWN_FAILURE`, `UPDATE_AVAILABLE_NETWORKS_ABORTED`, `UPDATE_AVAILABLE_NETWORKS_INVALID_ARGUMENTS`, `UPDATE_AVAILABLE_NETWORKS_NO_CARRIER_PRIVILEGE`, `UPDATE_AVAILABLE_NETWORKS_DISABLE_MODEM_FAIL`, `UPDATE_AVAILABLE_NETWORKS_ENABLE_MODEM_FAIL`, `UPDATE_AVAILABLE_NETWORKS_MULTIPLE_NETWORKS_NOT_SUPPORTED`, `UPDATE_AVAILABLE_NETWORKS_NO_OPPORTUNISTIC_SUB_AVAILABLE`, `UPDATE_AVAILABLE_NETWORKS_REMOTE_SERVICE_EXCEPTION`, or `UPDATE_AVAILABLE_NETWORKS_SERVICE_IS_DISABLED` This value may be `null`.

### uploadCallComposerPicture

    public void uploadCallComposerPicture (InputStream pictureToUpload,
                    String contentType,
                    Executor executor,
                    OutcomeReceiver<ParcelUuid, TelephonyManager.CallComposerException> callback)

Uploads a picture to the carrier network for use with call composer. This method allows a dialer app to upload a picture to the carrier network that can then later be attached to an outgoing call. In order to attach the picture to a call, use the `ParcelUuid` returned from `callback` upon successful upload as the value to `TelecomManager#EXTRA_OUTGOING_PICTURE`. This functionality is only available to the app filling the `RoleManager#ROLE_DIALER` role on the device. This functionality is only available when `CarrierConfigManager#KEY_SUPPORTS_CALL_COMPOSER_BOOL` is set to `true` in the bundle returned from `getCarrierConfig()`.

Parameters
`pictureToUpload` | `InputStream`: An `InputStream` that supplies the bytes representing the picture to upload. The client bears responsibility for closing this stream after `callback` is called with success or failure. Additionally, if the stream supplies more bytes than the return value of `getMaximumCallComposerPictureSize()`, the upload will be aborted and the callback will be called with an exception containing `CallComposerException#ERROR_FILE_TOO_LARGE`. This value cannot be `null`.
`contentType` | `String`: The MIME type of the picture you're uploading (e.g. image/jpeg). The list of acceptable content types can be found at 3GPP TS 26.141 sections 4.2 and 4.3. This value cannot be `null`.
`executor` | `Executor`: The `Executor` on which the `pictureToUpload` stream will be read, as well as on which the callback will be called. Callback and listener events are dispatched through this `Executor`, providing an easy way to control which thread is used. To dispatch events through the main thread of your application, you can use `Context.getMainExecutor()`. To dispatch events through a shared thread pool, you can use `AsyncTask#THREAD_POOL_EXECUTOR`. This value cannot be `null`.
`callback` | `OutcomeReceiver`: A callback called when the upload operation terminates, either in success or in error. This value cannot be `null`.

### uploadCallComposerPicture

    public void uploadCallComposerPicture (Path pictureToUpload,
                    String contentType,
                    Executor executor,
                    OutcomeReceiver<ParcelUuid, TelephonyManager.CallComposerException> callback)

Uploads a picture to the carrier network for use with call composer.

Parameters
`pictureToUpload` | `Path`: Path to a local file containing the picture to upload. This value cannot be `null`.
`contentType` | `String`: The MIME type of the picture you're uploading (e.g. image/jpeg) This value cannot be `null`.
`executor` | `Executor`: The `Executor` on which the `pictureToUpload` file will be read from disk, as well as on which `callback` will be called. Callback and listener events are dispatched through this `Executor`, providing an easy way to control which thread is used. To dispatch events through the main thread of your application, you can use `Context.getMainExecutor()`. To dispatch events through a shared thread pool, you can use `AsyncTask#THREAD_POOL_EXECUTOR`. This value cannot be `null`.
`callback` | `OutcomeReceiver`: A callback called when the upload operation terminates, either in success or in error. This value cannot be `null`.

See also:

- `uploadCallComposerPicture(InputStream, String, Executor, OutcomeReceiver)`

Full name *
Email address *
Company / developer name
One of your Play Store app URLs *
Which best describes your business:*
Apps
Games
Apps & Games
*
*