# Print output for @column tags ?>
Developers

- Design
- Develop
- Distribute

Developer Console

## Most visited

## Recently visited

## Results for

Summary: Constants | Inherited Constants | Fields | Ctors | Methods | Inherited Methods

# NetworkCapabilities

`public final class NetworkCapabilities`
`extends Object` `implements Parcelable`

java.lang.Object
↳ | android.net.NetworkCapabilities

Representation of the capabilities of an active network. Instances are typically obtained through `NetworkCallback#onCapabilitiesChanged(Network, NetworkCapabilities)` or `ConnectivityManager#getNetworkCapabilities(Network)`.

This replaces the old `ConnectivityManager#TYPE_MOBILE` method of network selection. Rather than indicate a need for Wi-Fi because an application needs high bandwidth and risk obsolescence when a new, fast network appears (like LTE), the application should specify it needs high bandwidth. Similarly if an application needs an unmetered network for a bulk transfer it can specify that rather than assuming all cellular based connections are metered and all Wi-Fi based connections are not.

## Summary

### Constants
`int` | `NET_CAPABILITY_CAPTIVE_PORTAL` Indicates that this network was found to have a captive portal in place last time it was probed.
`int` | `NET_CAPABILITY_CBS` Indicates this is a network that has the ability to reach the carrier's CBS servers, used for carrier specific services.
`int` | `NET_CAPABILITY_DUN` Indicates this is a network that has the ability to reach the carrier's DUN or tethering gateway.
`int` | `NET_CAPABILITY_EIMS` Indicates this is a network that has the ability to reach a carrier's Emergency IMS servers or other services, used for network signaling during emergency calls.
`int` | `NET_CAPABILITY_ENTERPRISE` Indicates that this network is intended for enterprise use.
`int` | `NET_CAPABILITY_FOREGROUND` Indicates that this network is available for use by apps, and not a network that is being kept up in the background to facilitate fast network switching.
`int` | `NET_CAPABILITY_FOTA` Indicates this is a network that has the ability to reach the carrier's FOTA portal, used for over the air updates.
`int` | `NET_CAPABILITY_HEAD_UNIT` Indicates that this network is connected to an automotive head unit.
`int` | `NET_CAPABILITY_IA` Indicates this is a network that has the ability to reach a carrier's Initial Attach servers.
`int` | `NET_CAPABILITY_IMS` Indicates this is a network that has the ability to reach the carrier's IMS servers, used for network registration and signaling.
`int` | `NET_CAPABILITY_INTERNET` Indicates that this network should be able to reach the internet.
`int` | `NET_CAPABILITY_MCX` Indicates this is a network that has the ability to reach a carrier's Mission Critical servers.
`int` | `NET_CAPABILITY_MMS` Indicates this is a network that has the ability to reach the carrier's MMSC for sending and receiving MMS messages.
`int` | `NET_CAPABILITY_NOT_CONGESTED` Indicates that this network is not congested.
`int` | `NET_CAPABILITY_NOT_METERED` Indicates that this network is unmetered.
`int` | `NET_CAPABILITY_NOT_RESTRICTED` Indicates that this network is available for general use.
`int` | `NET_CAPABILITY_NOT_ROAMING` Indicates that this network is not roaming.
`int` | `NET_CAPABILITY_NOT_SUSPENDED` Indicates that this network is not currently suspended.
`int` | `NET_CAPABILITY_NOT_VPN` Indicates that this network is not a VPN.
`int` | `NET_CAPABILITY_RCS` Indicates this is a network that has the ability to reach a carrier's RCS servers, used for Rich Communication Services.
`int` | `NET_CAPABILITY_SUPL` Indicates this is a network that has the ability to reach the carrier's SUPL server, used to retrieve GPS information.
`int` | `NET_CAPABILITY_TEMPORARILY_NOT_METERED` Indicates that this network is temporarily unmetered.
`int` | `NET_CAPABILITY_TRUSTED` Indicates that the user has indicated implicit trust of this network.
`int` | `NET_CAPABILITY_VALIDATED` Indicates that connectivity on this network was successfully validated.
`int` | `NET_CAPABILITY_WIFI_P2P` Indicates this is a network that has the ability to reach a Wi-Fi direct peer.
`int` | `NET_CAPABILITY_XCAP` Indicates this is a network that has the ability to reach a carrier's XCAP servers, used for configuration and control.
`int` | `SIGNAL_STRENGTH_UNSPECIFIED` Magic value that indicates no signal strength provided.
`int` | `TRANSPORT_BLUETOOTH` Indicates this network uses a Bluetooth transport.
`int` | `TRANSPORT_CELLULAR` Indicates this network uses a Cellular transport.
`int` | `TRANSPORT_ETHERNET` Indicates this network uses an Ethernet transport.
`int` | `TRANSPORT_LOWPAN` Indicates this network uses a LoWPAN transport.
`int` | `TRANSPORT_USB` Indicates this network uses a USB transport.
`int` | `TRANSPORT_VPN` Indicates this network uses a VPN transport.
`int` | `TRANSPORT_WIFI` Indicates this network uses a Wi-Fi transport.
`int` | `TRANSPORT_WIFI_AWARE` Indicates this network uses a Wi-Fi Aware transport.

### Inherited constants
From interface `android.os.Parcelable`
`int` | `CONTENTS_FILE_DESCRIPTOR` Descriptor bit used with `describeContents()`: indicates that the Parcelable object's flattened representation includes a file descriptor.
`int` | `PARCELABLE_WRITE_RETURN_VALUE` Flag for use with `writeToParcel(Parcel, int)`: the object being written is a return value, that is the result of a function such as "`Parcelable someFunction()`", "`void someFunction(out Parcelable)`", or "`void someFunction(inout Parcelable)`".

### Fields
`public static final Creator<NetworkCapabilities>` | `CREATOR`

### Public constructors
`NetworkCapabilities()`
`NetworkCapabilities(NetworkCapabilities nc)`

### Public methods
`int` | `describeContents()` Describe the kinds of special objects contained in this Parcelable instance's marshaled representation.
`boolean` | `equals(Object obj)` Indicates whether some other object is "equal to" this one.
`int[]` | `getCapabilities()` Gets all the capabilities set on this `NetworkCapability` instance.
`int` | `getLinkDownstreamBandwidthKbps()` Retrieves the downstream bandwidth for this network in Kbps.
`int` | `getLinkUpstreamBandwidthKbps()` Retrieves the upstream bandwidth for this network in Kbps.
`NetworkSpecifier` | `getNetworkSpecifier()` Gets the optional bearer specific network specifier.
`int` | `getOwnerUid()` Retrieves the UID of the app that owns this network.
`int` | `getSignalStrength()` Retrieves the signal strength.
`TransportInfo` | `getTransportInfo()` Returns a transport-specific information container.
`boolean` | `hasCapability(int capability)` Tests for the presence of a capability on this instance.
`boolean` | `hasTransport(int transportType)` Tests for the presence of a transport on this instance.
`int` | `hashCode()` Returns a hash code value for the object.
`String` | `toString()` Returns a string representation of the object.
`void` | `writeToParcel(Parcel dest, int flags)` Flatten this object in to a Parcel.

### Inherited methods
From class `java.lang.Object`
`Object` | `clone()` Creates and returns a copy of this object.
`boolean` | `equals(Object obj)` Indicates whether some other object is "equal to" this one.
`void` | `finalize()` Called by the garbage collector on an object when garbage collection determines that there are no more references to the object.
`final Class<?>` | `getClass()` Returns the runtime class of this `Object`.
`int` | `hashCode()` Returns a hash code value for the object.
`final void` | `notify()` Wakes up a single thread that is waiting on this object's monitor.
`final void` | `notifyAll()` Wakes up all threads that are waiting on this object's monitor.
`String` | `toString()` Returns a string representation of the object.
`final void` | `wait(long timeout, int nanos)` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object, or some other thread interrupts the current thread, or a certain amount of real time has elapsed.
`final void` | `wait(long timeout)` Causes the current thread to wait until either another thread invokes the `notify()` method or the `notifyAll()` method for this object, or a specified amount of time has elapsed.
`final void` | `wait()` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object.
From interface `android.os.Parcelable`
`abstract int` | `describeContents()` Describe the kinds of special objects contained in this Parcelable instance's marshaled representation.
`abstract void` | `writeToParcel(Parcel dest, int flags)` Flatten this object in to a Parcel.

## Constants

### NET_CAPABILITY_CAPTIVE_PORTAL

    public static final int NET_CAPABILITY_CAPTIVE_PORTAL

Indicates that this network was found to have a captive portal in place last time it was probed.

Constant Value: 17 (0x00000011)

### NET_CAPABILITY_CBS

    public static final int NET_CAPABILITY_CBS

Indicates this is a network that has the ability to reach the carrier's CBS servers, used for carrier specific services.

Constant Value: 5 (0x00000005)

### NET_CAPABILITY_DUN

    public static final int NET_CAPABILITY_DUN

Indicates this is a network that has the ability to reach the carrier's DUN or tethering gateway.

Constant Value: 2 (0x00000002)

### NET_CAPABILITY_EIMS

    public static final int NET_CAPABILITY_EIMS

Indicates this is a network that has the ability to reach a carrier's Emergency IMS servers or other services, used for network signaling during emergency calls.

Constant Value: 10 (0x0000000a)

### NET_CAPABILITY_ENTERPRISE

    public static final int NET_CAPABILITY_ENTERPRISE

Indicates that this network is intended for enterprise use.

5G URSP rules may indicate that all data should use a connection dedicated for enterprise use. If the enterprise capability is requested, all enterprise traffic will be routed over the connection with this capability.

Constant Value: 29 (0x0000001d)

### NET_CAPABILITY_FOREGROUND

    public static final int NET_CAPABILITY_FOREGROUND

Indicates that this network is available for use by apps, and not a network that is being kept up in the background to facilitate fast network switching.

Constant Value: 19 (0x00000013)

### NET_CAPABILITY_FOTA

    public static final int NET_CAPABILITY_FOTA

Indicates this is a network that has the ability to reach the carrier's FOTA portal, used for over the air updates.

Constant Value: 3 (0x00000003)

### NET_CAPABILITY_HEAD_UNIT

    public static final int NET_CAPABILITY_HEAD_UNIT

Indicates that this network is connected to an automotive head unit.

Constant Value: 32 (0x00000020)

### NET_CAPABILITY_IA

    public static final int NET_CAPABILITY_IA

Indicates this is a network that has the ability to reach a carrier's Initial Attach servers.

Constant Value: 7 (0x00000007)

### NET_CAPABILITY_IMS

    public static final int NET_CAPABILITY_IMS

Indicates this is a network that has the ability to reach the carrier's IMS servers, used for network registration and signaling.

Constant Value: 4 (0x00000004)

### NET_CAPABILITY_INTERNET

    public static final int NET_CAPABILITY_INTERNET

Indicates that this network should be able to reach the internet.

Constant Value: 12 (0x0000000c)

### NET_CAPABILITY_MCX

    public static final int NET_CAPABILITY_MCX

Indicates this is a network that has the ability to reach a carrier's Mission Critical servers.

Constant Value: 23 (0x00000017)

### NET_CAPABILITY_MMS

    public static final int NET_CAPABILITY_MMS

Indicates this is a network that has the ability to reach the carrier's MMSC for sending and receiving MMS messages.

Constant Value: 0 (0x00000000)

### NET_CAPABILITY_NOT_CONGESTED

    public static final int NET_CAPABILITY_NOT_CONGESTED

Indicates that this network is not congested.

When a network is congested, applications should defer network traffic that can be done at a later time, such as uploading analytics.

Constant Value: 20 (0x00000014)

### NET_CAPABILITY_NOT_METERED

    public static final int NET_CAPABILITY_NOT_METERED

Indicates that this network is unmetered.

Constant Value: 11 (0x0000000b)

### NET_CAPABILITY_NOT_RESTRICTED

    public static final int NET_CAPABILITY_NOT_RESTRICTED

Indicates that this network is available for general use. If this is not set applications should not attempt to communicate on this network. Note that this is simply informative and not enforcement - enforcement is handled via other means. Set by default.

Constant Value: 13 (0x0000000d)

### NET_CAPABILITY_NOT_ROAMING

    public static final int NET_CAPABILITY_NOT_ROAMING

Indicates that this network is not roaming.

Constant Value: 18 (0x00000012)

### NET_CAPABILITY_NOT_SUSPENDED

    public static final int NET_CAPABILITY_NOT_SUSPENDED

Indicates that this network is not currently suspended.

When a network is suspended, the network's IP addresses and any connections established on the network remain valid, but the network is temporarily unable to transfer data. This can happen, for example, if a cellular network experiences a temporary loss of signal, such as when driving through a tunnel, etc. A network with this capability is not suspended, so is expected to be able to transfer data.

Constant Value: 21 (0x00000015)

### NET_CAPABILITY_NOT_VPN

    public static final int NET_CAPABILITY_NOT_VPN

Indicates that this network is not a VPN. This capability is set by default and should be explicitly cleared for VPN networks.

Constant Value: 15 (0x0000000f)

### NET_CAPABILITY_RCS

    public static final int NET_CAPABILITY_RCS

Indicates this is a network that has the ability to reach a carrier's RCS servers, used for Rich Communication Services.

Constant Value: 8 (0x00000008)

### NET_CAPABILITY_SUPL

    public static final int NET_CAPABILITY_SUPL

Indicates this is a network that has the ability to reach the carrier's SUPL server, used to retrieve GPS information.

Constant Value: 1 (0x00000001)

### NET_CAPABILITY_TEMPORARILY_NOT_METERED

    public static final int NET_CAPABILITY_TEMPORARILY_NOT_METERED

Indicates that this network is temporarily unmetered.

This capability will be set for networks that are generally metered, but are currently unmetered, e.g., because the user is in a particular area. This capability can be changed at any time. When it is removed, applications are responsible for stopping any data transfer that should not occur on a metered network. Note that most apps should use `NET_CAPABILITY_NOT_METERED` instead. For more information, see https://developer.android.com/about/versions/11/features/5g#meteredness.

Constant Value: 25 (0x00000019)

### NET_CAPABILITY_TRUSTED

    public static final int NET_CAPABILITY_TRUSTED

Indicates that the user has indicated implicit trust of this network. This generally means it's a sim-selected carrier, a plugged in ethernet, a paired BT device or a wifi the user asked to connect to. Untrusted networks are probably limited to unknown wifi AP. Set by default.

Constant Value: 14 (0x0000000e)

### NET_CAPABILITY_VALIDATED

    public static final int NET_CAPABILITY_VALIDATED

Indicates that connectivity on this network was successfully validated. For example, for a network with NET_CAPABILITY_INTERNET, it means that Internet connectivity was successfully detected.

Constant Value: 16 (0x00000010)

### NET_CAPABILITY_WIFI_P2P

    public static final int NET_CAPABILITY_WIFI_P2P

Indicates this is a network that has the ability to reach a Wi-Fi direct peer.

Constant Value: 6 (0x00000006)

### NET_CAPABILITY_XCAP

    public static final int NET_CAPABILITY_XCAP

Indicates this is a network that has the ability to reach a carrier's XCAP servers, used for configuration and control.

Constant Value: 9 (0x00000009)

### SIGNAL_STRENGTH_UNSPECIFIED

    public static final int SIGNAL_STRENGTH_UNSPECIFIED

Magic value that indicates no signal strength provided. A request specifying this value is always satisfied.

Constant Value: -2147483648 (0x80000000)

### TRANSPORT_BLUETOOTH

    public static final int TRANSPORT_BLUETOOTH

Indicates this network uses a Bluetooth transport.

Constant Value: 2 (0x00000002)

### TRANSPORT_CELLULAR

    public static final int TRANSPORT_CELLULAR

Indicates this network uses a Cellular transport.

Constant Value: 0 (0x00000000)

### TRANSPORT_ETHERNET

    public static final int TRANSPORT_ETHERNET

Indicates this network uses an Ethernet transport.

Constant Value: 3 (0x00000003)

### TRANSPORT_LOWPAN

    public static final int TRANSPORT_LOWPAN

Indicates this network uses a LoWPAN transport.

Constant Value: 6 (0x00000006)

### TRANSPORT_USB

    public static final int TRANSPORT_USB

Indicates this network uses a USB transport.

Constant Value: 8 (0x00000008)

### TRANSPORT_VPN

    public static final int TRANSPORT_VPN

Indicates this network uses a VPN transport.

Constant Value: 4 (0x00000004)

### TRANSPORT_WIFI

    public static final int TRANSPORT_WIFI

Indicates this network uses a Wi-Fi transport.

Constant Value: 1 (0x00000001)

### TRANSPORT_WIFI_AWARE

    public static final int TRANSPORT_WIFI_AWARE

Indicates this network uses a Wi-Fi Aware transport.

Constant Value: 5 (0x00000005)

## Fields

### CREATOR

    public static final Creator<NetworkCapabilities> CREATOR

## Public constructors

### NetworkCapabilities

    public NetworkCapabilities ()

### NetworkCapabilities

    public NetworkCapabilities (NetworkCapabilities nc)

Parameters
`nc` | `NetworkCapabilities`

## Public methods

### describeContents

    public int describeContents ()

Describe the kinds of special objects contained in this Parcelable instance's marshaled representation. For example, if the object will include a file descriptor in the output of `writeToParcel(android.os.Parcel, int)`, the return value of this method must include the `CONTENTS_FILE_DESCRIPTOR` bit.

Returns
`int` | a bitmask indicating the set of special object types marshaled by this Parcelable object instance. Value is either `0` or `CONTENTS_FILE_DESCRIPTOR`

### equals

    public boolean equals (Object obj)

Indicates whether some other object is "equal to" this one.

The `equals` method implements an equivalence relation on non-null object references:

- It is reflexive: for any non-null reference value `x`, `x.equals(x)` should return `true`.
- It is symmetric: for any non-null reference values `x` and `y`, `x.equals(y)` should return `true` if and only if `y.equals(x)` returns `true`.
- It is transitive: for any non-null reference values `x`, `y`, and `z`, if `x.equals(y)` returns `true` and `y.equals(z)` returns `true`, then `x.equals(z)` should return `true`.
- It is consistent: for any non-null reference values `x` and `y`, multiple invocations of `x.equals(y)` consistently return `true` or consistently return `false`, provided no information used in `equals` comparisons on the objects is modified.
- For any non-null reference value `x`, `x.equals(null)` should return `false`.

The `equals` method for class `Object` implements the most discriminating possible equivalence relation on objects; that is, for any non-null reference values `x` and `y`, this method returns `true` if and only if `x` and `y` refer to the same object (`x == y` has the value `true`).

Note that it is generally necessary to override the `hashCode` method whenever this method is overridden, so as to maintain the general contract for the `hashCode` method, which states that equal objects must have equal hash codes.

Parameters
`obj` | `Object`: This value may be `null`.

Returns
`boolean` | `true` if this object is the same as the obj argument; `false` otherwise.

### getCapabilities

    public int[] getCapabilities ()

Gets all the capabilities set on this `NetworkCapability` instance.

Returns
`int[]` | an array of capability values for this instance. This value cannot be `null`. Value is `NET_CAPABILITY_MMS`, `NET_CAPABILITY_SUPL`, `NET_CAPABILITY_DUN`, `NET_CAPABILITY_FOTA`, `NET_CAPABILITY_IMS`, `NET_CAPABILITY_CBS`, `NET_CAPABILITY_WIFI_P2P`, `NET_CAPABILITY_IA`, `NET_CAPABILITY_RCS`, `NET_CAPABILITY_XCAP`, `NET_CAPABILITY_EIMS`, `NET_CAPABILITY_NOT_METERED`, `NET_CAPABILITY_INTERNET`, `NET_CAPABILITY_NOT_RESTRICTED`, `NET_CAPABILITY_TRUSTED`, `NET_CAPABILITY_NOT_VPN`, `NET_CAPABILITY_VALIDATED`, `NET_CAPABILITY_CAPTIVE_PORTAL`, `NET_CAPABILITY_NOT_ROAMING`, `NET_CAPABILITY_FOREGROUND`, `NET_CAPABILITY_NOT_CONGESTED`, `NET_CAPABILITY_NOT_SUSPENDED`, android.net.NetworkCapabilities.NET_CAPABILITY_OEM_PAID, `NET_CAPABILITY_MCX`, android.net.NetworkCapabilities.NET_CAPABILITY_PARTIAL_CONNECTIVITY, `NET_CAPABILITY_TEMPORARILY_NOT_METERED`, android.net.NetworkCapabilities.NET_CAPABILITY_OEM_PRIVATE, android.net.NetworkCapabilities.NET_CAPABILITY_VEHICLE_INTERNAL, android.net.NetworkCapabilities.NET_CAPABILITY_NOT_VCN_MANAGED, `NET_CAPABILITY_ENTERPRISE`, android.net.NetworkCapabilities.NET_CAPABILITY_VSIM, android.net.NetworkCapabilities.NET_CAPABILITY_BIP, or `NET_CAPABILITY_HEAD_UNIT`

### getLinkDownstreamBandwidthKbps

    public int getLinkDownstreamBandwidthKbps ()

Retrieves the downstream bandwidth for this network in Kbps. This always only refers to the estimated first hop transport bandwidth.

Returns
`int` | The estimated first hop downstream (network to device) bandwidth.

### getLinkUpstreamBandwidthKbps

    public int getLinkUpstreamBandwidthKbps ()

Retrieves the upstream bandwidth for this network in Kbps. This always only refers to the estimated first hop transport bandwidth.

Returns
`int` | The estimated first hop upstream (device to network) bandwidth.

### getNetworkSpecifier

    public NetworkSpecifier getNetworkSpecifier ()

Gets the optional bearer specific network specifier. May be `null` if not set.

Returns
`NetworkSpecifier` | The optional `NetworkSpecifier` specifying the bearer specific network specifier or `null`.

### getOwnerUid

    public int getOwnerUid ()

Retrieves the UID of the app that owns this network.

For user privacy reasons, this field will only be populated if the following conditions are met:

The caller is the network owner, AND one of the following sets of requirements is met:

1. The described Network is a VPN

OR:

1. The calling app is the network owner
2. The calling app has the ACCESS_FINE_LOCATION permission granted
3. The user's location toggle is on

Instances of NetworkCapabilities sent to apps without the appropriate permissions will have this field cleared out.

This field will only be populated for VPN and wifi network suggestor apps (i.e using `WifiNetworkSuggestion`), and only for the network they own. In the case of wifi network suggestors apps, this field is also location sensitive, so the app needs to hold `Manifest.permission.ACCESS_FINE_LOCATION` permission. If the app targets SDK version greater than or equal to `Build.VERSION_CODES#S`, then they also need to use `NetworkCallback#FLAG_INCLUDE_LOCATION_INFO` to get the info in their callback. If the apps targets SDK version equal to {`Build.VERSION_CODES#R`, this field will always be included. The app will be blamed for location access if this field is included.

Returns
`int` |

### getSignalStrength

    public int getSignalStrength ()

Retrieves the signal strength.

Returns
`int` | The bearer-specific signal strength.

### getTransportInfo

    public TransportInfo getTransportInfo ()

Returns a transport-specific information container. The application may cast this container to a concrete sub-class based on its knowledge of the network request. The application should be able to deal with a `null` return value or an invalid case, e.g. use `instanceof` operator to verify expected type.

Returns
`TransportInfo` | A concrete implementation of the `TransportInfo` class or null if not available for the network.

### hasCapability

    public boolean hasCapability (int capability)

Tests for the presence of a capability on this instance.

Parameters
`capability` | `int`: the capabilities to be tested for. Value is `NET_CAPABILITY_MMS`, `NET_CAPABILITY_SUPL`, `NET_CAPABILITY_DUN`, `NET_CAPABILITY_FOTA`, `NET_CAPABILITY_IMS`, `NET_CAPABILITY_CBS`, `NET_CAPABILITY_WIFI_P2P`, `NET_CAPABILITY_IA`, `NET_CAPABILITY_RCS`, `NET_CAPABILITY_XCAP`, `NET_CAPABILITY_EIMS`, `NET_CAPABILITY_NOT_METERED`, `NET_CAPABILITY_INTERNET`, `NET_CAPABILITY_NOT_RESTRICTED`, `NET_CAPABILITY_TRUSTED`, `NET_CAPABILITY_NOT_VPN`, `NET_CAPABILITY_VALIDATED`, `NET_CAPABILITY_CAPTIVE_PORTAL`, `NET_CAPABILITY_NOT_ROAMING`, `NET_CAPABILITY_FOREGROUND`, `NET_CAPABILITY_NOT_CONGESTED`, `NET_CAPABILITY_NOT_SUSPENDED`, android.net.NetworkCapabilities.NET_CAPABILITY_OEM_PAID, `NET_CAPABILITY_MCX`, android.net.NetworkCapabilities.NET_CAPABILITY_PARTIAL_CONNECTIVITY, `NET_CAPABILITY_TEMPORARILY_NOT_METERED`, android.net.NetworkCapabilities.NET_CAPABILITY_OEM_PRIVATE, android.net.NetworkCapabilities.NET_CAPABILITY_VEHICLE_INTERNAL, android.net.NetworkCapabilities.NET_CAPABILITY_NOT_VCN_MANAGED, `NET_CAPABILITY_ENTERPRISE`, android.net.NetworkCapabilities.NET_CAPABILITY_VSIM, android.net.NetworkCapabilities.NET_CAPABILITY_BIP, or `NET_CAPABILITY_HEAD_UNIT`

Returns
`boolean` | `true` if set on this instance.

### hasTransport

    public boolean hasTransport (int transportType)

Tests for the presence of a transport on this instance.

Parameters
`transportType` | `int`: the transport type to be tested for. Value is `TRANSPORT_CELLULAR`, `TRANSPORT_WIFI`, `TRANSPORT_BLUETOOTH`, `TRANSPORT_ETHERNET`, `TRANSPORT_VPN`, `TRANSPORT_WIFI_AWARE`, `TRANSPORT_LOWPAN`, android.net.NetworkCapabilities.TRANSPORT_TEST, or `TRANSPORT_USB`

Returns
`boolean` | `true` if set on this instance.

### hashCode

    public int hashCode ()

Returns a hash code value for the object. This method is supported for the benefit of hash tables such as those provided by `HashMap`.

The general contract of `hashCode` is:

- Whenever it is invoked on the same object more than once during an execution of a Java application, the `hashCode` method must consistently return the same integer, provided no information used in `equals` comparisons on the object is modified. This integer need not remain consistent from one execution of an application to another execution of the same application.
- If two objects are equal according to the `equals(Object)` method, then calling the `hashCode` method on each of the two objects must produce the same integer result.
- It is not required that if two objects are unequal according to the `equals(java.lang.Object)` method, then calling the `hashCode` method on each of the two objects must produce distinct integer results. However, the programmer should be aware that producing distinct integer results for unequal objects may improve the performance of hash tables.

As much as is reasonably practical, the hashCode method defined by class `Object` does return distinct integers for distinct objects. (This is typically implemented by converting the internal address of the object into an integer, but this implementation technique is not required by the Java™ programming language.)

Returns
`int` | a hash code value for this object.

### toString

    public String toString ()

Returns a string representation of the object. In general, the `toString` method returns a string that "textually represents" this object. The result should be a concise but informative representation that is easy for a person to read. It is recommended that all subclasses override this method.

The `toString` method for class `Object` returns a string consisting of the name of the class of which the object is an instance, the at-sign character ``@`', and the unsigned hexadecimal representation of the hash code of the object. In other words, this method returns a string equal to the value of:

>      getClass().getName() + '@' + Integer.toHexString(hashCode())

Returns
`String` | This value cannot be `null`.

### writeToParcel

    public void writeToParcel (Parcel dest,
                    int flags)

Flatten this object in to a Parcel.

Parameters
`dest` | `Parcel`: The Parcel in which the object should be written.
`flags` | `int`: Additional flags about how the object should be written. May be 0 or `Parcelable.PARCELABLE_WRITE_RETURN_VALUE`. Value is either `0` or a combination of `Parcelable.PARCELABLE_WRITE_RETURN_VALUE`, and android.os.Parcelable.PARCELABLE_ELIDE_DUPLICATES

Full name *
Email address *
Company / developer name
One of your Play Store app URLs *
Which best describes your business:*
Apps
Games
Apps & Games
*
*