# Print output for @column tags ?>
Developers

- Design
- Develop
- Distribute

Developer Console

## Most visited

## Recently visited

## Results for

Summary: Constants | Inherited Methods

# DataFailCause

`public final class DataFailCause`
`extends Object` ``

java.lang.Object
↳ | android.telephony.DataFailCause

DataFailCause collects data connection failure causes code from different sources.

## Summary

### Constants
`int` | `ACCESS_ATTEMPT_ALREADY_IN_PROGRESS` Access attempt is already in progress.
`int` | `ACCESS_BLOCK` Access blocked by the base station.
`int` | `ACCESS_BLOCK_ALL` Access blocked by the base station for all mobile devices.
`int` | `ACCESS_CLASS_DSAC_REJECTION` Access class blocking restrictions for the current camped cell.
`int` | `ACCESS_CONTROL_LIST_CHECK_FAILURE` Access control list check failure at the lower layer.
`int` | `ACTIVATION_REJECTED_BCM_VIOLATION` UE requested to modify QoS parameters or the bearer control mode, which is not compatible with the selected bearer control mode.
`int` | `ACTIVATION_REJECT_GGSN` Activation rejected by Gateway GPRS Support Node (GGSN), Serving Gateway or PDN Gateway.
`int` | `ACTIVATION_REJECT_UNSPECIFIED` Activation rejected, unspecified.
`int` | `ACTIVE_PDP_CONTEXT_MAX_NUMBER_REACHED` Max number of Packet Data Protocol (PDP) context reached.
`int` | `ALL_MATCHING_RULES_FAILED` If connection failed for all matching URSP rules.
`int` | `APN_DISABLED` APN has been disabled.
`int` | `APN_DISALLOWED_ON_ROAMING` PDN connection to the APN is disallowed on the roaming network.
`int` | `APN_MISMATCH` New PDN bring up is rejected during interface selection because the UE has already allotted the available interfaces for other PDNs.
`int` | `APN_PARAMETERS_CHANGED` APN-related parameters are changed.
`int` | `APN_PENDING_HANDOVER` Interface bring up is attempted for an APN that is yet to be handed over to target RAT.
`int` | `APN_TYPE_CONFLICT` APN type conflict.
`int` | `AUTH_FAILURE_ON_EMERGENCY_CALL` Authentication failure on emergency call.
`int` | `BEARER_HANDLING_NOT_SUPPORTED` Procedure requested by the UE was rejected because the bearer handling is not supported.
`int` | `CALL_DISALLOWED_IN_ROAMING` Roaming is disallowed during call bring up.
`int` | `CALL_PREEMPT_BY_EMERGENCY_APN` Emergency call bring up on a different ePDG.
`int` | `CANNOT_ENCODE_OTA_MESSAGE` Unable to encode the OTA message for MT PDP or deactivate PDP.
`int` | `CDMA_ALERT_STOP` Received an alert stop from the base station due to incoming only.
`int` | `CDMA_INCOMING_CALL` Receiving an incoming call from the base station.
`int` | `CDMA_INTERCEPT` Received an intercept order from the base station.
`int` | `CDMA_LOCK` Device in CDMA locked state.
`int` | `CDMA_RELEASE_DUE_TO_SO_REJECTION` Receiving a release from the base station with a SO (Service Option) Reject reason.
`int` | `CDMA_REORDER` Receiving a reorder from the base station.
`int` | `CDMA_RETRY_ORDER` Receiving a retry order from the base station.
`int` | `CHANNEL_ACQUISITION_FAILURE` Channel acquisition failures.
`int` | `CLOSE_IN_PROGRESS` Tearing down is in progress.
`int` | `COLLISION_WITH_NETWORK_INITIATED_REQUEST` Network has already initiated the activation, modification, or deactivation of bearer resources that was requested by the UE.
`int` | `COMPANION_IFACE_IN_USE` Companion interface in use.
`int` | `CONCURRENT_SERVICES_INCOMPATIBLE` The concurrent services requested were not compatible.
`int` | `CONCURRENT_SERVICES_NOT_ALLOWED` In favor of a voice call or SMS when concurrent voice and data are not supported.
`int` | `CONCURRENT_SERVICE_NOT_SUPPORTED_BY_BASE_STATION` Concurrent service is not supported by base station.
`int` | `CONDITIONAL_IE_ERROR` Conditional Information Element (IE) error.
`int` | `CONGESTION` Network cannot serve a request from the MS due to congestion.
`int` | `CONNECTION_RELEASED` Indicate the connection was released.
`int` | `CS_DOMAIN_NOT_AVAILABLE` CS domain is not available.
`int` | `CS_FALLBACK_CALL_ESTABLISHMENT_NOT_ALLOWED` CS fallback call establishment is not allowed.
`int` | `DATA_PLAN_EXPIRED` Network initiates a detach on LTE with error cause ""data plan has been replenished or has expired.
`int` | `DATA_ROAMING_SETTINGS_DISABLED` PDN Connection to a given APN is disallowed because data roaming is disabled from the device user interface settings and the UE is roaming.
`int` | `DATA_SETTINGS_DISABLED` PDN Connection to a given APN is disallowed because data is disabled from the device user interface settings.
`int` | `DBM_OR_SMS_IN_PROGRESS` DBM or SMS is in progress.
`int` | `DDS_SWITCHED` DDS (Default data subscription) switch occurs.
`int` | `DDS_SWITCH_IN_PROGRESS` Default data subscription switch is in progress.
`int` | `DRB_RELEASED_BY_RRC` Data radio bearer is released by the RRC.
`int` | `DS_EXPLICIT_DEACTIVATION` Dedicated bearer will be deactivated regardless of the network response.
`int` | `DUAL_SWITCH` Dual switch from single standby to dual standby is in progress.
`int` | `DUN_CALL_DISALLOWED` Dial up networking (DUN) call bring up is rejected since UE is in eHRPD RAT.
`int` | `DUPLICATE_BEARER_ID` Active dedicated bearer was requested using the same default bearer ID.
`int` | `EHRPD_TO_HRPD_FALLBACK` Device falls back from eHRPD to HRPD.
`int` | `EMBMS_NOT_ENABLED` Data call has been brought down because EMBMS is not enabled at the RRC layer.
`int` | `EMBMS_REGULAR_DEACTIVATION` EMBMS data call has been successfully brought down.
`int` | `EMERGENCY_IFACE_ONLY` Emergency interface only.
`int` | `EMERGENCY_MODE` Device is operating in Emergency mode.
`int` | `EMM_ACCESS_BARRED` EPS (Evolved Packet System) Mobility Management (EMM) access barred.
`int` | `EMM_ACCESS_BARRED_INFINITE_RETRY` EPS (Evolved Packet System) Mobility Management (EMM) access barred infinity retry.
`int` | `EMM_ATTACH_FAILED` Attach procedure is rejected by the network.
`int` | `EMM_ATTACH_STARTED` Attach procedure is started for EMC purposes.
`int` | `EMM_DETACHED` UE is detached.
`int` | `EMM_T3417_EXPIRED` T3417 timer expiration of the service request procedure.
`int` | `EMM_T3417_EXT_EXPIRED` Extended service request fails due to expiration of the T3417 EXT timer.
`int` | `EPS_SERVICES_AND_NON_EPS_SERVICES_NOT_ALLOWED` EPS and non-EPS services are not allowed by the network.
`int` | `EPS_SERVICES_NOT_ALLOWED_IN_PLMN` EPS services are not allowed in the PLMN.
`int` | `ERROR_UNSPECIFIED` Data call fail due to unspecific errors.
`int` | `ESM_BAD_OTA_MESSAGE` Bad OTA message is received from the network.
`int` | `ESM_BEARER_DEACTIVATED_TO_SYNC_WITH_NETWORK` Bearer must be deactivated to synchronize with the network.
`int` | `ESM_COLLISION_SCENARIOS` Collision scenarios for the UE and network-initiated procedures.
`int` | `ESM_CONTEXT_TRANSFERRED_DUE_TO_IRAT` PDN was disconnected by the downlaod server due to IRAT.
`int` | `ESM_DOWNLOAD_SERVER_REJECTED_THE_CALL` Download server rejected the call.
`int` | `ESM_FAILURE` ESM level failure.
`int` | `ESM_INFO_NOT_RECEIVED` EPS Session Management (ESM) information is not received.
`int` | `ESM_LOCAL_CAUSE_NONE` No specific local cause is mentioned, usually a valid OTA cause.
`int` | `ESM_NW_ACTIVATED_DED_BEARER_WITH_ID_OF_DEF_BEARER` Active dedicated bearer was requested for an existing default bearer.
`int` | `ESM_PROCEDURE_TIME_OUT` ESM procedure maximum attempt timeout failure.
`int` | `ESM_UNKNOWN_EPS_BEARER_CONTEXT` Invalid EPS bearer identity in the request.
`int` | `EVDO_CONNECTION_DENY_BY_BILLING_OR_AUTHENTICATION_FAILURE` Received a connection deny due to billing or authentication failure on EVDO network.
`int` | `EVDO_CONNECTION_DENY_BY_GENERAL_OR_NETWORK_BUSY` Received a connection deny due to general or network busy on EVDO network.
`int` | `EVDO_HDR_CHANGED` HDR system has been changed due to redirection or the PRL was not preferred.
`int` | `EVDO_HDR_CONNECTION_SETUP_TIMEOUT` Connection setup on the HDR system was time out.
`int` | `EVDO_HDR_EXITED` Device exited HDR due to redirection or the PRL was not preferred.
`int` | `EVDO_HDR_NO_SESSION` Device does not have an HDR session.
`int` | `EVDO_USING_GPS_FIX_INSTEAD_OF_HDR_CALL` It is ending an HDR call origination in favor of a GPS fix.
`int` | `FADE` Device lost the system due to fade.
`int` | `FAILED_TO_ACQUIRE_COLOCATED_HDR` Device failed to acquire a co-located HDR for origination.
`int` | `FEATURE_NOT_SUPP` Feature not supported.
`int` | `FILTER_SEMANTIC_ERROR` Semantic errors in packet filter.
`int` | `FILTER_SYTAX_ERROR` Syntactical errors in packet filter(s).
`int` | `FORBIDDEN_APN_NAME` PDN being brought up with an APN that is part of forbidden APN Name list.
`int` | `GPRS_REGISTRATION_FAIL` Data fail due to GPRS registration failure.
`int` | `GPRS_SERVICES_AND_NON_GPRS_SERVICES_NOT_ALLOWED` Not allowed to operate either GPRS or non-GPRS services.
`int` | `GPRS_SERVICES_NOT_ALLOWED` MS is not allowed to operate GPRS services.
`int` | `GPRS_SERVICES_NOT_ALLOWED_IN_THIS_PLMN` UE requests GPRS service or the network initiates a detach request in a PLMN that does not offer roaming for GPRS services.
`int` | `HANDOFF_PREFERENCE_CHANGED` System preference change back to SRAT during handoff
`int` | `HDR_ACCESS_FAILURE` HDR system access failure.
`int` | `HDR_FADE` HDR module released the call due to fade.
`int` | `HDR_NO_LOCK_GRANTED` HDR module could not be obtained because of the RF locked.
`int` | `IFACE_AND_POL_FAMILY_MISMATCH`
`int` | `IFACE_MISMATCH` Interface mismatch.
`int` | `ILLEGAL_ME` ME could not be authenticated and the ME used is not acceptable to the network.
`int` | `ILLEGAL_MS` Network refuses service to the MS because either an identity of the MS is not acceptable to the network or the MS does not pass the authentication check.
`int` | `IMEI_NOT_ACCEPTED` IMEI of the UE is not accepted by the network.
`int` | `IMPLICITLY_DETACHED` Mobile reachable timer has expired, or the GMM context data related to the subscription does not exist in the SGSN.
`int` | `IMSI_UNKNOWN_IN_HOME_SUBSCRIBER_SERVER` IMSI present in the UE is unknown in the home subscriber server.
`int` | `INCOMING_CALL_REJECTED` The other clients rejected incoming call.
`int` | `INSUFFICIENT_RESOURCES` Insufficient resources.
`int` | `INTERFACE_IN_USE` The current interface is being in use.
`int` | `INTERNAL_CALL_PREEMPT_BY_HIGH_PRIO_APN` Internal data call preempt by high priority APN.
`int` | `INTERNAL_EPC_NONEPC_TRANSITION` Rejected/Brought down since UE is transition between EPC and NONEPC RAT.
`int` | `INVALID_CONNECTION_ID` No PDP exists with the given connection ID while modifying or deactivating or activation for an already active PDP.
`int` | `INVALID_DNS_ADDR` Not receiving a DNS address that was mandatory.
`int` | `INVALID_EMM_STATE` Invalid EMM state.
`int` | `INVALID_MANDATORY_INFO` Invalid mandatory information.
`int` | `INVALID_MODE` Device operational mode is different from the mode requested in the traffic channel bring up.
`int` | `INVALID_PCSCF_ADDR` Invalid Proxy-Call Session Control Function (P-CSCF) address.
`int` | `INVALID_PCSCF_OR_DNS_ADDRESS` Not receiving either a PCSCF or a DNS address, one of them being mandatory.
`int` | `INVALID_PRIMARY_NSAPI` Primary context for NSAPI does not exist.
`int` | `INVALID_SIM_STATE` SIM was marked by the network as invalid for the circuit and/or packet service domain.
`int` | `INVALID_TRANSACTION_ID` Invalid transaction id.
`int` | `IPV6_ADDRESS_TRANSFER_FAILED` IPv6 address transfer failed.
`int` | `IPV6_PREFIX_UNAVAILABLE` Device failure to obtain the prefix from the network.
`int` | `IP_ADDRESS_MISMATCH` IP address mismatch.
`int` | `IP_VERSION_MISMATCH` New call bring up is rejected since the existing data call IP type doesn't match the requested IP.
`int` | `IRAT_HANDOVER_FAILED` Data call was unsuccessfully transferred during the IRAT handover.
`int` | `IS707B_MAX_ACCESS_PROBES` Maximum access probes for the IS-707B call.
`int` | `IWLAN_AUTHORIZATION_REJECTED` The user is barred from using the non-3GPP access or the subscribed APN.
`int` | `IWLAN_DNS_RESOLUTION_NAME_FAILURE` Unable to resolve FQDN for the ePDG to an IP address
`int` | `IWLAN_DNS_RESOLUTION_TIMEOUT` No response received from the DNS Server due to a timeout
`int` | `IWLAN_IKEV2_AUTH_FAILURE` Sent in the response to an IKE_AUTH message when, for some reason, the authentication failed.
`int` | `IWLAN_IKEV2_CERT_INVALID` IKE Certification validation failure
`int` | `IWLAN_IKEV2_CONFIG_FAILURE` IKE configuration error resulting in failure
`int` | `IWLAN_IKEV2_MSG_TIMEOUT` IKE message timeout, tunnel setup failed due to no response from EPDG
`int` | `IWLAN_ILLEGAL_ME` The Mobile Equipment used is not acceptable to the network
`int` | `IWLAN_IMEI_NOT_ACCEPTED` The network does not accept emergency PDN bringup request using an IMEI
`int` | `IWLAN_MAX_CONNECTION_REACHED` The PDN connection has been rejected.
`int` | `IWLAN_NETWORK_FAILURE` The network has determined that the requested procedure cannot be completed successfully due to network failure.
`int` | `IWLAN_NON_3GPP_ACCESS_TO_EPC_NOT_ALLOWED` No non-3GPP subscription is associated with the IMSI.
`int` | `IWLAN_NO_APN_SUBSCRIPTION` The requested APN is not included in the user's profile, and therefore is not authorized for that user.
`int` | `IWLAN_PDN_CONNECTION_REJECTION` The PDN connection corresponding to the requested APN has been rejected.
`int` | `IWLAN_PLMN_NOT_ALLOWED` The ePDG performs PLMN filtering (based on roaming agreements) and rejects the request from the UE.
`int` | `IWLAN_RAT_TYPE_NOT_ALLOWED` The access type is restricted to the user.
`int` | `IWLAN_SEMANTIC_ERRORS_IN_PACKET_FILTERS` The PDN connection has been rejected due to sematic errors in the packet filter.
`int` | `IWLAN_SEMANTIC_ERROR_IN_THE_TFT_OPERATION` The PDN connection has been rejected due to a semantic error in TFT operation.
`int` | `IWLAN_SYNTACTICAL_ERRORS_IN_PACKET_FILTERS` The PDN connection has been rejected due to syntactic errors in the packet filter.
`int` | `IWLAN_SYNTACTICAL_ERROR_IN_THE_TFT_OPERATION` The PDN connection has been rejected due to a syntactic error in TFT operation.
`int` | `IWLAN_UNAUTHENTICATED_EMERGENCY_NOT_SUPPORTED` The ePDG does not support un-authenticated IMSI based emergency PDN bringup *
`int` | `IWLAN_USER_UNKNOWN` The user identified by the IMSI is unknown.
`int` | `LIMITED_TO_IPV4` IPv6 interface bring up fails because the network provided only the IPv4 address for the upcoming PDN permanent client can reattempt a IPv6 call bring up after the IPv4 interface is also brought down.
`int` | `LIMITED_TO_IPV6` IPv4 interface bring up fails because the network provided only the IPv6 address for the upcoming PDN permanent client can reattempt a IPv4 call bring up after the IPv6 interface is also brought down.
`int` | `LLC_SNDCP` Logical Link Control (LLC) Sub Network Dependent Convergence Protocol (SNDCP).
`int` | `LOCAL_END` Client ended the data call.
`int` | `LOCATION_AREA_NOT_ALLOWED` MS requests service, or the network initiates a detach request, in a location area where the HPLMN determines that the MS, by subscription, is not allowed to operate.
`int` | `LOST_CONNECTION` Data connection was lost.
`int` | `LOWER_LAYER_REGISTRATION_FAILURE` Lower layer registration failure.
`int` | `LOW_POWER_MODE_OR_POWERING_DOWN` Device is going into lower power mode or powering down.
`int` | `LTE_NAS_SERVICE_REQUEST_FAILED` Service request procedure failure.
`int` | `LTE_THROTTLING_NOT_REQUIRED` Throttling is not needed for this service request failure.
`int` | `MAC_FAILURE` MAC level failure.
`int` | `MATCH_ALL_RULE_NOT_ALLOWED` No matching rule available for the request, and match-all rule is not allowed for it.
`int` | `MAXIMIUM_NSAPIS_EXCEEDED` Maximum NSAPIs have been exceeded during PDP activation.
`int` | `MAXINUM_SIZE_OF_L2_MESSAGE_EXCEEDED` Maximum size of the L2 message was exceeded.
`int` | `MAX_ACCESS_PROBE` Maximum access probes transmitted.
`int` | `MAX_IPV4_CONNECTIONS` IPv4 data call bring up is rejected because the UE already maintains the allotted maximum number of IPv4 data connections.
`int` | `MAX_IPV6_CONNECTIONS` IPv6 data call bring up is rejected because the UE already maintains the allotted maximum number of IPv6 data connections.
`int` | `MAX_PPP_INACTIVITY_TIMER_EXPIRED` Maximum PPP inactivity timer expired.
`int` | `MESSAGE_INCORRECT_SEMANTIC` Incorrect message semantic.
`int` | `MESSAGE_TYPE_UNSUPPORTED` Unsupported message type.
`int` | `MIP_CONFIG_FAILURE` UE is in MIP-only configuration but the MIP configuration fails on call bring up due to incorrect provisioning.
`int` | `MIP_FA_ADMIN_PROHIBITED` Foreign agent administratively prohibited MIP (Mobile IP) registration.
`int` | `MIP_FA_DELIVERY_STYLE_NOT_SUPPORTED` Foreign agent rejected MIP (Mobile IP) registration because of delivery style was not supported.
`int` | `MIP_FA_ENCAPSULATION_UNAVAILABLE` Foreign agent rejected MIP (Mobile IP) registration because of requested encapsulation was unavailable.
`int` | `MIP_FA_HOME_AGENT_AUTHENTICATION_FAILURE` Foreign agent rejected MIP (Mobile IP) registration because of home agent authentication failure.
`int` | `MIP_FA_INSUFFICIENT_RESOURCES` Foreign agent rejected MIP (Mobile IP) registration because of insufficient resources.
`int` | `MIP_FA_MALFORMED_REPLY` Foreign agent rejected MIP (Mobile IP) registration because of malformed reply.
`int` | `MIP_FA_MALFORMED_REQUEST` Foreign agent rejected MIP (Mobile IP) registration because of malformed request.
`int` | `MIP_FA_MISSING_CHALLENGE` Foreign agent rejected MIP (Mobile IP) registration because of missing challenge.
`int` | `MIP_FA_MISSING_HOME_ADDRESS` Foreign agent rejected MIP (Mobile IP) registration because of missing Home Address.
`int` | `MIP_FA_MISSING_HOME_AGENT` Foreign agent rejected MIP (Mobile IP) registration because of missing Home Agent.
`int` | `MIP_FA_MISSING_NAI` Foreign agent rejected MIP (Mobile IP) registration because of missing NAI (Network Access Identifier).
`int` | `MIP_FA_MOBILE_NODE_AUTHENTICATION_FAILURE` Foreign agent rejected MIP (Mobile IP) registration because of MN-AAA authenticator was wrong.
`int` | `MIP_FA_REASON_UNSPECIFIED` Reason unspecified for foreign agent rejected MIP (Mobile IP) registration.
`int` | `MIP_FA_REQUESTED_LIFETIME_TOO_LONG` Foreign agent rejected MIP (Mobile IP) registration because of requested lifetime was too long.
`int` | `MIP_FA_REVERSE_TUNNEL_IS_MANDATORY` Foreign agent rejected MIP (Mobile IP) registration because of reverse tunnel was mandatory but not requested by device.
`int` | `MIP_FA_REVERSE_TUNNEL_UNAVAILABLE` Foreign agent rejected MIP (Mobile IP) registration because of reverse tunnel was unavailable.
`int` | `MIP_FA_STALE_CHALLENGE` Foreign agent rejected MIP (Mobile IP) registration because of stale challenge.
`int` | `MIP_FA_UNKNOWN_CHALLENGE` Foreign agent rejected MIP (Mobile IP) registration because of unknown challenge.
`int` | `MIP_FA_VJ_HEADER_COMPRESSION_UNAVAILABLE` Foreign agent rejected MIP (Mobile IP) registration of VJ Header Compression was unavailable.
`int` | `MIP_HA_ADMIN_PROHIBITED` Home agent administratively prohibited MIP (Mobile IP) registration.
`int` | `MIP_HA_ENCAPSULATION_UNAVAILABLE` Home agent rejected MIP (Mobile IP) registration because of encapsulation unavailable.
`int` | `MIP_HA_FOREIGN_AGENT_AUTHENTICATION_FAILURE` Home agent rejected MIP (Mobile IP) registration because of foreign agent authentication failure.
`int` | `MIP_HA_INSUFFICIENT_RESOURCES` Home agent rejected MIP (Mobile IP) registration because of insufficient resources.
`int` | `MIP_HA_MALFORMED_REQUEST` Home agent rejected MIP (Mobile IP) registration because of malformed request.
`int` | `MIP_HA_MOBILE_NODE_AUTHENTICATION_FAILURE` Home agent rejected MIP (Mobile IP) registration because of MN-HA authenticator was wrong.
`int` | `MIP_HA_REASON_UNSPECIFIED` Reason unspecified for home agent rejected MIP (Mobile IP) registration.
`int` | `MIP_HA_REGISTRATION_ID_MISMATCH` Home agent rejected MIP (Mobile IP) registration because of registration id mismatch.
`int` | `MIP_HA_REVERSE_TUNNEL_IS_MANDATORY` Home agent rejected MIP (Mobile IP) registration because of reverse tunnel is mandatory but not requested by device.
`int` | `MIP_HA_REVERSE_TUNNEL_UNAVAILABLE` Home agent rejected MIP (Mobile IP) registration because of reverse tunnel was unavailable.
`int` | `MIP_HA_UNKNOWN_HOME_AGENT_ADDRESS` Home agent rejected MIP (Mobile IP) registration because of unknown home agent address.
`int` | `MISSING_UNKNOWN_APN` Missing or unknown APN.
`int` | `MODEM_APP_PREEMPTED` Another application in modem preempts the data call.
`int` | `MODEM_RESTART` Modem restart.
`int` | `MSC_TEMPORARILY_NOT_REACHABLE` Mobile switching center is temporarily unreachable.
`int` | `MSG_AND_PROTOCOL_STATE_UNCOMPATIBLE` Message and protocol state uncompatible.
`int` | `MSG_TYPE_NONCOMPATIBLE_STATE` Message type uncompatible.
`int` | `MS_IDENTITY_CANNOT_BE_DERIVED_BY_THE_NETWORK` No matching identity or context could be found in the network.
`int` | `MULTIPLE_PDP_CALL_NOT_ALLOWED` Multiple PDP call feature is disabled.
`int` | `MULTI_CONN_TO_SAME_PDN_NOT_ALLOWED` Multiple connections to a same PDN is not allowed.
`int` | `NAS_LAYER_FAILURE` Non-Access Spectrum layer failure.
`int` | `NAS_REQUEST_REJECTED_BY_NETWORK` Non-access stratum (NAS) request was rejected by the network.
`int` | `NAS_SIGNALLING` NAS signalling.
`int` | `NETWORK_FAILURE` Network Failure.
`int` | `NETWORK_INITIATED_DETACH_NO_AUTO_REATTACH` Network-initiated detach without reattach.
`int` | `NETWORK_INITIATED_DETACH_WITH_AUTO_REATTACH` Network-initiated detach with reattach.
`int` | `NETWORK_INITIATED_TERMINATION` Brought down by the network.
`int` | `NONE` There is no failure
`int` | `NON_IP_NOT_SUPPORTED` UE is unable to bring up a non-IP data call because the device is not camped on a NB1 cell.
`int` | `NORMAL_RELEASE` Receiving a release from the base station with no reason.
`int` | `NO_CDMA_SERVICE` Device does not have CDMA service.
`int` | `NO_COLLOCATED_HDR` There is no co-located HDR.
`int` | `NO_EPS_BEARER_CONTEXT_ACTIVATED` No EPS bearer context was activated.
`int` | `NO_GPRS_CONTEXT` GPRS context is not available.
`int` | `NO_HYBRID_HDR_SERVICE` Device has no hybrid HDR service.
`int` | `NO_PDP_CONTEXT_ACTIVATED` MS requests an establishment of the radio access bearers for all active PDP contexts by sending a service request message indicating data to the network, but the SGSN does not have any active PDP context.
`int` | `NO_RESPONSE_FROM_BASE_STATION` There was no response received from the base station.
`int` | `NO_SERVICE` Device has no service.
`int` | `NO_SERVICE_ON_GATEWAY` No service on the gateway.
`int` | `NSAPI_IN_USE` The Network Service Access Point Identifier (NSAPI) is in use.
`int` | `NULL_APN_DISALLOWED` PDN is attempted to be brought up with NULL APN but NULL APN is not supported.
`int` | `OEM_DCFAILCAUSE_1`
`int` | `OEM_DCFAILCAUSE_10`
`int` | `OEM_DCFAILCAUSE_11`
`int` | `OEM_DCFAILCAUSE_12`
`int` | `OEM_DCFAILCAUSE_13`
`int` | `OEM_DCFAILCAUSE_14`
`int` | `OEM_DCFAILCAUSE_15`
`int` | `OEM_DCFAILCAUSE_2`
`int` | `OEM_DCFAILCAUSE_3`
`int` | `OEM_DCFAILCAUSE_4`
`int` | `OEM_DCFAILCAUSE_5`
`int` | `OEM_DCFAILCAUSE_6`
`int` | `OEM_DCFAILCAUSE_7`
`int` | `OEM_DCFAILCAUSE_8`
`int` | `OEM_DCFAILCAUSE_9`
`int` | `ONLY_IPV4V6_ALLOWED` Network supports IPv4v6 PDP type only.
`int` | `ONLY_IPV4_ALLOWED` Packet Data Protocol (PDP) type IPv4 only allowed.
`int` | `ONLY_IPV6_ALLOWED` Packet Data Protocol (PDP) type IPv6 only allowed.
`int` | `ONLY_NON_IP_ALLOWED` Network supports non-IP PDP type only.
`int` | `ONLY_SINGLE_BEARER_ALLOWED` Single address bearers only allowed.
`int` | `OPERATOR_BARRED` Operator determined barring.
`int` | `OTASP_COMMIT_IN_PROGRESS` OTASP commit is in progress.
`int` | `PDN_CONN_DOES_NOT_EXIST` PDN connection does not exist.
`int` | `PDN_INACTIVITY_TIMER_EXPIRED` PDN inactivity timer expired due to no data transmission in a configurable duration of time.
`int` | `PDN_IPV4_CALL_DISALLOWED` IPV4 PDN is in throttled state due to network providing only IPV6 address during the previous VSNCP bringup (subs_limited_to_v6).
`int` | `PDN_IPV4_CALL_THROTTLED` IPV4 PDN is in throttled state due to previous VSNCP bringup failure(s).
`int` | `PDN_IPV6_CALL_DISALLOWED` IPV6 PDN is in throttled state due to network providing only IPV4 address during the previous VSNCP bringup (subs_limited_to_v4).
`int` | `PDN_IPV6_CALL_THROTTLED` IPV6 PDN is in throttled state due to previous VSNCP bringup failure(s).
`int` | `PDN_NON_IP_CALL_DISALLOWED` Non-IP PDN is in disallowed state due to the network providing only an IP address.
`int` | `PDN_NON_IP_CALL_THROTTLED` Non-IP PDN is in throttled state due to previous VSNCP bringup failure(s).
`int` | `PDP_ACTIVATE_MAX_RETRY_FAILED` SM attempts PDP activation for a maximum of four attempts.
`int` | `PDP_DUPLICATE` PDP context already exists.
`int` | `PDP_ESTABLISH_TIMEOUT_EXPIRED` Expiration of the PDP establish timer with a maximum of five retries.
`int` | `PDP_INACTIVE_TIMEOUT_EXPIRED` Expiration of the PDP deactivate timer with a maximum of four retries.
`int` | `PDP_LOWERLAYER_ERROR` PDP activation failed due to RRC_ABORT or a forbidden PLMN.
`int` | `PDP_MODIFY_COLLISION` MO PDP modify collision when the MT PDP is already in progress.
`int` | `PDP_MODIFY_TIMEOUT_EXPIRED` Expiration of the PDP modify timer with a maximum of four retries.
`int` | `PDP_PPP_NOT_SUPPORTED` PDP PPP calls are not supported.
`int` | `PDP_WITHOUT_ACTIVE_TFT` Packet Data Protocol (PDP) without active traffic flow template (TFT).
`int` | `PHONE_IN_USE` Device is in use (e.g., voice call).
`int` | `PHYSICAL_LINK_CLOSE_IN_PROGRESS` Physical link is in the process of cleanup.
`int` | `PLMN_NOT_ALLOWED` UE requests GPRS service, or the network initiates a detach request in a PLMN which does not offer roaming for GPRS services to that MS.
`int` | `PPP_AUTH_FAILURE` Data call bring up fails in the PPP setup due to an authorization failure.
`int` | `PPP_CHAP_FAILURE` Data call bring up fails in the PPP setup due to a CHAP failure.
`int` | `PPP_CLOSE_IN_PROGRESS` Data call bring up fails in the PPP setup because the PPP is in the process of cleaning the previous PPP session.
`int` | `PPP_OPTION_MISMATCH` Data call bring up fails in the PPP setup due to an option mismatch.
`int` | `PPP_PAP_FAILURE` Data call bring up fails in the PPP setup due to a PAP failure.
`int` | `PPP_TIMEOUT` Data call bring up fails in the PPP setup due to a timeout.
`int` | `PREF_RADIO_TECH_CHANGED` Preferred technology has changed, must retry with parameters appropriate for new technology.
`int` | `PROFILE_BEARER_INCOMPATIBLE` APN bearer type in the profile does not match preferred network mode.
`int` | `PROTOCOL_ERRORS` Protocol errors.
`int` | `QOS_NOT_ACCEPTED` Quality of service (QoS) is not accepted.
`int` | `RADIO_ACCESS_BEARER_FAILURE` Radio access bearer failure.
`int` | `RADIO_ACCESS_BEARER_SETUP_FAILURE` Radio access bearer is not established by the lower layers during activation, modification, or deactivation.
`int` | `RADIO_NOT_AVAILABLE` Data fail due to radio not unavailable.
`int` | `RADIO_POWER_OFF` data call was disconnected because radio was resetting, powered off.
`int` | `REDIRECTION_OR_HANDOFF_IN_PROGRESS` Device is in the process of redirecting or handing off to a different target system.
`int` | `REGISTRATION_FAIL` Data fail due to registration failure.
`int` | `REGULAR_DEACTIVATION` Regular deactivation.
`int` | `REJECTED_BY_BASE_STATION` The base station rejecting the call.
`int` | `RRC_CONNECTION_ABORTED_AFTER_HANDOVER` Radio resource control (RRC) connection was aborted by the non-access stratum (NAS) after an IRAT to LTE IRAT handover.
`int` | `RRC_CONNECTION_ABORTED_AFTER_IRAT_CELL_CHANGE` Radio resource control (RRC) connection was aborted before deactivating the LTE stack after a successful LTE to GSM/EDGE IRAT cell change order procedure.
`int` | `RRC_CONNECTION_ABORTED_DUE_TO_IRAT_CHANGE` Radio resource control (RRC) connection was aborted before deactivating the LTE stack due to a successful LTE to WCDMA/GSM/TD-SCDMA IRAT change.
`int` | `RRC_CONNECTION_ABORTED_DURING_IRAT_CELL_CHANGE` Radio resource control (RRC) connection was aborted in the middle of a LTE to GSM IRAT cell change order procedure.
`int` | `RRC_CONNECTION_ABORT_REQUEST` Connection has been released by the radio resource control (RRC) due to an abort request.
`int` | `RRC_CONNECTION_ACCESS_BARRED` Radio resource control (RRC) connection establishment failed due to access barrred.
`int` | `RRC_CONNECTION_ACCESS_STRATUM_FAILURE` Radio resource control (RRC) connection failure at access stratum.
`int` | `RRC_CONNECTION_ANOTHER_PROCEDURE_IN_PROGRESS` Radio resource control (RRC) connection establishment is aborted due to another procedure.
`int` | `RRC_CONNECTION_CELL_NOT_CAMPED` Connection establishment failed as the radio resource control (RRC) is not camped on any cell.
`int` | `RRC_CONNECTION_CELL_RESELECTION` Radio resource control (RRC) connection establishment failed due to cell reselection at access stratum.
`int` | `RRC_CONNECTION_CONFIG_FAILURE` Connection establishment failed due to configuration failure at the radio resource control (RRC).
`int` | `RRC_CONNECTION_INVALID_REQUEST` Radio resource control (RRC) connection establishment failure due to an error in the request message.
`int` | `RRC_CONNECTION_LINK_FAILURE` Connection establishment failed due to a link failure at the radio resource control (RRC).
`int` | `RRC_CONNECTION_NORMAL_RELEASE` Normal radio resource control (RRC) connection release.
`int` | `RRC_CONNECTION_OUT_OF_SERVICE_DURING_CELL_REGISTER` UE is out of service during the call register.
`int` | `RRC_CONNECTION_RADIO_LINK_FAILURE` Radio resource control (RRC) connection release failed due to radio link failure conditions.
`int` | `RRC_CONNECTION_REESTABLISHMENT_FAILURE` Radio resource control (RRC) connection re-establishment failure.
`int` | `RRC_CONNECTION_REJECT_BY_NETWORK` Radio resource control (RRC) connection establishment failed due to the network rejecting the UE connection request.
`int` | `RRC_CONNECTION_RELEASED_SECURITY_NOT_ACTIVE` If the UE has an LTE radio link failure before security is established, the radio resource control (RRC) connection must be released and the UE must return to idle.
`int` | `RRC_CONNECTION_RF_UNAVAILABLE` Radio resource control (RRC) connection establishment failure due to the RF was unavailable.
`int` | `RRC_CONNECTION_SYSTEM_INFORMATION_BLOCK_READ_ERROR` Radio resource control (RRC) connection released due to a system information block read error.
`int` | `RRC_CONNECTION_SYSTEM_INTERVAL_FAILURE` Connection establishment failed due to a service interval failure at the radio resource control (RRC).
`int` | `RRC_CONNECTION_TIMER_EXPIRED` Radio resource control (RRC) connection could not be established in the time limit.
`int` | `RRC_CONNECTION_TRACKING_AREA_ID_CHANGED` Radio resource control (RRC) connection establishment failure due to a change in the tracking area ID.
`int` | `RRC_UPLINK_CONNECTION_RELEASE` Radio resource control (RRC) uplink data delivery failed due to a connection release.
`int` | `RRC_UPLINK_DATA_TRANSMISSION_FAILURE` Transmission failure of radio resource control (RRC) uplink data.
`int` | `RRC_UPLINK_DELIVERY_FAILED_DUE_TO_HANDOVER` Radio resource control (RRC) uplink data delivery failed due to a handover.
`int` | `RRC_UPLINK_ERROR_REQUEST_FROM_NAS` Radio resource control (RRC) is not connected but the non-access stratum (NAS) sends an uplink data request.
`int` | `RRC_UPLINK_RADIO_LINK_FAILURE` Radio resource control (RRC) uplink data delivery failed due to a radio link failure.
`int` | `RUIM_NOT_PRESENT` RUIM not being present.
`int` | `SECURITY_MODE_REJECTED` Unspecified security mode reject.
`int` | `SERVICE_NOT_ALLOWED_ON_PLMN` Service is not allowed on the requested PLMN.
`int` | `SERVICE_OPTION_NOT_SUBSCRIBED` Requested service option not subscribed.
`int` | `SERVICE_OPTION_NOT_SUPPORTED` Service option not supported.
`int` | `SERVICE_OPTION_OUT_OF_ORDER` Service option temporarily out of order.
`int` | `SIGNAL_LOST` Data call drop due to network/modem disconnect.
`int` | `SIM_CARD_CHANGED` Card was refreshed or removed.
`int` | `SLICE_REJECTED` Data call fail due to the slice not being allowed for the data call.
`int` | `SYNCHRONIZATION_FAILURE` Synchronization failure.
`int` | `TEST_LOOPBACK_REGULAR_DEACTIVATION` Test loop-back data call has been successfully brought down.
`int` | `TETHERED_CALL_ACTIVE` Data call was disconnected by modem because tethered.
`int` | `TFT_SEMANTIC_ERROR` Semantic error in the Traffic flow templates (TFT) operation.
`int` | `TFT_SYTAX_ERROR` Syntactical error in the Traffic flow templates (TFT) operation.
`int` | `THERMAL_EMERGENCY` Put device in thermal emergency.
`int` | `THERMAL_MITIGATION` Thermal level increases and causes calls to be torn down when normal mode of operation is not allowed.
`int` | `TRAT_SWAP_FAILED` Target RAT swap failed.
`int` | `UE_INITIATED_DETACH_OR_DISCONNECT` UE performs a detach or disconnect PDN action based on TE requirements.
`int` | `UE_IS_ENTERING_POWERSAVE_MODE` UE is entering power save mode.
`int` | `UE_RAT_CHANGE` RAT change on the UE.
`int` | `UE_SECURITY_CAPABILITIES_MISMATCH` UE security capabilities mismatch.
`int` | `UMTS_HANDOVER_TO_IWLAN` UMTS interface is brought down due to handover from UMTS to iWLAN.
`int` | `UMTS_REACTIVATION_REQ` Universal Mobile Telecommunications System (UMTS) reactivation request.
`int` | `UNACCEPTABLE_NETWORK_PARAMETER` Data fail due to unacceptable network parameter.
`int` | `UNACCEPTABLE_NON_EPS_AUTHENTICATION` Unacceptable non-EPS authentication.
`int` | `UNKNOWN` Unknown data failure cause.
`int` | `UNKNOWN_INFO_ELEMENT` Unknown info element.
`int` | `UNKNOWN_PDP_ADDRESS_TYPE` Unknown Packet Data Protocol (PDP) address type.
`int` | `UNKNOWN_PDP_CONTEXT` Unknown Packet Data Protocol (PDP) context.
`int` | `UNPREFERRED_RAT` RAT on which the data call is attempted/connected is no longer the preferred RAT.
`int` | `UNSUPPORTED_1X_PREV` P_rev supported by 1 base station is less than 6, which is not supported for a 1X data call.
`int` | `UNSUPPORTED_APN_IN_CURRENT_PLMN` Unsupported APN in current public land mobile network (PLMN).
`int` | `UNSUPPORTED_QCI_VALUE` QCI (QoS Class Identifier) indicated in the UE request cannot be supported.
`int` | `USER_AUTHENTICATION` User authentication.
`int` | `VSNCP_ADMINISTRATIVELY_PROHIBITED` Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request with the reason of administratively prohibited at the HSGW.
`int` | `VSNCP_APN_UNAUTHORIZED` Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request because the requested APN is unauthorized.
`int` | `VSNCP_GEN_ERROR` Data call bring up fails in the VSNCP phase due to a general error.
`int` | `VSNCP_INSUFFICIENT_PARAMETERS` Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request with the reason of insufficient parameter.
`int` | `VSNCP_NO_PDN_GATEWAY_ADDRESS` Data call bring up fails in the VSNCP phase due to the network rejected the VSNCP configuration request due to no PDN gateway address.
`int` | `VSNCP_PDN_EXISTS_FOR_THIS_APN` Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request because the PDN exists for this APN.
`int` | `VSNCP_PDN_GATEWAY_REJECT` Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request due to a PDN gateway reject.
`int` | `VSNCP_PDN_GATEWAY_UNREACHABLE` Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request because the PDN gateway is unreachable.
`int` | `VSNCP_PDN_ID_IN_USE` Data call bring up fails in the VSNCP phase due to a network rejection of PDN ID in use, or all existing PDNs are brought down with this end reason because one of the PDN bring up was rejected by the network with the reason of PDN ID in use.
`int` | `VSNCP_PDN_LIMIT_EXCEEDED` Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request because the PDN limit has been exceeded.
`int` | `VSNCP_RECONNECT_NOT_ALLOWED` Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request with reconnect to this PDN not allowed, or an active data call is terminated by the network because reconnection to this PDN is not allowed.
`int` | `VSNCP_RESOURCE_UNAVAILABLE` Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request with the reason of resource unavailable.
`int` | `VSNCP_SUBSCRIBER_LIMITATION` Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request for the reason of subscriber limitation.
`int` | `VSNCP_TIMEOUT` Data call bring up fails in the VSNCP phase due to a VSNCP timeout error.

### Inherited methods
From class `java.lang.Object`
`Object` | `clone()` Creates and returns a copy of this object.
`boolean` | `equals(Object obj)` Indicates whether some other object is "equal to" this one.
`void` | `finalize()` Called by the garbage collector on an object when garbage collection determines that there are no more references to the object.
`final Class<?>` | `getClass()` Returns the runtime class of this `Object`.
`int` | `hashCode()` Returns a hash code value for the object.
`final void` | `notify()` Wakes up a single thread that is waiting on this object's monitor.
`final void` | `notifyAll()` Wakes up all threads that are waiting on this object's monitor.
`String` | `toString()` Returns a string representation of the object.
`final void` | `wait(long timeout, int nanos)` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object, or some other thread interrupts the current thread, or a certain amount of real time has elapsed.
`final void` | `wait(long timeout)` Causes the current thread to wait until either another thread invokes the `notify()` method or the `notifyAll()` method for this object, or a specified amount of time has elapsed.
`final void` | `wait()` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object.

## Constants

### ACCESS_ATTEMPT_ALREADY_IN_PROGRESS

    public static final int ACCESS_ATTEMPT_ALREADY_IN_PROGRESS

Access attempt is already in progress.

Constant Value: 2219 (0x000008ab)

### ACCESS_BLOCK

    public static final int ACCESS_BLOCK

Access blocked by the base station.

Constant Value: 2087 (0x00000827)

### ACCESS_BLOCK_ALL

    public static final int ACCESS_BLOCK_ALL

Access blocked by the base station for all mobile devices.

Constant Value: 2088 (0x00000828)

### ACCESS_CLASS_DSAC_REJECTION

    public static final int ACCESS_CLASS_DSAC_REJECTION

Access class blocking restrictions for the current camped cell.

Constant Value: 2108 (0x0000083c)

### ACCESS_CONTROL_LIST_CHECK_FAILURE

    public static final int ACCESS_CONTROL_LIST_CHECK_FAILURE

Access control list check failure at the lower layer.

Constant Value: 2128 (0x00000850)

### ACTIVATION_REJECTED_BCM_VIOLATION

    public static final int ACTIVATION_REJECTED_BCM_VIOLATION

UE requested to modify QoS parameters or the bearer control mode, which is not compatible with the selected bearer control mode.

Constant Value: 48 (0x00000030)

### ACTIVATION_REJECT_GGSN

    public static final int ACTIVATION_REJECT_GGSN

Activation rejected by Gateway GPRS Support Node (GGSN), Serving Gateway or PDN Gateway.

Constant Value: 30 (0x0000001e)

### ACTIVATION_REJECT_UNSPECIFIED

    public static final int ACTIVATION_REJECT_UNSPECIFIED

Activation rejected, unspecified.

Constant Value: 31 (0x0000001f)

### ACTIVE_PDP_CONTEXT_MAX_NUMBER_REACHED

    public static final int ACTIVE_PDP_CONTEXT_MAX_NUMBER_REACHED

Max number of Packet Data Protocol (PDP) context reached.

Constant Value: 65 (0x00000041)

### ALL_MATCHING_RULES_FAILED

    public static final int ALL_MATCHING_RULES_FAILED

If connection failed for all matching URSP rules.

Constant Value: 2254 (0x000008ce)

### APN_DISABLED

    public static final int APN_DISABLED

APN has been disabled.

Constant Value: 2045 (0x000007fd)

### APN_DISALLOWED_ON_ROAMING

    public static final int APN_DISALLOWED_ON_ROAMING

PDN connection to the APN is disallowed on the roaming network.

Constant Value: 2059 (0x0000080b)

### APN_MISMATCH

    public static final int APN_MISMATCH

New PDN bring up is rejected during interface selection because the UE has already allotted the available interfaces for other PDNs.

Constant Value: 2054 (0x00000806)

### APN_PARAMETERS_CHANGED

    public static final int APN_PARAMETERS_CHANGED

APN-related parameters are changed.

Constant Value: 2060 (0x0000080c)

### APN_PENDING_HANDOVER

    public static final int APN_PENDING_HANDOVER

Interface bring up is attempted for an APN that is yet to be handed over to target RAT.

Constant Value: 2041 (0x000007f9)

### APN_TYPE_CONFLICT

    public static final int APN_TYPE_CONFLICT

APN type conflict.

Constant Value: 112 (0x00000070)

### AUTH_FAILURE_ON_EMERGENCY_CALL

    public static final int AUTH_FAILURE_ON_EMERGENCY_CALL

Authentication failure on emergency call.

Constant Value: 122 (0x0000007a)

### BEARER_HANDLING_NOT_SUPPORTED

    public static final int BEARER_HANDLING_NOT_SUPPORTED

Procedure requested by the UE was rejected because the bearer handling is not supported.

Constant Value: 60 (0x0000003c)

### CALL_DISALLOWED_IN_ROAMING

    public static final int CALL_DISALLOWED_IN_ROAMING

Roaming is disallowed during call bring up.

Constant Value: 2068 (0x00000814)

### CALL_PREEMPT_BY_EMERGENCY_APN

    public static final int CALL_PREEMPT_BY_EMERGENCY_APN

Emergency call bring up on a different ePDG.

Constant Value: 127 (0x0000007f)

### CANNOT_ENCODE_OTA_MESSAGE

    public static final int CANNOT_ENCODE_OTA_MESSAGE

Unable to encode the OTA message for MT PDP or deactivate PDP.

Constant Value: 2159 (0x0000086f)

### CDMA_ALERT_STOP

    public static final int CDMA_ALERT_STOP

Received an alert stop from the base station due to incoming only.

Constant Value: 2077 (0x0000081d)

### CDMA_INCOMING_CALL

    public static final int CDMA_INCOMING_CALL

Receiving an incoming call from the base station.

Constant Value: 2076 (0x0000081c)

### CDMA_INTERCEPT

    public static final int CDMA_INTERCEPT

Received an intercept order from the base station.

Constant Value: 2073 (0x00000819)

### CDMA_LOCK

    public static final int CDMA_LOCK

Device in CDMA locked state.

Constant Value: 2072 (0x00000818)

### CDMA_RELEASE_DUE_TO_SO_REJECTION

    public static final int CDMA_RELEASE_DUE_TO_SO_REJECTION

Receiving a release from the base station with a SO (Service Option) Reject reason.

Constant Value: 2075 (0x0000081b)

### CDMA_REORDER

    public static final int CDMA_REORDER

Receiving a reorder from the base station.

Constant Value: 2074 (0x0000081a)

### CDMA_RETRY_ORDER

    public static final int CDMA_RETRY_ORDER

Receiving a retry order from the base station.

Constant Value: 2086 (0x00000826)

### CHANNEL_ACQUISITION_FAILURE

    public static final int CHANNEL_ACQUISITION_FAILURE

Channel acquisition failures. This indicates that device has failed acquiring all the channels in the PRL.

Constant Value: 2078 (0x0000081e)

### CLOSE_IN_PROGRESS

    public static final int CLOSE_IN_PROGRESS

Tearing down is in progress.

Constant Value: 2030 (0x000007ee)

### COLLISION_WITH_NETWORK_INITIATED_REQUEST

    public static final int COLLISION_WITH_NETWORK_INITIATED_REQUEST

Network has already initiated the activation, modification, or deactivation of bearer resources that was requested by the UE.

Constant Value: 56 (0x00000038)

### COMPANION_IFACE_IN_USE

    public static final int COMPANION_IFACE_IN_USE

Companion interface in use.

Constant Value: 118 (0x00000076)

### CONCURRENT_SERVICES_INCOMPATIBLE

    public static final int CONCURRENT_SERVICES_INCOMPATIBLE

The concurrent services requested were not compatible.

Constant Value: 2083 (0x00000823)

### CONCURRENT_SERVICES_NOT_ALLOWED

    public static final int CONCURRENT_SERVICES_NOT_ALLOWED

In favor of a voice call or SMS when concurrent voice and data are not supported.

Constant Value: 2091 (0x0000082b)

### CONCURRENT_SERVICE_NOT_SUPPORTED_BY_BASE_STATION

    public static final int CONCURRENT_SERVICE_NOT_SUPPORTED_BY_BASE_STATION

Concurrent service is not supported by base station.

Constant Value: 2080 (0x00000820)

### CONDITIONAL_IE_ERROR

    public static final int CONDITIONAL_IE_ERROR

Conditional Information Element (IE) error.

Constant Value: 100 (0x00000064)

### CONGESTION

    public static final int CONGESTION

Network cannot serve a request from the MS due to congestion.

Constant Value: 2106 (0x0000083a)

### CONNECTION_RELEASED

    public static final int CONNECTION_RELEASED

Indicate the connection was released.

Constant Value: 2113 (0x00000841)

### CS_DOMAIN_NOT_AVAILABLE

    public static final int CS_DOMAIN_NOT_AVAILABLE

CS domain is not available.

Constant Value: 2181 (0x00000885)

### CS_FALLBACK_CALL_ESTABLISHMENT_NOT_ALLOWED

    public static final int CS_FALLBACK_CALL_ESTABLISHMENT_NOT_ALLOWED

CS fallback call establishment is not allowed.

Constant Value: 2188 (0x0000088c)

### DATA_PLAN_EXPIRED

    public static final int DATA_PLAN_EXPIRED

Network initiates a detach on LTE with error cause ""data plan has been replenished or has expired.

Constant Value: 2198 (0x00000896)

### DATA_ROAMING_SETTINGS_DISABLED

    public static final int DATA_ROAMING_SETTINGS_DISABLED

PDN Connection to a given APN is disallowed because data roaming is disabled from the device user interface settings and the UE is roaming.

Constant Value: 2064 (0x00000810)

### DATA_SETTINGS_DISABLED

    public static final int DATA_SETTINGS_DISABLED

PDN Connection to a given APN is disallowed because data is disabled from the device user interface settings.

Constant Value: 2063 (0x0000080f)

### DBM_OR_SMS_IN_PROGRESS

    public static final int DBM_OR_SMS_IN_PROGRESS

DBM or SMS is in progress.

Constant Value: 2211 (0x000008a3)

### DDS_SWITCHED

    public static final int DDS_SWITCHED

DDS (Default data subscription) switch occurs.

Constant Value: 2065 (0x00000811)

### DDS_SWITCH_IN_PROGRESS

    public static final int DDS_SWITCH_IN_PROGRESS

Default data subscription switch is in progress.

Constant Value: 2067 (0x00000813)

### DRB_RELEASED_BY_RRC

    public static final int DRB_RELEASED_BY_RRC

Data radio bearer is released by the RRC.

Constant Value: 2112 (0x00000840)

### DS_EXPLICIT_DEACTIVATION

    public static final int DS_EXPLICIT_DEACTIVATION

Dedicated bearer will be deactivated regardless of the network response.

Constant Value: 2125 (0x0000084d)

### DUAL_SWITCH

    public static final int DUAL_SWITCH

Dual switch from single standby to dual standby is in progress.

Constant Value: 2227 (0x000008b3)

### DUN_CALL_DISALLOWED

    public static final int DUN_CALL_DISALLOWED

Dial up networking (DUN) call bring up is rejected since UE is in eHRPD RAT.

Constant Value: 2056 (0x00000808)

### DUPLICATE_BEARER_ID

    public static final int DUPLICATE_BEARER_ID

Active dedicated bearer was requested using the same default bearer ID.

Constant Value: 2118 (0x00000846)

### EHRPD_TO_HRPD_FALLBACK

    public static final int EHRPD_TO_HRPD_FALLBACK

Device falls back from eHRPD to HRPD.

Constant Value: 2049 (0x00000801)

### EMBMS_NOT_ENABLED

    public static final int EMBMS_NOT_ENABLED

Data call has been brought down because EMBMS is not enabled at the RRC layer.

Constant Value: 2193 (0x00000891)

### EMBMS_REGULAR_DEACTIVATION

    public static final int EMBMS_REGULAR_DEACTIVATION

EMBMS data call has been successfully brought down.

Constant Value: 2195 (0x00000893)

### EMERGENCY_IFACE_ONLY

    public static final int EMERGENCY_IFACE_ONLY

Emergency interface only.

Constant Value: 116 (0x00000074)

### EMERGENCY_MODE

    public static final int EMERGENCY_MODE

Device is operating in Emergency mode.

Constant Value: 2221 (0x000008ad)

### EMM_ACCESS_BARRED

    public static final int EMM_ACCESS_BARRED

EPS (Evolved Packet System) Mobility Management (EMM) access barred.

Constant Value: 115 (0x00000073)

### EMM_ACCESS_BARRED_INFINITE_RETRY

    public static final int EMM_ACCESS_BARRED_INFINITE_RETRY

EPS (Evolved Packet System) Mobility Management (EMM) access barred infinity retry. *

Constant Value: 121 (0x00000079)

### EMM_ATTACH_FAILED

    public static final int EMM_ATTACH_FAILED

Attach procedure is rejected by the network.

Constant Value: 2115 (0x00000843)

### EMM_ATTACH_STARTED

    public static final int EMM_ATTACH_STARTED

Attach procedure is started for EMC purposes.

Constant Value: 2116 (0x00000844)

### EMM_DETACHED

    public static final int EMM_DETACHED

UE is detached.

Constant Value: 2114 (0x00000842)

### EMM_T3417_EXPIRED

    public static final int EMM_T3417_EXPIRED

T3417 timer expiration of the service request procedure.

Constant Value: 2130 (0x00000852)

### EMM_T3417_EXT_EXPIRED

    public static final int EMM_T3417_EXT_EXPIRED

Extended service request fails due to expiration of the T3417 EXT timer.

Constant Value: 2131 (0x00000853)

### EPS_SERVICES_AND_NON_EPS_SERVICES_NOT_ALLOWED

    public static final int EPS_SERVICES_AND_NON_EPS_SERVICES_NOT_ALLOWED

EPS and non-EPS services are not allowed by the network.

Constant Value: 2178 (0x00000882)

### EPS_SERVICES_NOT_ALLOWED_IN_PLMN

    public static final int EPS_SERVICES_NOT_ALLOWED_IN_PLMN

EPS services are not allowed in the PLMN.

Constant Value: 2179 (0x00000883)

### ERROR_UNSPECIFIED

    public static final int ERROR_UNSPECIFIED

Data call fail due to unspecific errors.

Constant Value: 65535 (0x0000ffff)

### ESM_BAD_OTA_MESSAGE

    public static final int ESM_BAD_OTA_MESSAGE

Bad OTA message is received from the network.

Constant Value: 2122 (0x0000084a)

### ESM_BEARER_DEACTIVATED_TO_SYNC_WITH_NETWORK

    public static final int ESM_BEARER_DEACTIVATED_TO_SYNC_WITH_NETWORK

Bearer must be deactivated to synchronize with the network.

Constant Value: 2120 (0x00000848)

### ESM_COLLISION_SCENARIOS

    public static final int ESM_COLLISION_SCENARIOS

Collision scenarios for the UE and network-initiated procedures.

Constant Value: 2119 (0x00000847)

### ESM_CONTEXT_TRANSFERRED_DUE_TO_IRAT

    public static final int ESM_CONTEXT_TRANSFERRED_DUE_TO_IRAT

PDN was disconnected by the downlaod server due to IRAT.

Constant Value: 2124 (0x0000084c)

### ESM_DOWNLOAD_SERVER_REJECTED_THE_CALL

    public static final int ESM_DOWNLOAD_SERVER_REJECTED_THE_CALL

Download server rejected the call.

Constant Value: 2123 (0x0000084b)

### ESM_FAILURE

    public static final int ESM_FAILURE

ESM level failure.

Constant Value: 2182 (0x00000886)

### ESM_INFO_NOT_RECEIVED

    public static final int ESM_INFO_NOT_RECEIVED

EPS Session Management (ESM) information is not received.

Constant Value: 53 (0x00000035)

### ESM_LOCAL_CAUSE_NONE

    public static final int ESM_LOCAL_CAUSE_NONE

No specific local cause is mentioned, usually a valid OTA cause.

Constant Value: 2126 (0x0000084e)

### ESM_NW_ACTIVATED_DED_BEARER_WITH_ID_OF_DEF_BEARER

    public static final int ESM_NW_ACTIVATED_DED_BEARER_WITH_ID_OF_DEF_BEARER

Active dedicated bearer was requested for an existing default bearer.

Constant Value: 2121 (0x00000849)

### ESM_PROCEDURE_TIME_OUT

    public static final int ESM_PROCEDURE_TIME_OUT

ESM procedure maximum attempt timeout failure.

Constant Value: 2155 (0x0000086b)

### ESM_UNKNOWN_EPS_BEARER_CONTEXT

    public static final int ESM_UNKNOWN_EPS_BEARER_CONTEXT

Invalid EPS bearer identity in the request.

Constant Value: 2111 (0x0000083f)

### EVDO_CONNECTION_DENY_BY_BILLING_OR_AUTHENTICATION_FAILURE

    public static final int EVDO_CONNECTION_DENY_BY_BILLING_OR_AUTHENTICATION_FAILURE

Received a connection deny due to billing or authentication failure on EVDO network.

Constant Value: 2201 (0x00000899)

### EVDO_CONNECTION_DENY_BY_GENERAL_OR_NETWORK_BUSY

    public static final int EVDO_CONNECTION_DENY_BY_GENERAL_OR_NETWORK_BUSY

Received a connection deny due to general or network busy on EVDO network.

Constant Value: 2200 (0x00000898)

### EVDO_HDR_CHANGED

    public static final int EVDO_HDR_CHANGED

HDR system has been changed due to redirection or the PRL was not preferred.

Constant Value: 2202 (0x0000089a)

### EVDO_HDR_CONNECTION_SETUP_TIMEOUT

    public static final int EVDO_HDR_CONNECTION_SETUP_TIMEOUT

Connection setup on the HDR system was time out.

Constant Value: 2206 (0x0000089e)

### EVDO_HDR_EXITED

    public static final int EVDO_HDR_EXITED

Device exited HDR due to redirection or the PRL was not preferred.

Constant Value: 2203 (0x0000089b)

### EVDO_HDR_NO_SESSION

    public static final int EVDO_HDR_NO_SESSION

Device does not have an HDR session.

Constant Value: 2204 (0x0000089c)

### EVDO_USING_GPS_FIX_INSTEAD_OF_HDR_CALL

    public static final int EVDO_USING_GPS_FIX_INSTEAD_OF_HDR_CALL

It is ending an HDR call origination in favor of a GPS fix.

Constant Value: 2205 (0x0000089d)

### FADE

    public static final int FADE

Device lost the system due to fade.

Constant Value: 2217 (0x000008a9)

### FAILED_TO_ACQUIRE_COLOCATED_HDR

    public static final int FAILED_TO_ACQUIRE_COLOCATED_HDR

Device failed to acquire a co-located HDR for origination.

Constant Value: 2207 (0x0000089f)

### FEATURE_NOT_SUPP

    public static final int FEATURE_NOT_SUPP

Feature not supported.

Constant Value: 40 (0x00000028)

### FILTER_SEMANTIC_ERROR

    public static final int FILTER_SEMANTIC_ERROR

Semantic errors in packet filter.

Constant Value: 44 (0x0000002c)

### FILTER_SYTAX_ERROR

    public static final int FILTER_SYTAX_ERROR

Syntactical errors in packet filter(s).

Constant Value: 45 (0x0000002d)

### FORBIDDEN_APN_NAME

    public static final int FORBIDDEN_APN_NAME

PDN being brought up with an APN that is part of forbidden APN Name list.

Constant Value: 2066 (0x00000812)

### GPRS_REGISTRATION_FAIL

    public static final int GPRS_REGISTRATION_FAIL

Data fail due to GPRS registration failure.

Constant Value: -2 (0xfffffffe)

### GPRS_SERVICES_AND_NON_GPRS_SERVICES_NOT_ALLOWED

    public static final int GPRS_SERVICES_AND_NON_GPRS_SERVICES_NOT_ALLOWED

Not allowed to operate either GPRS or non-GPRS services.

Constant Value: 2097 (0x00000831)

### GPRS_SERVICES_NOT_ALLOWED

    public static final int GPRS_SERVICES_NOT_ALLOWED

MS is not allowed to operate GPRS services.

Constant Value: 2098 (0x00000832)

### GPRS_SERVICES_NOT_ALLOWED_IN_THIS_PLMN

    public static final int GPRS_SERVICES_NOT_ALLOWED_IN_THIS_PLMN

UE requests GPRS service or the network initiates a detach request in a PLMN that does not offer roaming for GPRS services.

Constant Value: 2103 (0x00000837)

### HANDOFF_PREFERENCE_CHANGED

    public static final int HANDOFF_PREFERENCE_CHANGED

System preference change back to SRAT during handoff

Constant Value: 2251 (0x000008cb)

### HDR_ACCESS_FAILURE

    public static final int HDR_ACCESS_FAILURE

HDR system access failure.

Constant Value: 2213 (0x000008a5)

### HDR_FADE

    public static final int HDR_FADE

HDR module released the call due to fade.

Constant Value: 2212 (0x000008a4)

### HDR_NO_LOCK_GRANTED

    public static final int HDR_NO_LOCK_GRANTED

HDR module could not be obtained because of the RF locked.

Constant Value: 2210 (0x000008a2)

### IFACE_AND_POL_FAMILY_MISMATCH

    public static final int IFACE_AND_POL_FAMILY_MISMATCH

Constant Value: 120 (0x00000078)

### IFACE_MISMATCH

    public static final int IFACE_MISMATCH

Interface mismatch.

Constant Value: 117 (0x00000075)

### ILLEGAL_ME

    public static final int ILLEGAL_ME

ME could not be authenticated and the ME used is not acceptable to the network.

Constant Value: 2096 (0x00000830)

### ILLEGAL_MS

    public static final int ILLEGAL_MS

Network refuses service to the MS because either an identity of the MS is not acceptable to the network or the MS does not pass the authentication check.

Constant Value: 2095 (0x0000082f)

### IMEI_NOT_ACCEPTED

    public static final int IMEI_NOT_ACCEPTED

IMEI of the UE is not accepted by the network.

Constant Value: 2177 (0x00000881)

### IMPLICITLY_DETACHED

    public static final int IMPLICITLY_DETACHED

Mobile reachable timer has expired, or the GMM context data related to the subscription does not exist in the SGSN.

Constant Value: 2100 (0x00000834)

### IMSI_UNKNOWN_IN_HOME_SUBSCRIBER_SERVER

    public static final int IMSI_UNKNOWN_IN_HOME_SUBSCRIBER_SERVER

IMSI present in the UE is unknown in the home subscriber server.

Constant Value: 2176 (0x00000880)

### INCOMING_CALL_REJECTED

    public static final int INCOMING_CALL_REJECTED

The other clients rejected incoming call.

Constant Value: 2092 (0x0000082c)

### INSUFFICIENT_RESOURCES

    public static final int INSUFFICIENT_RESOURCES

Insufficient resources.

Constant Value: 26 (0x0000001a)

### INTERFACE_IN_USE

    public static final int INTERFACE_IN_USE

The current interface is being in use.

Constant Value: 2058 (0x0000080a)

### INTERNAL_CALL_PREEMPT_BY_HIGH_PRIO_APN

    public static final int INTERNAL_CALL_PREEMPT_BY_HIGH_PRIO_APN

Internal data call preempt by high priority APN.

Constant Value: 114 (0x00000072)

### INTERNAL_EPC_NONEPC_TRANSITION

    public static final int INTERNAL_EPC_NONEPC_TRANSITION

Rejected/Brought down since UE is transition between EPC and NONEPC RAT.

Constant Value: 2057 (0x00000809)

### INVALID_CONNECTION_ID

    public static final int INVALID_CONNECTION_ID

No PDP exists with the given connection ID while modifying or deactivating or activation for an already active PDP.

Constant Value: 2156 (0x0000086c)

### INVALID_DNS_ADDR

    public static final int INVALID_DNS_ADDR

Not receiving a DNS address that was mandatory.

Constant Value: 123 (0x0000007b)

### INVALID_EMM_STATE

    public static final int INVALID_EMM_STATE

Invalid EMM state.

Constant Value: 2190 (0x0000088e)

### INVALID_MANDATORY_INFO

    public static final int INVALID_MANDATORY_INFO

Invalid mandatory information.

Constant Value: 96 (0x00000060)

### INVALID_MODE

    public static final int INVALID_MODE

Device operational mode is different from the mode requested in the traffic channel bring up.

Constant Value: 2223 (0x000008af)

### INVALID_PCSCF_ADDR

    public static final int INVALID_PCSCF_ADDR

Invalid Proxy-Call Session Control Function (P-CSCF) address.

Constant Value: 113 (0x00000071)

### INVALID_PCSCF_OR_DNS_ADDRESS

    public static final int INVALID_PCSCF_OR_DNS_ADDRESS

Not receiving either a PCSCF or a DNS address, one of them being mandatory.

Constant Value: 124 (0x0000007c)

### INVALID_PRIMARY_NSAPI

    public static final int INVALID_PRIMARY_NSAPI

Primary context for NSAPI does not exist.

Constant Value: 2158 (0x0000086e)

### INVALID_SIM_STATE

    public static final int INVALID_SIM_STATE

SIM was marked by the network as invalid for the circuit and/or packet service domain.

Constant Value: 2224 (0x000008b0)

### INVALID_TRANSACTION_ID

    public static final int INVALID_TRANSACTION_ID

Invalid transaction id.

Constant Value: 81 (0x00000051)

### IPV6_ADDRESS_TRANSFER_FAILED

    public static final int IPV6_ADDRESS_TRANSFER_FAILED

IPv6 address transfer failed.

Constant Value: 2047 (0x000007ff)

### IPV6_PREFIX_UNAVAILABLE

    public static final int IPV6_PREFIX_UNAVAILABLE

Device failure to obtain the prefix from the network.

Constant Value: 2250 (0x000008ca)

### IP_ADDRESS_MISMATCH

    public static final int IP_ADDRESS_MISMATCH

IP address mismatch.

Constant Value: 119 (0x00000077)

### IP_VERSION_MISMATCH

    public static final int IP_VERSION_MISMATCH

New call bring up is rejected since the existing data call IP type doesn't match the requested IP.

Constant Value: 2055 (0x00000807)

### IRAT_HANDOVER_FAILED

    public static final int IRAT_HANDOVER_FAILED

Data call was unsuccessfully transferred during the IRAT handover.

Constant Value: 2194 (0x00000892)

### IS707B_MAX_ACCESS_PROBES

    public static final int IS707B_MAX_ACCESS_PROBES

Maximum access probes for the IS-707B call.

Constant Value: 2089 (0x00000829)

### IWLAN_AUTHORIZATION_REJECTED

    public static final int IWLAN_AUTHORIZATION_REJECTED

The user is barred from using the non-3GPP access or the subscribed APN.

Constant Value: 9003 (0x0000232b)

### IWLAN_DNS_RESOLUTION_NAME_FAILURE

    public static final int IWLAN_DNS_RESOLUTION_NAME_FAILURE

Unable to resolve FQDN for the ePDG to an IP address

Constant Value: 16388 (0x00004004)

### IWLAN_DNS_RESOLUTION_TIMEOUT

    public static final int IWLAN_DNS_RESOLUTION_TIMEOUT

No response received from the DNS Server due to a timeout

Constant Value: 16389 (0x00004005)

### IWLAN_IKEV2_AUTH_FAILURE

    public static final int IWLAN_IKEV2_AUTH_FAILURE

Sent in the response to an IKE_AUTH message when, for some reason, the authentication failed.

Constant Value: 16385 (0x00004001)

### IWLAN_IKEV2_CERT_INVALID

    public static final int IWLAN_IKEV2_CERT_INVALID

IKE Certification validation failure

Constant Value: 16387 (0x00004003)

### IWLAN_IKEV2_CONFIG_FAILURE

    public static final int IWLAN_IKEV2_CONFIG_FAILURE

IKE configuration error resulting in failure

Constant Value: 16384 (0x00004000)

### IWLAN_IKEV2_MSG_TIMEOUT

    public static final int IWLAN_IKEV2_MSG_TIMEOUT

IKE message timeout, tunnel setup failed due to no response from EPDG

Constant Value: 16386 (0x00004002)

### IWLAN_ILLEGAL_ME

    public static final int IWLAN_ILLEGAL_ME

The Mobile Equipment used is not acceptable to the network

Constant Value: 9006 (0x0000232e)

### IWLAN_IMEI_NOT_ACCEPTED

    public static final int IWLAN_IMEI_NOT_ACCEPTED

The network does not accept emergency PDN bringup request using an IMEI

Constant Value: 11005 (0x00002afd)

### IWLAN_MAX_CONNECTION_REACHED

    public static final int IWLAN_MAX_CONNECTION_REACHED

The PDN connection has been rejected. No additional PDN connections can be established for the UE due to the network policies or capabilities.

Constant Value: 8193 (0x00002001)

### IWLAN_NETWORK_FAILURE

    public static final int IWLAN_NETWORK_FAILURE

The network has determined that the requested procedure cannot be completed successfully due to network failure.

Constant Value: 10500 (0x00002904)

### IWLAN_NON_3GPP_ACCESS_TO_EPC_NOT_ALLOWED

    public static final int IWLAN_NON_3GPP_ACCESS_TO_EPC_NOT_ALLOWED

No non-3GPP subscription is associated with the IMSI. The UE is not allowed to use non-3GPP access to EPC.

Constant Value: 9000 (0x00002328)

### IWLAN_NO_APN_SUBSCRIPTION

    public static final int IWLAN_NO_APN_SUBSCRIPTION

The requested APN is not included in the user's profile, and therefore is not authorized for that user.

Constant Value: 9002 (0x0000232a)

### IWLAN_PDN_CONNECTION_REJECTION

    public static final int IWLAN_PDN_CONNECTION_REJECTION

The PDN connection corresponding to the requested APN has been rejected.

Constant Value: 8192 (0x00002000)

### IWLAN_PLMN_NOT_ALLOWED

    public static final int IWLAN_PLMN_NOT_ALLOWED

The ePDG performs PLMN filtering (based on roaming agreements) and rejects the request from the UE. The UE requests service in a PLMN where the UE is not allowed to operate.

Constant Value: 11011 (0x00002b03)

### IWLAN_RAT_TYPE_NOT_ALLOWED

    public static final int IWLAN_RAT_TYPE_NOT_ALLOWED

The access type is restricted to the user.

Constant Value: 11001 (0x00002af9)

### IWLAN_SEMANTIC_ERRORS_IN_PACKET_FILTERS

    public static final int IWLAN_SEMANTIC_ERRORS_IN_PACKET_FILTERS

The PDN connection has been rejected due to sematic errors in the packet filter.

Constant Value: 8244 (0x00002034)

### IWLAN_SEMANTIC_ERROR_IN_THE_TFT_OPERATION

    public static final int IWLAN_SEMANTIC_ERROR_IN_THE_TFT_OPERATION

The PDN connection has been rejected due to a semantic error in TFT operation.

Constant Value: 8241 (0x00002031)

### IWLAN_SYNTACTICAL_ERRORS_IN_PACKET_FILTERS

    public static final int IWLAN_SYNTACTICAL_ERRORS_IN_PACKET_FILTERS

The PDN connection has been rejected due to syntactic errors in the packet filter.

Constant Value: 8245 (0x00002035)

### IWLAN_SYNTACTICAL_ERROR_IN_THE_TFT_OPERATION

    public static final int IWLAN_SYNTACTICAL_ERROR_IN_THE_TFT_OPERATION

The PDN connection has been rejected due to a syntactic error in TFT operation.

Constant Value: 8242 (0x00002032)

### IWLAN_UNAUTHENTICATED_EMERGENCY_NOT_SUPPORTED

    public static final int IWLAN_UNAUTHENTICATED_EMERGENCY_NOT_SUPPORTED

The ePDG does not support un-authenticated IMSI based emergency PDN bringup *

Constant Value: 11055 (0x00002b2f)

### IWLAN_USER_UNKNOWN

    public static final int IWLAN_USER_UNKNOWN

The user identified by the IMSI is unknown.

Constant Value: 9001 (0x00002329)

### LIMITED_TO_IPV4

    public static final int LIMITED_TO_IPV4

IPv6 interface bring up fails because the network provided only the IPv4 address for the upcoming PDN permanent client can reattempt a IPv6 call bring up after the IPv4 interface is also brought down. However, there is no guarantee that the network will provide a IPv6 address.

Constant Value: 2234 (0x000008ba)

### LIMITED_TO_IPV6

    public static final int LIMITED_TO_IPV6

IPv4 interface bring up fails because the network provided only the IPv6 address for the upcoming PDN permanent client can reattempt a IPv4 call bring up after the IPv6 interface is also brought down. However there is no guarantee that the network will provide a IPv4 address.

Constant Value: 2235 (0x000008bb)

### LLC_SNDCP

    public static final int LLC_SNDCP

Logical Link Control (LLC) Sub Network Dependent Convergence Protocol (SNDCP).

Constant Value: 25 (0x00000019)

### LOCAL_END

    public static final int LOCAL_END

Client ended the data call.

Constant Value: 2215 (0x000008a7)

### LOCATION_AREA_NOT_ALLOWED

    public static final int LOCATION_AREA_NOT_ALLOWED

MS requests service, or the network initiates a detach request, in a location area where the HPLMN determines that the MS, by subscription, is not allowed to operate.

Constant Value: 2102 (0x00000836)

### LOST_CONNECTION

    public static final int LOST_CONNECTION

Data connection was lost.

Constant Value: 65540 (0x00010004)

### LOWER_LAYER_REGISTRATION_FAILURE

    public static final int LOWER_LAYER_REGISTRATION_FAILURE

Lower layer registration failure.

Constant Value: 2197 (0x00000895)

### LOW_POWER_MODE_OR_POWERING_DOWN

    public static final int LOW_POWER_MODE_OR_POWERING_DOWN

Device is going into lower power mode or powering down.

Constant Value: 2044 (0x000007fc)

### LTE_NAS_SERVICE_REQUEST_FAILED

    public static final int LTE_NAS_SERVICE_REQUEST_FAILED

Service request procedure failure.

Constant Value: 2117 (0x00000845)

### LTE_THROTTLING_NOT_REQUIRED

    public static final int LTE_THROTTLING_NOT_REQUIRED

Throttling is not needed for this service request failure.

Constant Value: 2127 (0x0000084f)

### MAC_FAILURE

    public static final int MAC_FAILURE

MAC level failure.

Constant Value: 2183 (0x00000887)

### MATCH_ALL_RULE_NOT_ALLOWED

    public static final int MATCH_ALL_RULE_NOT_ALLOWED

No matching rule available for the request, and match-all rule is not allowed for it.

Constant Value: 2253 (0x000008cd)

### MAXIMIUM_NSAPIS_EXCEEDED

    public static final int MAXIMIUM_NSAPIS_EXCEEDED

Maximum NSAPIs have been exceeded during PDP activation.

Constant Value: 2157 (0x0000086d)

### MAXINUM_SIZE_OF_L2_MESSAGE_EXCEEDED

    public static final int MAXINUM_SIZE_OF_L2_MESSAGE_EXCEEDED

Maximum size of the L2 message was exceeded.

Constant Value: 2166 (0x00000876)

### MAX_ACCESS_PROBE

    public static final int MAX_ACCESS_PROBE

Maximum access probes transmitted.

Constant Value: 2079 (0x0000081f)

### MAX_IPV4_CONNECTIONS

    public static final int MAX_IPV4_CONNECTIONS

IPv4 data call bring up is rejected because the UE already maintains the allotted maximum number of IPv4 data connections.

Constant Value: 2052 (0x00000804)

### MAX_IPV6_CONNECTIONS

    public static final int MAX_IPV6_CONNECTIONS

IPv6 data call bring up is rejected because the UE already maintains the allotted maximum number of IPv6 data connections.

Constant Value: 2053 (0x00000805)

### MAX_PPP_INACTIVITY_TIMER_EXPIRED

    public static final int MAX_PPP_INACTIVITY_TIMER_EXPIRED

Maximum PPP inactivity timer expired.

Constant Value: 2046 (0x000007fe)

### MESSAGE_INCORRECT_SEMANTIC

    public static final int MESSAGE_INCORRECT_SEMANTIC

Incorrect message semantic.

Constant Value: 95 (0x0000005f)

### MESSAGE_TYPE_UNSUPPORTED

    public static final int MESSAGE_TYPE_UNSUPPORTED

Unsupported message type.

Constant Value: 97 (0x00000061)

### MIP_CONFIG_FAILURE

    public static final int MIP_CONFIG_FAILURE

UE is in MIP-only configuration but the MIP configuration fails on call bring up due to incorrect provisioning.

Constant Value: 2050 (0x00000802)

### MIP_FA_ADMIN_PROHIBITED

    public static final int MIP_FA_ADMIN_PROHIBITED

Foreign agent administratively prohibited MIP (Mobile IP) registration.

Constant Value: 2001 (0x000007d1)

### MIP_FA_DELIVERY_STYLE_NOT_SUPPORTED

    public static final int MIP_FA_DELIVERY_STYLE_NOT_SUPPORTED

Foreign agent rejected MIP (Mobile IP) registration because of delivery style was not supported.

Constant Value: 2012 (0x000007dc)

### MIP_FA_ENCAPSULATION_UNAVAILABLE

    public static final int MIP_FA_ENCAPSULATION_UNAVAILABLE

Foreign agent rejected MIP (Mobile IP) registration because of requested encapsulation was unavailable.

Constant Value: 2008 (0x000007d8)

### MIP_FA_HOME_AGENT_AUTHENTICATION_FAILURE

    public static final int MIP_FA_HOME_AGENT_AUTHENTICATION_FAILURE

Foreign agent rejected MIP (Mobile IP) registration because of home agent authentication failure.

Constant Value: 2004 (0x000007d4)

### MIP_FA_INSUFFICIENT_RESOURCES

    public static final int MIP_FA_INSUFFICIENT_RESOURCES

Foreign agent rejected MIP (Mobile IP) registration because of insufficient resources.

Constant Value: 2002 (0x000007d2)

### MIP_FA_MALFORMED_REPLY

    public static final int MIP_FA_MALFORMED_REPLY

Foreign agent rejected MIP (Mobile IP) registration because of malformed reply.

Constant Value: 2007 (0x000007d7)

### MIP_FA_MALFORMED_REQUEST

    public static final int MIP_FA_MALFORMED_REQUEST

Foreign agent rejected MIP (Mobile IP) registration because of malformed request.

Constant Value: 2006 (0x000007d6)

### MIP_FA_MISSING_CHALLENGE

    public static final int MIP_FA_MISSING_CHALLENGE

Foreign agent rejected MIP (Mobile IP) registration because of missing challenge.

Constant Value: 2017 (0x000007e1)

### MIP_FA_MISSING_HOME_ADDRESS

    public static final int MIP_FA_MISSING_HOME_ADDRESS

Foreign agent rejected MIP (Mobile IP) registration because of missing Home Address.

Constant Value: 2015 (0x000007df)

### MIP_FA_MISSING_HOME_AGENT

    public static final int MIP_FA_MISSING_HOME_AGENT

Foreign agent rejected MIP (Mobile IP) registration because of missing Home Agent.

Constant Value: 2014 (0x000007de)

### MIP_FA_MISSING_NAI

    public static final int MIP_FA_MISSING_NAI

Foreign agent rejected MIP (Mobile IP) registration because of missing NAI (Network Access Identifier).

Constant Value: 2013 (0x000007dd)

### MIP_FA_MOBILE_NODE_AUTHENTICATION_FAILURE

    public static final int MIP_FA_MOBILE_NODE_AUTHENTICATION_FAILURE

Foreign agent rejected MIP (Mobile IP) registration because of MN-AAA authenticator was wrong.

Constant Value: 2003 (0x000007d3)

### MIP_FA_REASON_UNSPECIFIED

    public static final int MIP_FA_REASON_UNSPECIFIED

Reason unspecified for foreign agent rejected MIP (Mobile IP) registration.

Constant Value: 2000 (0x000007d0)

### MIP_FA_REQUESTED_LIFETIME_TOO_LONG

    public static final int MIP_FA_REQUESTED_LIFETIME_TOO_LONG

Foreign agent rejected MIP (Mobile IP) registration because of requested lifetime was too long.

Constant Value: 2005 (0x000007d5)

### MIP_FA_REVERSE_TUNNEL_IS_MANDATORY

    public static final int MIP_FA_REVERSE_TUNNEL_IS_MANDATORY

Foreign agent rejected MIP (Mobile IP) registration because of reverse tunnel was mandatory but not requested by device.

Constant Value: 2011 (0x000007db)

### MIP_FA_REVERSE_TUNNEL_UNAVAILABLE

    public static final int MIP_FA_REVERSE_TUNNEL_UNAVAILABLE

Foreign agent rejected MIP (Mobile IP) registration because of reverse tunnel was unavailable.

Constant Value: 2010 (0x000007da)

### MIP_FA_STALE_CHALLENGE

    public static final int MIP_FA_STALE_CHALLENGE

Foreign agent rejected MIP (Mobile IP) registration because of stale challenge.

Constant Value: 2018 (0x000007e2)

### MIP_FA_UNKNOWN_CHALLENGE

    public static final int MIP_FA_UNKNOWN_CHALLENGE

Foreign agent rejected MIP (Mobile IP) registration because of unknown challenge.

Constant Value: 2016 (0x000007e0)

### MIP_FA_VJ_HEADER_COMPRESSION_UNAVAILABLE

    public static final int MIP_FA_VJ_HEADER_COMPRESSION_UNAVAILABLE

Foreign agent rejected MIP (Mobile IP) registration of VJ Header Compression was unavailable.

Constant Value: 2009 (0x000007d9)

### MIP_HA_ADMIN_PROHIBITED

    public static final int MIP_HA_ADMIN_PROHIBITED

Home agent administratively prohibited MIP (Mobile IP) registration.

Constant Value: 2020 (0x000007e4)

### MIP_HA_ENCAPSULATION_UNAVAILABLE

    public static final int MIP_HA_ENCAPSULATION_UNAVAILABLE

Home agent rejected MIP (Mobile IP) registration because of encapsulation unavailable.

Constant Value: 2029 (0x000007ed)

### MIP_HA_FOREIGN_AGENT_AUTHENTICATION_FAILURE

    public static final int MIP_HA_FOREIGN_AGENT_AUTHENTICATION_FAILURE

Home agent rejected MIP (Mobile IP) registration because of foreign agent authentication failure.

Constant Value: 2023 (0x000007e7)

### MIP_HA_INSUFFICIENT_RESOURCES

    public static final int MIP_HA_INSUFFICIENT_RESOURCES

Home agent rejected MIP (Mobile IP) registration because of insufficient resources.

Constant Value: 2021 (0x000007e5)

### MIP_HA_MALFORMED_REQUEST

    public static final int MIP_HA_MALFORMED_REQUEST

Home agent rejected MIP (Mobile IP) registration because of malformed request.

Constant Value: 2025 (0x000007e9)

### MIP_HA_MOBILE_NODE_AUTHENTICATION_FAILURE

    public static final int MIP_HA_MOBILE_NODE_AUTHENTICATION_FAILURE

Home agent rejected MIP (Mobile IP) registration because of MN-HA authenticator was wrong.

Constant Value: 2022 (0x000007e6)

### MIP_HA_REASON_UNSPECIFIED

    public static final int MIP_HA_REASON_UNSPECIFIED

Reason unspecified for home agent rejected MIP (Mobile IP) registration.

Constant Value: 2019 (0x000007e3)

### MIP_HA_REGISTRATION_ID_MISMATCH

    public static final int MIP_HA_REGISTRATION_ID_MISMATCH

Home agent rejected MIP (Mobile IP) registration because of registration id mismatch.

Constant Value: 2024 (0x000007e8)

### MIP_HA_REVERSE_TUNNEL_IS_MANDATORY

    public static final int MIP_HA_REVERSE_TUNNEL_IS_MANDATORY

Home agent rejected MIP (Mobile IP) registration because of reverse tunnel is mandatory but not requested by device.

Constant Value: 2028 (0x000007ec)

### MIP_HA_REVERSE_TUNNEL_UNAVAILABLE

    public static final int MIP_HA_REVERSE_TUNNEL_UNAVAILABLE

Home agent rejected MIP (Mobile IP) registration because of reverse tunnel was unavailable.

Constant Value: 2027 (0x000007eb)

### MIP_HA_UNKNOWN_HOME_AGENT_ADDRESS

    public static final int MIP_HA_UNKNOWN_HOME_AGENT_ADDRESS

Home agent rejected MIP (Mobile IP) registration because of unknown home agent address.

Constant Value: 2026 (0x000007ea)

### MISSING_UNKNOWN_APN

    public static final int MISSING_UNKNOWN_APN

Missing or unknown APN.

Constant Value: 27 (0x0000001b)

### MODEM_APP_PREEMPTED

    public static final int MODEM_APP_PREEMPTED

Another application in modem preempts the data call.

Constant Value: 2032 (0x000007f0)

### MODEM_RESTART

    public static final int MODEM_RESTART

Modem restart.

Constant Value: 2037 (0x000007f5)

### MSC_TEMPORARILY_NOT_REACHABLE

    public static final int MSC_TEMPORARILY_NOT_REACHABLE

Mobile switching center is temporarily unreachable.

Constant Value: 2180 (0x00000884)

### MSG_AND_PROTOCOL_STATE_UNCOMPATIBLE

    public static final int MSG_AND_PROTOCOL_STATE_UNCOMPATIBLE

Message and protocol state uncompatible.

Constant Value: 101 (0x00000065)

### MSG_TYPE_NONCOMPATIBLE_STATE

    public static final int MSG_TYPE_NONCOMPATIBLE_STATE

Message type uncompatible.

Constant Value: 98 (0x00000062)

### MS_IDENTITY_CANNOT_BE_DERIVED_BY_THE_NETWORK

    public static final int MS_IDENTITY_CANNOT_BE_DERIVED_BY_THE_NETWORK

No matching identity or context could be found in the network.

Constant Value: 2099 (0x00000833)

### MULTIPLE_PDP_CALL_NOT_ALLOWED

    public static final int MULTIPLE_PDP_CALL_NOT_ALLOWED

Multiple PDP call feature is disabled.

Constant Value: 2192 (0x00000890)

### MULTI_CONN_TO_SAME_PDN_NOT_ALLOWED

    public static final int MULTI_CONN_TO_SAME_PDN_NOT_ALLOWED

Multiple connections to a same PDN is not allowed.

Constant Value: 55 (0x00000037)

### NAS_LAYER_FAILURE

    public static final int NAS_LAYER_FAILURE

Non-Access Spectrum layer failure.

Constant Value: 2191 (0x0000088f)

### NAS_REQUEST_REJECTED_BY_NETWORK

    public static final int NAS_REQUEST_REJECTED_BY_NETWORK

Non-access stratum (NAS) request was rejected by the network.

Constant Value: 2167 (0x00000877)

### NAS_SIGNALLING

    public static final int NAS_SIGNALLING

NAS signalling.

Constant Value: 14 (0x0000000e)

### NETWORK_FAILURE

    public static final int NETWORK_FAILURE

Network Failure.

Constant Value: 38 (0x00000026)

### NETWORK_INITIATED_DETACH_NO_AUTO_REATTACH

    public static final int NETWORK_INITIATED_DETACH_NO_AUTO_REATTACH

Network-initiated detach without reattach.

Constant Value: 2154 (0x0000086a)

### NETWORK_INITIATED_DETACH_WITH_AUTO_REATTACH

    public static final int NETWORK_INITIATED_DETACH_WITH_AUTO_REATTACH

Network-initiated detach with reattach.

Constant Value: 2153 (0x00000869)

### NETWORK_INITIATED_TERMINATION

    public static final int NETWORK_INITIATED_TERMINATION

Brought down by the network.

Constant Value: 2031 (0x000007ef)

### NONE

    public static final int NONE

There is no failure

Constant Value: 0 (0x00000000)

### NON_IP_NOT_SUPPORTED

    public static final int NON_IP_NOT_SUPPORTED

UE is unable to bring up a non-IP data call because the device is not camped on a NB1 cell.

Constant Value: 2069 (0x00000815)

### NORMAL_RELEASE

    public static final int NORMAL_RELEASE

Receiving a release from the base station with no reason.

Constant Value: 2218 (0x000008aa)

### NO_CDMA_SERVICE

    public static final int NO_CDMA_SERVICE

Device does not have CDMA service.

Constant Value: 2084 (0x00000824)

### NO_COLLOCATED_HDR

    public static final int NO_COLLOCATED_HDR

There is no co-located HDR.

Constant Value: 2225 (0x000008b1)

### NO_EPS_BEARER_CONTEXT_ACTIVATED

    public static final int NO_EPS_BEARER_CONTEXT_ACTIVATED

No EPS bearer context was activated.

Constant Value: 2189 (0x0000088d)

### NO_GPRS_CONTEXT

    public static final int NO_GPRS_CONTEXT

GPRS context is not available.

Constant Value: 2094 (0x0000082e)

### NO_HYBRID_HDR_SERVICE

    public static final int NO_HYBRID_HDR_SERVICE

Device has no hybrid HDR service.

Constant Value: 2209 (0x000008a1)

### NO_PDP_CONTEXT_ACTIVATED

    public static final int NO_PDP_CONTEXT_ACTIVATED

MS requests an establishment of the radio access bearers for all active PDP contexts by sending a service request message indicating data to the network, but the SGSN does not have any active PDP context.

Constant Value: 2107 (0x0000083b)

### NO_RESPONSE_FROM_BASE_STATION

    public static final int NO_RESPONSE_FROM_BASE_STATION

There was no response received from the base station.

Constant Value: 2081 (0x00000821)

### NO_SERVICE

    public static final int NO_SERVICE

Device has no service.

Constant Value: 2216 (0x000008a8)

### NO_SERVICE_ON_GATEWAY

    public static final int NO_SERVICE_ON_GATEWAY

No service on the gateway.

Constant Value: 2093 (0x0000082d)

### NSAPI_IN_USE

    public static final int NSAPI_IN_USE

The Network Service Access Point Identifier (NSAPI) is in use.

Constant Value: 35 (0x00000023)

### NULL_APN_DISALLOWED

    public static final int NULL_APN_DISALLOWED

PDN is attempted to be brought up with NULL APN but NULL APN is not supported.

Constant Value: 2061 (0x0000080d)

### OEM_DCFAILCAUSE_1

    public static final int OEM_DCFAILCAUSE_1

Constant Value: 4097 (0x00001001)

### OEM_DCFAILCAUSE_10

    public static final int OEM_DCFAILCAUSE_10

Constant Value: 4106 (0x0000100a)

### OEM_DCFAILCAUSE_11

    public static final int OEM_DCFAILCAUSE_11

Constant Value: 4107 (0x0000100b)

### OEM_DCFAILCAUSE_12

    public static final int OEM_DCFAILCAUSE_12

Constant Value: 4108 (0x0000100c)

### OEM_DCFAILCAUSE_13

    public static final int OEM_DCFAILCAUSE_13

Constant Value: 4109 (0x0000100d)

### OEM_DCFAILCAUSE_14

    public static final int OEM_DCFAILCAUSE_14

Constant Value: 4110 (0x0000100e)

### OEM_DCFAILCAUSE_15

    public static final int OEM_DCFAILCAUSE_15

Constant Value: 4111 (0x0000100f)

### OEM_DCFAILCAUSE_2

    public static final int OEM_DCFAILCAUSE_2

Constant Value: 4098 (0x00001002)

### OEM_DCFAILCAUSE_3

    public static final int OEM_DCFAILCAUSE_3

Constant Value: 4099 (0x00001003)

### OEM_DCFAILCAUSE_4

    public static final int OEM_DCFAILCAUSE_4

Constant Value: 4100 (0x00001004)

### OEM_DCFAILCAUSE_5

    public static final int OEM_DCFAILCAUSE_5

Constant Value: 4101 (0x00001005)

### OEM_DCFAILCAUSE_6

    public static final int OEM_DCFAILCAUSE_6

Constant Value: 4102 (0x00001006)

### OEM_DCFAILCAUSE_7

    public static final int OEM_DCFAILCAUSE_7

Constant Value: 4103 (0x00001007)

### OEM_DCFAILCAUSE_8

    public static final int OEM_DCFAILCAUSE_8

Constant Value: 4104 (0x00001008)

### OEM_DCFAILCAUSE_9

    public static final int OEM_DCFAILCAUSE_9

Constant Value: 4105 (0x00001009)

### ONLY_IPV4V6_ALLOWED

    public static final int ONLY_IPV4V6_ALLOWED

Network supports IPv4v6 PDP type only. Non-IP type is not allowed. In LTE mode of operation, this is a PDN throttling cause code, meaning the UE may throttle further requests to the same APN.

Constant Value: 57 (0x00000039)

### ONLY_IPV4_ALLOWED

    public static final int ONLY_IPV4_ALLOWED

Packet Data Protocol (PDP) type IPv4 only allowed.

Constant Value: 50 (0x00000032)

### ONLY_IPV6_ALLOWED

    public static final int ONLY_IPV6_ALLOWED

Packet Data Protocol (PDP) type IPv6 only allowed.

Constant Value: 51 (0x00000033)

### ONLY_NON_IP_ALLOWED

    public static final int ONLY_NON_IP_ALLOWED

Network supports non-IP PDP type only. IPv4, IPv6 and IPv4v6 is not allowed. In LTE mode of operation, this is a PDN throttling cause code, meaning the UE can throttle further requests to the same APN.

Constant Value: 58 (0x0000003a)

### ONLY_SINGLE_BEARER_ALLOWED

    public static final int ONLY_SINGLE_BEARER_ALLOWED

Single address bearers only allowed.

Constant Value: 52 (0x00000034)

### OPERATOR_BARRED

    public static final int OPERATOR_BARRED

Operator determined barring. (no retry)

Constant Value: 8 (0x00000008)

### OTASP_COMMIT_IN_PROGRESS

    public static final int OTASP_COMMIT_IN_PROGRESS

OTASP commit is in progress.

Constant Value: 2208 (0x000008a0)

### PDN_CONN_DOES_NOT_EXIST

    public static final int PDN_CONN_DOES_NOT_EXIST

PDN connection does not exist.

Constant Value: 54 (0x00000036)

### PDN_INACTIVITY_TIMER_EXPIRED

    public static final int PDN_INACTIVITY_TIMER_EXPIRED

PDN inactivity timer expired due to no data transmission in a configurable duration of time.

Constant Value: 2051 (0x00000803)

### PDN_IPV4_CALL_DISALLOWED

    public static final int PDN_IPV4_CALL_DISALLOWED

IPV4 PDN is in throttled state due to network providing only IPV6 address during the previous VSNCP bringup (subs_limited_to_v6).

Constant Value: 2033 (0x000007f1)

### PDN_IPV4_CALL_THROTTLED

    public static final int PDN_IPV4_CALL_THROTTLED

IPV4 PDN is in throttled state due to previous VSNCP bringup failure(s).

Constant Value: 2034 (0x000007f2)

### PDN_IPV6_CALL_DISALLOWED

    public static final int PDN_IPV6_CALL_DISALLOWED

IPV6 PDN is in throttled state due to network providing only IPV4 address during the previous VSNCP bringup (subs_limited_to_v4).

Constant Value: 2035 (0x000007f3)

### PDN_IPV6_CALL_THROTTLED

    public static final int PDN_IPV6_CALL_THROTTLED

IPV6 PDN is in throttled state due to previous VSNCP bringup failure(s).

Constant Value: 2036 (0x000007f4)

### PDN_NON_IP_CALL_DISALLOWED

    public static final int PDN_NON_IP_CALL_DISALLOWED

Non-IP PDN is in disallowed state due to the network providing only an IP address.

Constant Value: 2071 (0x00000817)

### PDN_NON_IP_CALL_THROTTLED

    public static final int PDN_NON_IP_CALL_THROTTLED

Non-IP PDN is in throttled state due to previous VSNCP bringup failure(s).

Constant Value: 2070 (0x00000816)

### PDP_ACTIVATE_MAX_RETRY_FAILED

    public static final int PDP_ACTIVATE_MAX_RETRY_FAILED

SM attempts PDP activation for a maximum of four attempts.

Constant Value: 2109 (0x0000083d)

### PDP_DUPLICATE

    public static final int PDP_DUPLICATE

PDP context already exists.

Constant Value: 2104 (0x00000838)

### PDP_ESTABLISH_TIMEOUT_EXPIRED

    public static final int PDP_ESTABLISH_TIMEOUT_EXPIRED

Expiration of the PDP establish timer with a maximum of five retries.

Constant Value: 2161 (0x00000871)

### PDP_INACTIVE_TIMEOUT_EXPIRED

    public static final int PDP_INACTIVE_TIMEOUT_EXPIRED

Expiration of the PDP deactivate timer with a maximum of four retries.

Constant Value: 2163 (0x00000873)

### PDP_LOWERLAYER_ERROR

    public static final int PDP_LOWERLAYER_ERROR

PDP activation failed due to RRC_ABORT or a forbidden PLMN.

Constant Value: 2164 (0x00000874)

### PDP_MODIFY_COLLISION

    public static final int PDP_MODIFY_COLLISION

MO PDP modify collision when the MT PDP is already in progress.

Constant Value: 2165 (0x00000875)

### PDP_MODIFY_TIMEOUT_EXPIRED

    public static final int PDP_MODIFY_TIMEOUT_EXPIRED

Expiration of the PDP modify timer with a maximum of four retries.

Constant Value: 2162 (0x00000872)

### PDP_PPP_NOT_SUPPORTED

    public static final int PDP_PPP_NOT_SUPPORTED

PDP PPP calls are not supported.

Constant Value: 2038 (0x000007f6)

### PDP_WITHOUT_ACTIVE_TFT

    public static final int PDP_WITHOUT_ACTIVE_TFT

Packet Data Protocol (PDP) without active traffic flow template (TFT).

Constant Value: 46 (0x0000002e)

### PHONE_IN_USE

    public static final int PHONE_IN_USE

Device is in use (e.g., voice call).

Constant Value: 2222 (0x000008ae)

### PHYSICAL_LINK_CLOSE_IN_PROGRESS

    public static final int PHYSICAL_LINK_CLOSE_IN_PROGRESS

Physical link is in the process of cleanup.

Constant Value: 2040 (0x000007f8)

### PLMN_NOT_ALLOWED

    public static final int PLMN_NOT_ALLOWED

UE requests GPRS service, or the network initiates a detach request in a PLMN which does not offer roaming for GPRS services to that MS.

Constant Value: 2101 (0x00000835)

### PPP_AUTH_FAILURE

    public static final int PPP_AUTH_FAILURE

Data call bring up fails in the PPP setup due to an authorization failure. (e.g., authorization is required, but not negotiated with the network during an LCP phase)

Constant Value: 2229 (0x000008b5)

### PPP_CHAP_FAILURE

    public static final int PPP_CHAP_FAILURE

Data call bring up fails in the PPP setup due to a CHAP failure.

Constant Value: 2232 (0x000008b8)

### PPP_CLOSE_IN_PROGRESS

    public static final int PPP_CLOSE_IN_PROGRESS

Data call bring up fails in the PPP setup because the PPP is in the process of cleaning the previous PPP session.

Constant Value: 2233 (0x000008b9)

### PPP_OPTION_MISMATCH

    public static final int PPP_OPTION_MISMATCH

Data call bring up fails in the PPP setup due to an option mismatch.

Constant Value: 2230 (0x000008b6)

### PPP_PAP_FAILURE

    public static final int PPP_PAP_FAILURE

Data call bring up fails in the PPP setup due to a PAP failure.

Constant Value: 2231 (0x000008b7)

### PPP_TIMEOUT

    public static final int PPP_TIMEOUT

Data call bring up fails in the PPP setup due to a timeout. (e.g., an LCP conf ack was not received from the network)

Constant Value: 2228 (0x000008b4)

### PREF_RADIO_TECH_CHANGED

    public static final int PREF_RADIO_TECH_CHANGED

Preferred technology has changed, must retry with parameters appropriate for new technology.

Constant Value: -4 (0xfffffffc)

### PROFILE_BEARER_INCOMPATIBLE

    public static final int PROFILE_BEARER_INCOMPATIBLE

APN bearer type in the profile does not match preferred network mode.

Constant Value: 2042 (0x000007fa)

### PROTOCOL_ERRORS

    public static final int PROTOCOL_ERRORS

Protocol errors.

Constant Value: 111 (0x0000006f)

### QOS_NOT_ACCEPTED

    public static final int QOS_NOT_ACCEPTED

Quality of service (QoS) is not accepted.

Constant Value: 37 (0x00000025)

### RADIO_ACCESS_BEARER_FAILURE

    public static final int RADIO_ACCESS_BEARER_FAILURE

Radio access bearer failure.

Constant Value: 2110 (0x0000083e)

### RADIO_ACCESS_BEARER_SETUP_FAILURE

    public static final int RADIO_ACCESS_BEARER_SETUP_FAILURE

Radio access bearer is not established by the lower layers during activation, modification, or deactivation.

Constant Value: 2160 (0x00000870)

### RADIO_NOT_AVAILABLE

    public static final int RADIO_NOT_AVAILABLE

Data fail due to radio not unavailable.

Constant Value: 65537 (0x00010001)

### RADIO_POWER_OFF

    public static final int RADIO_POWER_OFF

data call was disconnected because radio was resetting, powered off.

Constant Value: -5 (0xfffffffb)

### REDIRECTION_OR_HANDOFF_IN_PROGRESS

    public static final int REDIRECTION_OR_HANDOFF_IN_PROGRESS

Device is in the process of redirecting or handing off to a different target system.

Constant Value: 2220 (0x000008ac)

### REGISTRATION_FAIL

    public static final int REGISTRATION_FAIL

Data fail due to registration failure.

Constant Value: -1 (0xffffffff)

### REGULAR_DEACTIVATION

    public static final int REGULAR_DEACTIVATION

Regular deactivation.

Constant Value: 36 (0x00000024)

### REJECTED_BY_BASE_STATION

    public static final int REJECTED_BY_BASE_STATION

The base station rejecting the call.

Constant Value: 2082 (0x00000822)

### RRC_CONNECTION_ABORTED_AFTER_HANDOVER

    public static final int RRC_CONNECTION_ABORTED_AFTER_HANDOVER

Radio resource control (RRC) connection was aborted by the non-access stratum (NAS) after an IRAT to LTE IRAT handover.

Constant Value: 2173 (0x0000087d)

### RRC_CONNECTION_ABORTED_AFTER_IRAT_CELL_CHANGE

    public static final int RRC_CONNECTION_ABORTED_AFTER_IRAT_CELL_CHANGE

Radio resource control (RRC) connection was aborted before deactivating the LTE stack after a successful LTE to GSM/EDGE IRAT cell change order procedure.

Constant Value: 2174 (0x0000087e)

### RRC_CONNECTION_ABORTED_DUE_TO_IRAT_CHANGE

    public static final int RRC_CONNECTION_ABORTED_DUE_TO_IRAT_CHANGE

Radio resource control (RRC) connection was aborted before deactivating the LTE stack due to a successful LTE to WCDMA/GSM/TD-SCDMA IRAT change.

Constant Value: 2171 (0x0000087b)

### RRC_CONNECTION_ABORTED_DURING_IRAT_CELL_CHANGE

    public static final int RRC_CONNECTION_ABORTED_DURING_IRAT_CELL_CHANGE

Radio resource control (RRC) connection was aborted in the middle of a LTE to GSM IRAT cell change order procedure.

Constant Value: 2175 (0x0000087f)

### RRC_CONNECTION_ABORT_REQUEST

    public static final int RRC_CONNECTION_ABORT_REQUEST

Connection has been released by the radio resource control (RRC) due to an abort request.

Constant Value: 2151 (0x00000867)

### RRC_CONNECTION_ACCESS_BARRED

    public static final int RRC_CONNECTION_ACCESS_BARRED

Radio resource control (RRC) connection establishment failed due to access barrred.

Constant Value: 2139 (0x0000085b)

### RRC_CONNECTION_ACCESS_STRATUM_FAILURE

    public static final int RRC_CONNECTION_ACCESS_STRATUM_FAILURE

Radio resource control (RRC) connection failure at access stratum.

Constant Value: 2137 (0x00000859)

### RRC_CONNECTION_ANOTHER_PROCEDURE_IN_PROGRESS

    public static final int RRC_CONNECTION_ANOTHER_PROCEDURE_IN_PROGRESS

Radio resource control (RRC) connection establishment is aborted due to another procedure.

Constant Value: 2138 (0x0000085a)

### RRC_CONNECTION_CELL_NOT_CAMPED

    public static final int RRC_CONNECTION_CELL_NOT_CAMPED

Connection establishment failed as the radio resource control (RRC) is not camped on any cell.

Constant Value: 2144 (0x00000860)

### RRC_CONNECTION_CELL_RESELECTION

    public static final int RRC_CONNECTION_CELL_RESELECTION

Radio resource control (RRC) connection establishment failed due to cell reselection at access stratum.

Constant Value: 2140 (0x0000085c)

### RRC_CONNECTION_CONFIG_FAILURE

    public static final int RRC_CONNECTION_CONFIG_FAILURE

Connection establishment failed due to configuration failure at the radio resource control (RRC).

Constant Value: 2141 (0x0000085d)

### RRC_CONNECTION_INVALID_REQUEST

    public static final int RRC_CONNECTION_INVALID_REQUEST

Radio resource control (RRC) connection establishment failure due to an error in the request message.

Constant Value: 2168 (0x00000878)

### RRC_CONNECTION_LINK_FAILURE

    public static final int RRC_CONNECTION_LINK_FAILURE

Connection establishment failed due to a link failure at the radio resource control (RRC).

Constant Value: 2143 (0x0000085f)

### RRC_CONNECTION_NORMAL_RELEASE

    public static final int RRC_CONNECTION_NORMAL_RELEASE

Normal radio resource control (RRC) connection release.

Constant Value: 2147 (0x00000863)

### RRC_CONNECTION_OUT_OF_SERVICE_DURING_CELL_REGISTER

    public static final int RRC_CONNECTION_OUT_OF_SERVICE_DURING_CELL_REGISTER

UE is out of service during the call register.

Constant Value: 2150 (0x00000866)

### RRC_CONNECTION_RADIO_LINK_FAILURE

    public static final int RRC_CONNECTION_RADIO_LINK_FAILURE

Radio resource control (RRC) connection release failed due to radio link failure conditions.

Constant Value: 2148 (0x00000864)

### RRC_CONNECTION_REESTABLISHMENT_FAILURE

    public static final int RRC_CONNECTION_REESTABLISHMENT_FAILURE

Radio resource control (RRC) connection re-establishment failure.

Constant Value: 2149 (0x00000865)

### RRC_CONNECTION_REJECT_BY_NETWORK

    public static final int RRC_CONNECTION_REJECT_BY_NETWORK

Radio resource control (RRC) connection establishment failed due to the network rejecting the UE connection request.

Constant Value: 2146 (0x00000862)

### RRC_CONNECTION_RELEASED_SECURITY_NOT_ACTIVE

    public static final int RRC_CONNECTION_RELEASED_SECURITY_NOT_ACTIVE

If the UE has an LTE radio link failure before security is established, the radio resource control (RRC) connection must be released and the UE must return to idle.

Constant Value: 2172 (0x0000087c)

### RRC_CONNECTION_RF_UNAVAILABLE

    public static final int RRC_CONNECTION_RF_UNAVAILABLE

Radio resource control (RRC) connection establishment failure due to the RF was unavailable.

Constant Value: 2170 (0x0000087a)

### RRC_CONNECTION_SYSTEM_INFORMATION_BLOCK_READ_ERROR

    public static final int RRC_CONNECTION_SYSTEM_INFORMATION_BLOCK_READ_ERROR

Radio resource control (RRC) connection released due to a system information block read error.

Constant Value: 2152 (0x00000868)

### RRC_CONNECTION_SYSTEM_INTERVAL_FAILURE

    public static final int RRC_CONNECTION_SYSTEM_INTERVAL_FAILURE

Connection establishment failed due to a service interval failure at the radio resource control (RRC).

Constant Value: 2145 (0x00000861)

### RRC_CONNECTION_TIMER_EXPIRED

    public static final int RRC_CONNECTION_TIMER_EXPIRED

Radio resource control (RRC) connection could not be established in the time limit.

Constant Value: 2142 (0x0000085e)

### RRC_CONNECTION_TRACKING_AREA_ID_CHANGED

    public static final int RRC_CONNECTION_TRACKING_AREA_ID_CHANGED

Radio resource control (RRC) connection establishment failure due to a change in the tracking area ID.

Constant Value: 2169 (0x00000879)

### RRC_UPLINK_CONNECTION_RELEASE

    public static final int RRC_UPLINK_CONNECTION_RELEASE

Radio resource control (RRC) uplink data delivery failed due to a connection release.

Constant Value: 2134 (0x00000856)

### RRC_UPLINK_DATA_TRANSMISSION_FAILURE

    public static final int RRC_UPLINK_DATA_TRANSMISSION_FAILURE

Transmission failure of radio resource control (RRC) uplink data.

Constant Value: 2132 (0x00000854)

### RRC_UPLINK_DELIVERY_FAILED_DUE_TO_HANDOVER

    public static final int RRC_UPLINK_DELIVERY_FAILED_DUE_TO_HANDOVER

Radio resource control (RRC) uplink data delivery failed due to a handover.

Constant Value: 2133 (0x00000855)

### RRC_UPLINK_ERROR_REQUEST_FROM_NAS

    public static final int RRC_UPLINK_ERROR_REQUEST_FROM_NAS

Radio resource control (RRC) is not connected but the non-access stratum (NAS) sends an uplink data request.

Constant Value: 2136 (0x00000858)

### RRC_UPLINK_RADIO_LINK_FAILURE

    public static final int RRC_UPLINK_RADIO_LINK_FAILURE

Radio resource control (RRC) uplink data delivery failed due to a radio link failure.

Constant Value: 2135 (0x00000857)

### RUIM_NOT_PRESENT

    public static final int RUIM_NOT_PRESENT

RUIM not being present.

Constant Value: 2085 (0x00000825)

### SECURITY_MODE_REJECTED

    public static final int SECURITY_MODE_REJECTED

Unspecified security mode reject.

Constant Value: 2186 (0x0000088a)

### SERVICE_NOT_ALLOWED_ON_PLMN

    public static final int SERVICE_NOT_ALLOWED_ON_PLMN

Service is not allowed on the requested PLMN.

Constant Value: 2129 (0x00000851)

### SERVICE_OPTION_NOT_SUBSCRIBED

    public static final int SERVICE_OPTION_NOT_SUBSCRIBED

Requested service option not subscribed.

Constant Value: 33 (0x00000021)

### SERVICE_OPTION_NOT_SUPPORTED

    public static final int SERVICE_OPTION_NOT_SUPPORTED

Service option not supported.

Constant Value: 32 (0x00000020)

### SERVICE_OPTION_OUT_OF_ORDER

    public static final int SERVICE_OPTION_OUT_OF_ORDER

Service option temporarily out of order.

Constant Value: 34 (0x00000022)

### SIGNAL_LOST

    public static final int SIGNAL_LOST

Data call drop due to network/modem disconnect.

Constant Value: -3 (0xfffffffd)

### SIM_CARD_CHANGED

    public static final int SIM_CARD_CHANGED

Card was refreshed or removed.

Constant Value: 2043 (0x000007fb)

### SLICE_REJECTED

    public static final int SLICE_REJECTED

Data call fail due to the slice not being allowed for the data call.

Constant Value: 2252 (0x000008cc)

### SYNCHRONIZATION_FAILURE

    public static final int SYNCHRONIZATION_FAILURE

Synchronization failure.

Constant Value: 2184 (0x00000888)

### TEST_LOOPBACK_REGULAR_DEACTIVATION

    public static final int TEST_LOOPBACK_REGULAR_DEACTIVATION

Test loop-back data call has been successfully brought down.

Constant Value: 2196 (0x00000894)

### TETHERED_CALL_ACTIVE

    public static final int TETHERED_CALL_ACTIVE

Data call was disconnected by modem because tethered.

Constant Value: -6 (0xfffffffa)

### TFT_SEMANTIC_ERROR

    public static final int TFT_SEMANTIC_ERROR

Semantic error in the Traffic flow templates (TFT) operation.

Constant Value: 41 (0x00000029)

### TFT_SYTAX_ERROR

    public static final int TFT_SYTAX_ERROR

Syntactical error in the Traffic flow templates (TFT) operation.

Constant Value: 42 (0x0000002a)

### THERMAL_EMERGENCY

    public static final int THERMAL_EMERGENCY

Put device in thermal emergency.

Constant Value: 2090 (0x0000082a)

### THERMAL_MITIGATION

    public static final int THERMAL_MITIGATION

Thermal level increases and causes calls to be torn down when normal mode of operation is not allowed.

Constant Value: 2062 (0x0000080e)

### TRAT_SWAP_FAILED

    public static final int TRAT_SWAP_FAILED

Target RAT swap failed.

Constant Value: 2048 (0x00000800)

### UE_INITIATED_DETACH_OR_DISCONNECT

    public static final int UE_INITIATED_DETACH_OR_DISCONNECT

UE performs a detach or disconnect PDN action based on TE requirements.

Constant Value: 128 (0x00000080)

### UE_IS_ENTERING_POWERSAVE_MODE

    public static final int UE_IS_ENTERING_POWERSAVE_MODE

UE is entering power save mode.

Constant Value: 2226 (0x000008b2)

### UE_RAT_CHANGE

    public static final int UE_RAT_CHANGE

RAT change on the UE.

Constant Value: 2105 (0x00000839)

### UE_SECURITY_CAPABILITIES_MISMATCH

    public static final int UE_SECURITY_CAPABILITIES_MISMATCH

UE security capabilities mismatch.

Constant Value: 2185 (0x00000889)

### UMTS_HANDOVER_TO_IWLAN

    public static final int UMTS_HANDOVER_TO_IWLAN

UMTS interface is brought down due to handover from UMTS to iWLAN.

Constant Value: 2199 (0x00000897)

### UMTS_REACTIVATION_REQ

    public static final int UMTS_REACTIVATION_REQ

Universal Mobile Telecommunications System (UMTS) reactivation request.

Constant Value: 39 (0x00000027)

### UNACCEPTABLE_NETWORK_PARAMETER

    public static final int UNACCEPTABLE_NETWORK_PARAMETER

Data fail due to unacceptable network parameter.

Constant Value: 65538 (0x00010002)

### UNACCEPTABLE_NON_EPS_AUTHENTICATION

    public static final int UNACCEPTABLE_NON_EPS_AUTHENTICATION

Unacceptable non-EPS authentication.

Constant Value: 2187 (0x0000088b)

### UNKNOWN

    public static final int UNKNOWN

Unknown data failure cause.

Constant Value: 65536 (0x00010000)

### UNKNOWN_INFO_ELEMENT

    public static final int UNKNOWN_INFO_ELEMENT

Unknown info element.

Constant Value: 99 (0x00000063)

### UNKNOWN_PDP_ADDRESS_TYPE

    public static final int UNKNOWN_PDP_ADDRESS_TYPE

Unknown Packet Data Protocol (PDP) address type.

Constant Value: 28 (0x0000001c)

### UNKNOWN_PDP_CONTEXT

    public static final int UNKNOWN_PDP_CONTEXT

Unknown Packet Data Protocol (PDP) context.

Constant Value: 43 (0x0000002b)

### UNPREFERRED_RAT

    public static final int UNPREFERRED_RAT

RAT on which the data call is attempted/connected is no longer the preferred RAT.

Constant Value: 2039 (0x000007f7)

### UNSUPPORTED_1X_PREV

    public static final int UNSUPPORTED_1X_PREV

P_rev supported by 1 base station is less than 6, which is not supported for a 1X data call. The UE must be in the footprint of BS which has p_rev >= 6 to support this SO33 call.

Constant Value: 2214 (0x000008a6)

### UNSUPPORTED_APN_IN_CURRENT_PLMN

    public static final int UNSUPPORTED_APN_IN_CURRENT_PLMN

Unsupported APN in current public land mobile network (PLMN).

Constant Value: 66 (0x00000042)

### UNSUPPORTED_QCI_VALUE

    public static final int UNSUPPORTED_QCI_VALUE

QCI (QoS Class Identifier) indicated in the UE request cannot be supported.

Constant Value: 59 (0x0000003b)

### USER_AUTHENTICATION

    public static final int USER_AUTHENTICATION

User authentication.

Constant Value: 29 (0x0000001d)

### VSNCP_ADMINISTRATIVELY_PROHIBITED

    public static final int VSNCP_ADMINISTRATIVELY_PROHIBITED

Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request with the reason of administratively prohibited at the HSGW.

Constant Value: 2245 (0x000008c5)

### VSNCP_APN_UNAUTHORIZED

    public static final int VSNCP_APN_UNAUTHORIZED

Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request because the requested APN is unauthorized.

Constant Value: 2238 (0x000008be)

### VSNCP_GEN_ERROR

    public static final int VSNCP_GEN_ERROR

Data call bring up fails in the VSNCP phase due to a general error. It's used when there is no other specific error code available to report the failure.

Constant Value: 2237 (0x000008bd)

### VSNCP_INSUFFICIENT_PARAMETERS

    public static final int VSNCP_INSUFFICIENT_PARAMETERS

Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request with the reason of insufficient parameter.

Constant Value: 2243 (0x000008c3)

### VSNCP_NO_PDN_GATEWAY_ADDRESS

    public static final int VSNCP_NO_PDN_GATEWAY_ADDRESS

Data call bring up fails in the VSNCP phase due to the network rejected the VSNCP configuration request due to no PDN gateway address.

Constant Value: 2240 (0x000008c0)

### VSNCP_PDN_EXISTS_FOR_THIS_APN

    public static final int VSNCP_PDN_EXISTS_FOR_THIS_APN

Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request because the PDN exists for this APN.

Constant Value: 2248 (0x000008c8)

### VSNCP_PDN_GATEWAY_REJECT

    public static final int VSNCP_PDN_GATEWAY_REJECT

Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request due to a PDN gateway reject.

Constant Value: 2242 (0x000008c2)

### VSNCP_PDN_GATEWAY_UNREACHABLE

    public static final int VSNCP_PDN_GATEWAY_UNREACHABLE

Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request because the PDN gateway is unreachable.

Constant Value: 2241 (0x000008c1)

### VSNCP_PDN_ID_IN_USE

    public static final int VSNCP_PDN_ID_IN_USE

Data call bring up fails in the VSNCP phase due to a network rejection of PDN ID in use, or all existing PDNs are brought down with this end reason because one of the PDN bring up was rejected by the network with the reason of PDN ID in use.

Constant Value: 2246 (0x000008c6)

### VSNCP_PDN_LIMIT_EXCEEDED

    public static final int VSNCP_PDN_LIMIT_EXCEEDED

Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request because the PDN limit has been exceeded.

Constant Value: 2239 (0x000008bf)

### VSNCP_RECONNECT_NOT_ALLOWED

    public static final int VSNCP_RECONNECT_NOT_ALLOWED

Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request with reconnect to this PDN not allowed, or an active data call is terminated by the network because reconnection to this PDN is not allowed. Upon receiving this error code from the network, the modem infinitely throttles the PDN until the next power cycle.

Constant Value: 2249 (0x000008c9)

### VSNCP_RESOURCE_UNAVAILABLE

    public static final int VSNCP_RESOURCE_UNAVAILABLE

Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request with the reason of resource unavailable.

Constant Value: 2244 (0x000008c4)

### VSNCP_SUBSCRIBER_LIMITATION

    public static final int VSNCP_SUBSCRIBER_LIMITATION

Data call bring up fails in the VSNCP phase due to a network rejection of the VSNCP configuration request for the reason of subscriber limitation.

Constant Value: 2247 (0x000008c7)

### VSNCP_TIMEOUT

    public static final int VSNCP_TIMEOUT

Data call bring up fails in the VSNCP phase due to a VSNCP timeout error.

Constant Value: 2236 (0x000008bc)

Full name *
Email address *
Company / developer name
One of your Play Store app URLs *
Which best describes your business:*
Apps
Games
Apps & Games
*
*